| CMSIS-Driver Peripheral Interface for Middleware and Application Code |

Loading...
Searching...
No Matches

### - r -

- range_filtering : ARM_CAN_OBJ_CAPABILITIES
- rb_monitor : ARM_NAND_CAPABILITIES
- read_wait : ARM_MCI_CAPABILITIES
- ReadCD : ARM_DRIVER_MCI
- ReadData : ARM_DRIVER_FLASH, ARM_DRIVER_NAND, ARM_DRIVER_STORAGE
- ReadFrame : ARM_DRIVER_ETH_MAC
- ReadSetupPacket : ARM_DRIVER_USBD
- ReadWP : ARM_DRIVER_MCI
- Receive : ARM_DRIVER_SAI, ARM_DRIVER_SPI, ARM_DRIVER_USART
- reentrant_operation : ARM_CAN_CAPABILITIES, ARM_NAND_CAPABILITIES
- reserved : ARM_CAN_CAPABILITIES, ARM_CAN_MSG_INFO, ARM_CAN_OBJ_CAPABILITIES, ARM_CAN_STATUS, ARM_ETH_LINK_INFO, ARM_ETH_MAC_CAPABILITIES, ARM_FLASH_CAPABILITIES, ARM_FLASH_INFO, ARM_FLASH_STATUS, ARM_I2C_CAPABILITIES, ARM_I2C_STATUS, ARM_MCI_CAPABILITIES, ARM_MCI_STATUS, ARM_NAND_CAPABILITIES, ARM_NAND_ECC_INFO, ARM_NAND_STATUS, ARM_SAI_CAPABILITIES, ARM_SAI_STATUS, ARM_SPI_CAPABILITIES, ARM_SPI_STATUS, ARM_STORAGE_BLOCK_ATTRIBUTES, ARM_STORAGE_CAPABILITIES, ARM_STORAGE_INFO, ARM_STORAGE_STATUS, ARM_USART_CAPABILITIES, ARM_USART_MODEM_STATUS, ARM_USART_STATUS, ARM_USBD_CAPABILITIES, ARM_USBD_STATE, ARM_USBH_CAPABILITIES, ARM_USBH_HCI_CAPABILITIES, ARM_USBH_PORT_STATE, ARM_WIFI_CAPABILITIES, ARM_WIFI_CONFIG_t
- reserved1 : ARM_STORAGE_SECURITY_FEATURES
- reserved2 : ARM_STORAGE_SECURITY_FEATURES
- ResolveAddress : ARM_DRIVER_STORAGE
- restricted_mode : ARM_CAN_CAPABILITIES
- retention_level : ARM_STORAGE_INFO
- ri : ARM_USART_CAPABILITIES, ARM_USART_MODEM_STATUS
- rollback_protection : ARM_STORAGE_SECURITY_FEATURES
- rssi : ARM_WIFI_NET_INFO_t, ARM_WIFI_SCAN_INFO_t
- rst_n : ARM_MCI_CAPABILITIES
- rtr : ARM_CAN_MSG_INFO
- rts : ARM_USART_CAPABILITIES
- rx : ARM_CAN_OBJ_CAPABILITIES
- rx_break : ARM_USART_STATUS
- rx_busy : ARM_SAI_STATUS, ARM_USART_STATUS
- rx_error_count : ARM_CAN_STATUS
- rx_framing_error : ARM_USART_STATUS
- rx_overflow : ARM_SAI_STATUS, ARM_USART_STATUS
- rx_parity_error : ARM_USART_STATUS
- rx_rtr_tx_data : ARM_CAN_OBJ_CAPABILITIES