| CMSIS-Core (Cortex-A) CMSIS-Core support for Cortex-A processor-based devices |

Loading...
Searching...
No Matches
Functions
PL1 Physical Count register (CNTPCT)
Core Register Access

Holds the 64-bit physical count value. More...

## Functions
__STATIC_FORCEINLINE uint64_t | __get_CNTPCT (void)
| Get CNTPCT.

## Description

Holds the 64-bit physical count value.

Consider __get_CNTPCT to access this register.

Consider using Generic Physical Timer Functions for controlling the PL1 Timer instead.

## Function Documentation

## ◆ __get_CNTPCT()

__STATIC_FORCEINLINE uint64_t __get_CNTPCT | ( | void |  | ) |

Get CNTPCT.

This function returns the value of the 64 bits PL1 Physical Count Register (CNTPCT).

Returns
  CNTPCT Register value

This function returns the value of the PL1 Physical Count register (CNTPCT).