| CMSIS-Core (Cortex-M) CMSIS-Core support for Cortex-M processor-based devices |

Loading...
Searching...
No Matches
Data Fields
SysTick_Type Struct Reference

Structure type to access the System Timer (SysTick). More...

## Data Fields
__IM uint32_t | CALIB
| Offset: 0x00C (R/ ) SysTick Calibration Register.
__IOM uint32_t | CTRL
| Offset: 0x000 (R/W) SysTick Control and Status Register.
__IOM uint32_t | LOAD
| Offset: 0x004 (R/W) SysTick Reload Value Register.
__IOM uint32_t | VAL
| Offset: 0x008 (R/W) SysTick Current Value Register.

## Description

Structure type to access the System Timer (SysTick).

## Field Documentation

## ◆ CALIB

__IM uint32_t SysTick_Type::CALIB

Offset: 0x00C (R/ ) SysTick Calibration Register.

## ◆ CTRL

__IOM uint32_t SysTick_Type::CTRL

Offset: 0x000 (R/W) SysTick Control and Status Register.

## ◆ LOAD

__IOM uint32_t SysTick_Type::LOAD

Offset: 0x004 (R/W) SysTick Reload Value Register.

## ◆ VAL

__IOM uint32_t SysTick_Type::VAL

Offset: 0x008 (R/W) SysTick Current Value Register.