| CMSIS-Driver Peripheral Interface for Middleware and Application Code |

Loading...
Searching...
No Matches
Functions
Driver_SAI.c File Reference

## Functions
ARM_DRIVER_VERSION | ARM_SAI_GetVersion (void)
| Get driver version.
ARM_SAI_CAPABILITIES | ARM_SAI_GetCapabilities (void)
| Get driver capabilities.
int32_t | ARM_SAI_Initialize (ARM_SAI_SignalEvent_t cb_event)
| Initialize SAI Interface.
int32_t | ARM_SAI_Uninitialize (void)
| De-initialize SAI Interface.
int32_t | ARM_SAI_PowerControl (ARM_POWER_STATE state)
| Control SAI Interface Power.
int32_t | ARM_SAI_Send (const void *data, uint32_t num)
| Start sending data to SAI transmitter.
int32_t | ARM_SAI_Receive (void *data, uint32_t num)
| Start receiving data from SAI receiver.
uint32_t | ARM_SAI_GetTxCount (void)
| Get transmitted data count.
uint32_t | ARM_SAI_GetRxCount (void)
| Get received data count.
int32_t | ARM_SAI_Control (uint32_t control, uint32_t arg1, uint32_t arg2)
| Control SAI Interface.
ARM_SAI_STATUS | ARM_SAI_GetStatus (void)
| Get SAI status.
void | ARM_SAI_SignalEvent (uint32_t event)
| Signal SAI Events.