| CMSIS-Core (Cortex-M) CMSIS-Core support for Cortex-M processor-based devices |

Loading...
Searching...
No Matches
Data Fields
DIB_Type Struct Reference

Structure type to access the Debug Identification Block Registers (DIB). More...

## Data Fields
__IM uint32_t | DAUTHSTATUS
| Offset: 0x008 (R/ ) Debug Authentication Status Register.
__IM uint32_t | DDEVARCH
| Offset: 0x00C (R/ ) SCS Device Architecture Register.
__IM uint32_t | DDEVTYPE
| Offset: 0x01C (R/ ) SCS Device Type Register.

## Description

Structure type to access the Debug Identification Block Registers (DIB).

## Field Documentation

## ◆ DAUTHSTATUS

__IM uint32_t DIB_Type::DAUTHSTATUS

Offset: 0x008 (R/ ) Debug Authentication Status Register.

## ◆ DDEVARCH

__IM uint32_t DIB_Type::DDEVARCH

Offset: 0x00C (R/ ) SCS Device Architecture Register.

## ◆ DDEVTYPE

__IM uint32_t DIB_Type::DDEVTYPE

Offset: 0x01C (R/ ) SCS Device Type Register.