| CMSIS-Driver Peripheral Interface for Middleware and Application Code |

Loading...
Searching...
No Matches
Macros
WiFi Protected Setup (WPS) Method
WiFi Interface » WiFi Management

Specifies WiFi WPS method for ARM_WIFI_Activate. More...

## Macros
#define | ARM_WIFI_WPS_METHOD_NONE 0U
| Not used.
#define | ARM_WIFI_WPS_METHOD_PBC 1U
| Push Button Configuration.
#define | ARM_WIFI_WPS_METHOD_PIN 2U
| PIN.

## Description

Specifies WiFi WPS method for ARM_WIFI_Activate.

The WiFi WPS method defines which WPS method is used.

## Macro Definition Documentation

## ◆ ARM_WIFI_WPS_METHOD_NONE

#define ARM_WIFI_WPS_METHOD_NONE 0U

Not used.

WPS not used.

See also
  WiFi Protected Setup (WPS) Method

## ◆ ARM_WIFI_WPS_METHOD_PBC

#define ARM_WIFI_WPS_METHOD_PBC 1U

Push Button Configuration.

WPS with Push Button Configuration.

See also
  WiFi Protected Setup (WPS) Method

## ◆ ARM_WIFI_WPS_METHOD_PIN

#define ARM_WIFI_WPS_METHOD_PIN 2U

PIN.

WPS with PIN.

See also
  WiFi Protected Setup (WPS) Method