| CMSIS-Driver Peripheral Interface for Middleware and Application Code |

Loading...
Searching...
No Matches
Macros
CAN Object Events
CAN Interface

Callback objects events notified via ARM_CAN_SignalObjectEvent. More...

## Macros
#define | ARM_CAN_EVENT_SEND_COMPLETE (1UL << 0)
| Send complete.
#define | ARM_CAN_EVENT_RECEIVE (1UL << 1)
| Message received.
#define | ARM_CAN_EVENT_RECEIVE_OVERRUN (1UL << 2)
| Received message overrun.

## Description

Callback objects events notified via ARM_CAN_SignalObjectEvent.

The CAN driver generates callback objects events that are notified via the function ARM_CAN_SignalObjectEvent.

The following callback notification object events are generated:

## Macro Definition Documentation

## ◆ ARM_CAN_EVENT_SEND_COMPLETE

#define ARM_CAN_EVENT_SEND_COMPLETE (1UL << 0)

Send complete.

See also
  ARM_CAN_SignalObjectEvent

## ◆ ARM_CAN_EVENT_RECEIVE

#define ARM_CAN_EVENT_RECEIVE (1UL << 1)

Message received.

See also
  ARM_CAN_SignalObjectEvent

## ◆ ARM_CAN_EVENT_RECEIVE_OVERRUN

#define ARM_CAN_EVENT_RECEIVE_OVERRUN (1UL << 2)

Received message overrun.

See also
  ARM_CAN_SignalObjectEvent