| CMSIS-Driver Peripheral Interface for Middleware and Application Code |

Loading...
Searching...
No Matches
Macros
NAND Driver Strength
NAND Interface » NAND Control Codes

Specify driver strength of the NAND interface. More...

## Macros
#define | ARM_NAND_DRIVER_STRENGTH_18 (0x00UL)
| Driver Strength 2.0x = 18 Ohms.
#define | ARM_NAND_DRIVER_STRENGTH_25 (0x01UL)
| Driver Strength 1.4x = 25 Ohms.
#define | ARM_NAND_DRIVER_STRENGTH_35 (0x02UL)
| Driver Strength 1.0x = 35 Ohms (default)
#define | ARM_NAND_DRIVER_STRENGTH_50 (0x03UL)
| Driver Strength 0.7x = 50 Ohms.

## Description

Specify driver strength of the NAND interface.

The defines can be used in the function ARM_NAND_Control for the parameter arg and with the ARM_NAND_DRIVER_STRENGTH as the control code.

## Macro Definition Documentation

## ◆ ARM_NAND_DRIVER_STRENGTH_18

#define ARM_NAND_DRIVER_STRENGTH_18 (0x00UL)

Driver Strength 2.0x = 18 Ohms.

## ◆ ARM_NAND_DRIVER_STRENGTH_25

#define ARM_NAND_DRIVER_STRENGTH_25 (0x01UL)

Driver Strength 1.4x = 25 Ohms.

## ◆ ARM_NAND_DRIVER_STRENGTH_35

#define ARM_NAND_DRIVER_STRENGTH_35 (0x02UL)

Driver Strength 1.0x = 35 Ohms (default)

## ◆ ARM_NAND_DRIVER_STRENGTH_50

#define ARM_NAND_DRIVER_STRENGTH_50 (0x03UL)

Driver Strength 0.7x = 50 Ohms.