| CMSIS-Driver Peripheral Interface for Middleware and Application Code |

Loading...
Searching...
No Matches
Macros
USART Parity Bit
USART Interface » USART Control Codes

Defines the parity bit. More...

## Macros
#define | ARM_USART_PARITY_NONE (0UL << ARM_USART_PARITY_Pos)
| No Parity (default)
#define | ARM_USART_PARITY_EVEN (1UL << ARM_USART_PARITY_Pos)
| Even Parity.
#define | ARM_USART_PARITY_ODD (2UL << ARM_USART_PARITY_Pos)
| Odd Parity.

## Description

Defines the parity bit.

## Macro Definition Documentation

## ◆ ARM_USART_PARITY_NONE

#define ARM_USART_PARITY_NONE (0UL << ARM_USART_PARITY_Pos)

No Parity (default)

See also
  ARM_USART_Control

## ◆ ARM_USART_PARITY_EVEN

#define ARM_USART_PARITY_EVEN (1UL << ARM_USART_PARITY_Pos)

Even Parity.

See also
  ARM_USART_Control

## ◆ ARM_USART_PARITY_ODD

#define ARM_USART_PARITY_ODD (2UL << ARM_USART_PARITY_Pos)

Odd Parity.

See also
  ARM_USART_Control