| CMSIS-Core (Cortex-A) CMSIS-Core support for Cortex-A processor-based devices |

Loading...
Searching...
No Matches
Functions
PL1 Physical Timer Value register (CNTP_TVAL)
Core Register Access

Holds the timer value for the PL1 physical timer. More...

## Functions
__STATIC_FORCEINLINE void | __set_CNTP_TVAL (uint32_t value)
| Set CNTP_TVAL.
__STATIC_FORCEINLINE uint32_t | __get_CNTP_TVAL (void)
| Get CNTP_TVAL.

## Description

Holds the timer value for the PL1 physical timer.

Consider __get_CNTP_TVAL and __set_CNTP_TVAL to access this register.

Consider using Generic Physical Timer Functions for controlling the PL1 Timer instead.

## Function Documentation

## ◆ __get_CNTP_TVAL()

__STATIC_FORCEINLINE uint32_t __get_CNTP_TVAL | ( | void |  | ) |

Get CNTP_TVAL.

This function returns the value of the PL1 Physical Timer Value Register (CNTP_TVAL).

Returns
  CNTP_TVAL Register value

This function returns the value of the PL1 Physical Timer Value register (CNTP_TVAL).

## ◆ __set_CNTP_TVAL()

__STATIC_FORCEINLINE void __set_CNTP_TVAL | ( | uint32_t | value | ) |

Set CNTP_TVAL.

This function assigns the given value to PL1 Physical Timer Value Register (CNTP_TVAL).

Parameters

  [in] | value | CNTP_TVAL Register value to set

This function assigns the given value to PL1 Physical Timer Value register (CNTP_TVAL).