| CMSIS-Driver Peripheral Interface for Middleware and Application Code |

Loading...
Searching...
No Matches
Macros
SAI Mode
SAI Interface » SAI Control Codes » SAI Configuration

Defines Transmitter/Receiver mode. More...

## Macros
#define | ARM_SAI_MODE_MASTER (1UL << ARM_SAI_MODE_Pos)
| Master Mode.
#define | ARM_SAI_MODE_SLAVE (0UL << ARM_SAI_MODE_Pos)
| Slave Mode (default)

## Description

Defines Transmitter/Receiver mode.

## Macro Definition Documentation

## ◆ ARM_SAI_MODE_MASTER

#define ARM_SAI_MODE_MASTER (1UL << ARM_SAI_MODE_Pos)

Master Mode.

## ◆ ARM_SAI_MODE_SLAVE

#define ARM_SAI_MODE_SLAVE (0UL << ARM_SAI_MODE_Pos)

Slave Mode (default)