| CMSIS-Core (Cortex-A) CMSIS-Core support for Cortex-A processor-based devices |

Loading...
Searching...
No Matches
Data Fields
ISR_Type Struct Reference
Core Register Access » Interrupt Status Register (ISR)

Bit field declaration for ISR layout. More...

`#include <core_ca.h>`

## Data Fields
struct {
uint32_t F:1
| bit: 6 FIQ pending bit More...
uint32_t I:1
| bit: 7 IRQ pending bit More...
uint32_t A:1
| bit: 8 External abort pending bit More...
} | b
| Structure used for bit access.
uint32_t | w
| Type used for word access.

## Description

Bit field declaration for ISR layout.

## Field Documentation

## ◆ A

uint32_t ISR_Type::A

bit: 8 External abort pending bit

## ◆

struct { ... } ISR_Type::b

Structure used for bit access.

## ◆ F

uint32_t ISR_Type::F

bit: 6 FIQ pending bit

## ◆ I

uint32_t ISR_Type::I

bit: 7 IRQ pending bit

## ◆ w

uint32_t ISR_Type::w

Type used for word access.