| CMSIS-Driver Peripheral Interface for Middleware and Application Code |

Loading...
Searching...
No Matches

### - a -

- AbortSequence : ARM_DRIVER_NAND
- AbortTransfer : ARM_DRIVER_MCI
- acls : ARM_STORAGE_SECURITY_FEATURES
- Activate : ARM_DRIVER_WIFI
- active : ARM_USBD_STATE
- addr : ARM_STORAGE_BLOCK
- address_10_bit : ARM_I2C_CAPABILITIES
- ap : ARM_WIFI_CAPABILITIES
- api : ARM_DRIVER_VERSION
- arbitration_lost : ARM_I2C_STATUS
- asynchronous : ARM_SAI_CAPABILITIES, ARM_USART_CAPABILITIES
- asynchronous_ops : ARM_STORAGE_CAPABILITIES
- attributes : ARM_STORAGE_BLOCK
- auto_split : ARM_USBH_CAPABILITIES