| CMSIS-Driver Peripheral Interface for Middleware and Application Code |

Loading...
Searching...
No Matches

### - c -

- CardPower : ARM_DRIVER_MCI
- ccs : ARM_MCI_CAPABILITIES, ARM_MCI_STATUS
- ccs_timeout : ARM_MCI_CAPABILITIES
- cd_event : ARM_MCI_CAPABILITIES
- cd_state : ARM_MCI_CAPABILITIES
- ce_lines : ARM_NAND_CAPABILITIES
- ce_manual : ARM_NAND_CAPABILITIES
- ch : ARM_WIFI_CONFIG_t, ARM_WIFI_NET_INFO_t, ARM_WIFI_SCAN_INFO_t
- checksum_offload_rx_icmp : ARM_ETH_MAC_CAPABILITIES
- checksum_offload_rx_ip4 : ARM_ETH_MAC_CAPABILITIES
- checksum_offload_rx_ip6 : ARM_ETH_MAC_CAPABILITIES
- checksum_offload_rx_tcp : ARM_ETH_MAC_CAPABILITIES
- checksum_offload_rx_udp : ARM_ETH_MAC_CAPABILITIES
- checksum_offload_tx_icmp : ARM_ETH_MAC_CAPABILITIES
- checksum_offload_tx_ip4 : ARM_ETH_MAC_CAPABILITIES
- checksum_offload_tx_ip6 : ARM_ETH_MAC_CAPABILITIES
- checksum_offload_tx_tcp : ARM_ETH_MAC_CAPABILITIES
- checksum_offload_tx_udp : ARM_ETH_MAC_CAPABILITIES
- chip_level_attacks : ARM_STORAGE_SECURITY_FEATURES
- ChipEnable : ARM_DRIVER_NAND
- codeword_gap : ARM_NAND_ECC_INFO
- codeword_offset : ARM_NAND_ECC_INFO
- codeword_size : ARM_NAND_ECC_INFO
- command_active : ARM_MCI_STATUS
- command_error : ARM_MCI_STATUS
- command_timeout : ARM_MCI_STATUS
- companding : ARM_SAI_CAPABILITIES
- connected : ARM_USBH_PORT_STATE
- Control : ARM_DRIVER_CAN, ARM_DRIVER_ETH_MAC, ARM_DRIVER_I2C, ARM_DRIVER_MCI, ARM_DRIVER_NAND, ARM_DRIVER_SAI, ARM_DRIVER_SPI, ARM_DRIVER_USART
- ControlTimer : ARM_DRIVER_ETH_MAC
- correctable_bits : ARM_NAND_ECC_INFO
- cts : ARM_USART_CAPABILITIES, ARM_USART_MODEM_STATUS