| CMSIS-Driver Peripheral Interface for Middleware and Application Code |

Loading...
Searching...
No Matches
Macros
SAI Mono Mode
SAI Interface » SAI Control Codes » SAI Configuration

Defines mono mode. More...

## Macros
#define | ARM_SAI_MONO_MODE (1UL << 19)
| Mono Mode (only for I2S, MSB/LSB justified)

## Description

Defines mono mode.

## Macro Definition Documentation

## ◆ ARM_SAI_MONO_MODE

#define ARM_SAI_MONO_MODE (1UL << 19)

Mono Mode (only for I2S, MSB/LSB justified)