| CMSIS-Driver Peripheral Interface for Middleware and Application Code |

Loading...
Searching...
No Matches
Macros
WiFi Socket Function return codes
WiFi Interface » WiFi Socket

WiFi Socket Function return codes. More...

## Macros
#define | ARM_SOCKET_ERROR (-1)
| Unspecified error.
#define | ARM_SOCKET_ESOCK (-2)
| Invalid socket.
#define | ARM_SOCKET_EINVAL (-3)
| Invalid argument.
#define | ARM_SOCKET_ENOTSUP (-4)
| Operation not supported.
#define | ARM_SOCKET_ENOMEM (-5)
| Not enough memory.
#define | ARM_SOCKET_EAGAIN (-6)
| Operation would block or timed out.
#define | ARM_SOCKET_EINPROGRESS (-7)
| Operation in progress.
#define | ARM_SOCKET_ETIMEDOUT (-8)
| Operation timed out.
#define | ARM_SOCKET_EISCONN (-9)
| Socket is connected.
#define | ARM_SOCKET_ENOTCONN (-10)
| Socket is not connected.
#define | ARM_SOCKET_ECONNREFUSED (-11)
| Connection rejected by the peer.
#define | ARM_SOCKET_ECONNRESET (-12)
| Connection reset by the peer.
#define | ARM_SOCKET_ECONNABORTED (-13)
| Connection aborted locally.
#define | ARM_SOCKET_EALREADY (-14)
| Connection already in progress.
#define | ARM_SOCKET_EADDRINUSE (-15)
| Address in use.
#define | ARM_SOCKET_EHOSTNOTFOUND (-16)
| Host not found.

## Description

WiFi Socket Function return codes.

This section lists all the return errors the WiFi socket functions will return. The error codes are negative. This makes it easy to check an error when the return code is less than 0.

## Macro Definition Documentation

## ◆ ARM_SOCKET_ERROR

#define ARM_SOCKET_ERROR (-1)

Unspecified error.

See also
  WiFi Socket Function return codes

## ◆ ARM_SOCKET_ESOCK

#define ARM_SOCKET_ESOCK (-2)

Invalid socket.

See also
  WiFi Socket Function return codes

## ◆ ARM_SOCKET_EINVAL

#define ARM_SOCKET_EINVAL (-3)

Invalid argument.

See also
  WiFi Socket Function return codes

## ◆ ARM_SOCKET_ENOTSUP

#define ARM_SOCKET_ENOTSUP (-4)

Operation not supported.

See also
  WiFi Socket Function return codes

## ◆ ARM_SOCKET_ENOMEM

#define ARM_SOCKET_ENOMEM (-5)

Not enough memory.

See also
  WiFi Socket Function return codes

## ◆ ARM_SOCKET_EAGAIN

#define ARM_SOCKET_EAGAIN (-6)

Operation would block or timed out.

See also
  WiFi Socket Function return codes

## ◆ ARM_SOCKET_EINPROGRESS

#define ARM_SOCKET_EINPROGRESS (-7)

Operation in progress.

See also
  WiFi Socket Function return codes

## ◆ ARM_SOCKET_ETIMEDOUT

#define ARM_SOCKET_ETIMEDOUT (-8)

Operation timed out.

See also
  WiFi Socket Function return codes

## ◆ ARM_SOCKET_EISCONN

#define ARM_SOCKET_EISCONN (-9)

Socket is connected.

See also
  WiFi Socket Function return codes

## ◆ ARM_SOCKET_ENOTCONN

#define ARM_SOCKET_ENOTCONN (-10)

Socket is not connected.

See also
  WiFi Socket Function return codes

## ◆ ARM_SOCKET_ECONNREFUSED

#define ARM_SOCKET_ECONNREFUSED (-11)

Connection rejected by the peer.

See also
  WiFi Socket Function return codes

## ◆ ARM_SOCKET_ECONNRESET

#define ARM_SOCKET_ECONNRESET (-12)

Connection reset by the peer.

See also
  WiFi Socket Function return codes

## ◆ ARM_SOCKET_ECONNABORTED

#define ARM_SOCKET_ECONNABORTED (-13)

Connection aborted locally.

See also
  WiFi Socket Function return codes

## ◆ ARM_SOCKET_EALREADY

#define ARM_SOCKET_EALREADY (-14)

Connection already in progress.

See also
  WiFi Socket Function return codes

## ◆ ARM_SOCKET_EADDRINUSE

#define ARM_SOCKET_EADDRINUSE (-15)

Address in use.

See also
  WiFi Socket Function return codes

## ◆ ARM_SOCKET_EHOSTNOTFOUND

#define ARM_SOCKET_EHOSTNOTFOUND (-16)

Host not found.

See also
  WiFi Socket Function return codes