| CMSIS-Driver Peripheral Interface for Middleware and Application Code |

Loading...
Searching...
No Matches
Macros
USBD Endpoint Events
USB Interface » USB Device Interface

The USB Device driver generates Endpoint call back events that are notified via the function ARM_USBD_SignalEndpointEvent. More...

## Macros
#define | ARM_USBD_EVENT_SETUP (1UL << 0)
| SETUP Packet.
#define | ARM_USBD_EVENT_OUT (1UL << 1)
| OUT Packet(s)
#define | ARM_USBD_EVENT_IN (1UL << 2)
| IN Packet(s)

## Description

The USB Device driver generates Endpoint call back events that are notified via the function ARM_USBD_SignalEndpointEvent.

This section provides the event values for the ARM_USBD_SignalEndpointEvent callback function.

The following call back notification events are generated:

## Macro Definition Documentation

## ◆ ARM_USBD_EVENT_SETUP

#define ARM_USBD_EVENT_SETUP (1UL << 0)

SETUP Packet.

## ◆ ARM_USBD_EVENT_OUT

#define ARM_USBD_EVENT_OUT (1UL << 1)

OUT Packet(s)

## ◆ ARM_USBD_EVENT_IN

#define ARM_USBD_EVENT_IN (1UL << 2)

IN Packet(s)