| CMSIS-Driver Peripheral Interface for Middleware and Application Code |

Loading...
Searching...
No Matches
Macros
Ethernet MAC Frame Transmit Flags
Ethernet Interface » Ethernet MAC Interface

Specify frame transmit flags. More...

## Macros
#define | ARM_ETH_MAC_TX_FRAME_FRAGMENT (1UL << 0)
| Indicate frame fragment.
#define | ARM_ETH_MAC_TX_FRAME_EVENT (1UL << 1)
| Generate event when frame is transmitted.
#define | ARM_ETH_MAC_TX_FRAME_TIMESTAMP (1UL << 2)
| Capture frame time stamp.

## Description

Specify frame transmit flags.

## Macro Definition Documentation

## ◆ ARM_ETH_MAC_TX_FRAME_FRAGMENT

#define ARM_ETH_MAC_TX_FRAME_FRAGMENT (1UL << 0)

Indicate frame fragment.

See also
  ARM_ETH_MAC_SendFrame

## ◆ ARM_ETH_MAC_TX_FRAME_EVENT

#define ARM_ETH_MAC_TX_FRAME_EVENT (1UL << 1)

Generate event when frame is transmitted.

See also
  ARM_ETH_MAC_SendFrame

## ◆ ARM_ETH_MAC_TX_FRAME_TIMESTAMP

#define ARM_ETH_MAC_TX_FRAME_TIMESTAMP (1UL << 2)

Capture frame time stamp.

See also
  ARM_ETH_MAC_SendFrame