| CMSIS-Driver Peripheral Interface for Middleware and Application Code |

Loading...
Searching...
No Matches
Macros
WiFi Events
WiFi Interface » WiFi Control

The WiFi driver generates call back events that are notified via the function ARM_WIFI_SignalEvent. More...

## Macros
#define | ARM_WIFI_EVENT_AP_CONNECT (1UL << 0)
| Access Point: Station has connected; arg = &mac, mac (uint8_t[6])
#define | ARM_WIFI_EVENT_AP_DISCONNECT (1UL << 1)
| Access Point: Station has disconnected; arg = &mac, mac (uint8_t[6])
#define | ARM_WIFI_EVENT_ETH_RX_FRAME (1UL << 4)
| Ethernet Frame Received (in bypass mode only); arg = interface (0 = Station, 1 = Access Point)

## Description

The WiFi driver generates call back events that are notified via the function ARM_WIFI_SignalEvent.

The following call back notification events are generated:

## Macro Definition Documentation

## ◆ ARM_WIFI_EVENT_AP_CONNECT

#define ARM_WIFI_EVENT_AP_CONNECT (1UL << 0)

Access Point: Station has connected; arg = &mac, mac (uint8_t[6])

## ◆ ARM_WIFI_EVENT_AP_DISCONNECT

#define ARM_WIFI_EVENT_AP_DISCONNECT (1UL << 1)

Access Point: Station has disconnected; arg = &mac, mac (uint8_t[6])

## ◆ ARM_WIFI_EVENT_ETH_RX_FRAME

#define ARM_WIFI_EVENT_ETH_RX_FRAME (1UL << 4)

Ethernet Frame Received (in bypass mode only); arg = interface (0 = Station, 1 = Access Point)