| CMSIS-Driver Peripheral Interface for Middleware and Application Code |

Loading...
Searching...
No Matches
Macros
USART Stop Bits
USART Interface » USART Control Codes

Defines the number of stop bits. More...

## Macros
#define | ARM_USART_STOP_BITS_1 (0UL << ARM_USART_STOP_BITS_Pos)
| 1 Stop bit (default)
#define | ARM_USART_STOP_BITS_2 (1UL << ARM_USART_STOP_BITS_Pos)
| 2 Stop bits
#define | ARM_USART_STOP_BITS_1_5 (2UL << ARM_USART_STOP_BITS_Pos)
| 1.5 Stop bits
#define | ARM_USART_STOP_BITS_0_5 (3UL << ARM_USART_STOP_BITS_Pos)
| 0.5 Stop bits

## Description

Defines the number of stop bits.

See also
  ARM_USART_Control

## Macro Definition Documentation

## ◆ ARM_USART_STOP_BITS_1

#define ARM_USART_STOP_BITS_1 (0UL << ARM_USART_STOP_BITS_Pos)

1 Stop bit (default)

See also
  ARM_USART_Control

## ◆ ARM_USART_STOP_BITS_2

#define ARM_USART_STOP_BITS_2 (1UL << ARM_USART_STOP_BITS_Pos)

2 Stop bits

See also
  ARM_USART_Control

## ◆ ARM_USART_STOP_BITS_1_5

#define ARM_USART_STOP_BITS_1_5 (2UL << ARM_USART_STOP_BITS_Pos)

1.5 Stop bits

See also
  ARM_USART_Control

## ◆ ARM_USART_STOP_BITS_0_5

#define ARM_USART_STOP_BITS_0_5 (3UL << ARM_USART_STOP_BITS_Pos)

0.5 Stop bits

See also
  ARM_USART_Control