| CMSIS-Driver Peripheral Interface for Middleware and Application Code |

Loading...
Searching...
No Matches
Enumerations
CAN Bus Communication Mode
CAN Interface » CAN Control Codes

Set or initialize the CAN bus. More...

## Enumerations
enum | ARM_CAN_MODE { ARM_CAN_MODE_INITIALIZATION , ARM_CAN_MODE_NORMAL , ARM_CAN_MODE_RESTRICTED , ARM_CAN_MODE_MONITOR , ARM_CAN_MODE_LOOPBACK_INTERNAL , ARM_CAN_MODE_LOOPBACK_EXTERNAL }

## Description

Set or initialize the CAN bus.

## Enumeration Type Documentation

## ◆ ARM_CAN_MODE

enum ARM_CAN_MODE

The enumerations below initialize and set the bus communication mode.

Parameter for:

- ARM_CAN_SetMode

Enumerator
ARM_CAN_MODE_INITIALIZATION | Initialization mode.
ARM_CAN_MODE_NORMAL | Normal operation mode.
ARM_CAN_MODE_RESTRICTED | Restricted operation mode.
ARM_CAN_MODE_MONITOR | Bus monitoring mode.
ARM_CAN_MODE_LOOPBACK_INTERNAL | Loopback internal mode.
ARM_CAN_MODE_LOOPBACK_EXTERNAL | Loopback external mode.