| CMSIS-Core (Cortex-A) CMSIS-Core support for Cortex-A processor-based devices |

Loading...
Searching...
No Matches
Data Structures | Functions
ref_timer.txt File Reference

## Data Structures
union | CNTP_CTL_Type
| Physical Timer Control register. More...

## Functions
__STATIC_INLINE void | PL1_SetCounterFrequency (uint32_t value)
| Configures the frequency the timer shall run at.
__STATIC_INLINE void | PL1_SetLoadValue (uint32_t value)
| Sets the reset value of the timer.
__STATIC_INLINE uint32_t | PL1_GetCurrentValue ()
| Get the current counter value.
__STATIC_INLINE uint64_t | PL1_GetCurrentPhysicalValue (void)
| Get the current physical counter value.
__STATIC_INLINE void | PL1_SetPhysicalCompareValue (uint64_t value)
| Set the physical compare value.
__STATIC_INLINE uint64_t | PL1_GetPhysicalCompareValue (void)
| Get the physical compare value.
__STATIC_INLINE void | PL1_SetControl (uint32_t value)
| Configure the timer by setting the control value.
__STATIC_INLINE uint32_t | PL1_GetControl ()
| Get the control value.