| CMSIS-Core (Cortex-M) CMSIS-Core support for Cortex-M processor-based devices |

Loading...
Searching...
No Matches
Macros
PMU Events for Armv8.1-M
PMU Functions for Armv8.1-M

IDs for Armv8.1-M architecture defined events. More...

## Macros
#define | ARM_PMU_BF_CANCEL 0x0109
| Branch future instruction not taken.
#define | ARM_PMU_BF_RETIRED 0x0104
| Branch future instruction architecturally executed and condition code check pass.
#define | ARM_PMU_BF_SPEC 0x0105
| Branch future instruction speculatively executed and condition code check pass.
#define | ARM_PMU_BR_IMMED_RETIRED 0x000D
| Immediate branch architecturally executed.
#define | ARM_PMU_BR_MIS_PRED 0x0010
| Mispredicted or not predicted branch speculatively executed.
#define | ARM_PMU_BR_MIS_PRED_RETIRED 0x0022
| Mispredicted branch instruction architecturally executed.
#define | ARM_PMU_BR_PRED 0x0012
| Predictable branch speculatively executed.
#define | ARM_PMU_BR_RETIRED 0x0021
| Branch instruction architecturally executed.
#define | ARM_PMU_BR_RETURN_RETIRED 0x000E
| Function return instruction architecturally executed and the condition code check pass.
#define | ARM_PMU_BUS_ACCESS 0x0019
| Bus access.
#define | ARM_PMU_BUS_CYCLES 0x001D
| Bus cycles.
#define | ARM_PMU_CHAIN 0x001E
| For an odd numbered counter, increment when an overflow occurs on the preceding even-numbered counter on the same PE.
#define | ARM_PMU_CPU_CYCLES 0x0011
| Cycle.
#define | ARM_PMU_CTI_TRIGOUT4 0x4018
| Cross-trigger Interface output trigger 4.
#define | ARM_PMU_CTI_TRIGOUT5 0x4019
| Cross-trigger Interface output trigger 5.
#define | ARM_PMU_CTI_TRIGOUT6 0x401A
| Cross-trigger Interface output trigger 6.
#define | ARM_PMU_CTI_TRIGOUT7 0x401B
| Cross-trigger Interface output trigger 7.
#define | ARM_PMU_DTCM_ACCESS 0x4008
| Data TCM access.
#define | ARM_PMU_DWT_CMPMATCH0 0x0118
| DWT comparator 0 match.
#define | ARM_PMU_DWT_CMPMATCH1 0x0119
| DWT comparator 1 match.
#define | ARM_PMU_DWT_CMPMATCH2 0x011A
| DWT comparator 2 match.
#define | ARM_PMU_DWT_CMPMATCH3 0x011B
| DWT comparator 3 match.
#define | ARM_PMU_EXC_RETURN 0x000A
| Exception return instruction architecturally executed and the condition code check pass.
#define | ARM_PMU_EXC_TAKEN 0x0009
| Exception entry.
#define | ARM_PMU_INST_RETIRED 0x0008
| Instruction architecturally executed.
#define | ARM_PMU_INST_SPEC 0x001B
| Instruction speculatively executed.
#define | ARM_PMU_ITCM_ACCESS 0x4007
| Instruction TCM access.
#define | ARM_PMU_L1D_CACHE 0x0004
| L1 D-Cache access.
#define | ARM_PMU_L1D_CACHE_ALLOCATE 0x001F
| Level 1 data cache allocation without refill.
#define | ARM_PMU_L1D_CACHE_MISS_RD 0x0039
| Level 1 data cache read miss.
#define | ARM_PMU_L1D_CACHE_RD 0x0040
| Level 1 data cache read.
#define | ARM_PMU_L1D_CACHE_REFILL 0x0003
| L1 D-Cache refill.
#define | ARM_PMU_L1D_CACHE_WB 0x0015
| Level 1 data cache write-back.
#define | ARM_PMU_L1I_CACHE 0x0014
| Level 1 instruction cache access.
#define | ARM_PMU_L1I_CACHE_REFILL 0x0001
| L1 I-Cache refill.
#define | ARM_PMU_L2D_CACHE 0x0016
| Level 2 data cache access.
#define | ARM_PMU_L2D_CACHE_ALLOCATE 0x0020
| Level 2 data cache allocation without refill.
#define | ARM_PMU_L2D_CACHE_REFILL 0x0017
| Level 2 data cache refill.
#define | ARM_PMU_L2D_CACHE_WB 0x0018
| Level 2 data cache write-back.
#define | ARM_PMU_L2I_CACHE 0x0027
| Level 2 instruction cache access.
#define | ARM_PMU_L2I_CACHE_REFILL 0x0028
| Level 2 instruction cache refill.
#define | ARM_PMU_L3D_CACHE 0x002B
| Level 3 data cache access.
#define | ARM_PMU_L3D_CACHE_ALLOCATE 0x0029
| Level 3 data cache allocation without refill.
#define | ARM_PMU_L3D_CACHE_REFILL 0x002A
| Level 3 data cache refill.
#define | ARM_PMU_L3D_CACHE_WB 0x002C
| Level 3 data cache write-back.
#define | ARM_PMU_LD_RETIRED 0x0006
| Memory-reading instruction architecturally executed and condition code check pass.
#define | ARM_PMU_LE_CANCEL 0x0108
| Loop end instruction not taken.
#define | ARM_PMU_LE_RETIRED 0x0100
| Loop end instruction executed.
#define | ARM_PMU_LE_SPEC 0x0101
| Loop end instruction speculatively executed.
#define | ARM_PMU_LL_CACHE_MISS_RD 0x0037
| Last level data cache read miss.
#define | ARM_PMU_LL_CACHE_RD 0x0036
| Last level data cache read.
#define | ARM_PMU_MEM_ACCESS 0x0013
| Data memory access.
#define | ARM_PMU_MEMORY_ERROR 0x001A
| Local memory error.
#define | ARM_PMU_MVE_FP_HP_RETIRED 0x0208
| MVE half-precision floating-point instruction architecturally executed.
#define | ARM_PMU_MVE_FP_HP_SPEC 0x0209
| MVE half-precision floating-point instruction speculatively executed.
#define | ARM_PMU_MVE_FP_MAC_RETIRED 0x0214
| MVE floating-point multiply or multiply-accumulate instruction architecturally executed.
#define | ARM_PMU_MVE_FP_MAC_SPEC 0x0215
| MVE floating-point multiply or multiply-accumulate instruction speculatively executed.
#define | ARM_PMU_MVE_FP_RETIRED 0x0204
| MVE floating-point instruction architecturally executed.
#define | ARM_PMU_MVE_FP_SP_RETIRED 0x020C
| MVE single-precision floating-point instruction architecturally executed.
#define | ARM_PMU_MVE_FP_SP_SPEC 0x020D
| MVE single-precision floating-point instruction speculatively executed.
#define | ARM_PMU_MVE_FP_SPEC 0x0205
| MVE floating-point instruction speculatively executed.
#define | ARM_PMU_MVE_INST_RETIRED 0x0200
| MVE instruction architecturally executed.
#define | ARM_PMU_MVE_INST_SPEC 0x0201
| MVE instruction speculatively executed.
#define | ARM_PMU_MVE_INT_MAC_RETIRED 0x0228
| MVE multiply or multiply-accumulate instruction architecturally executed.
#define | ARM_PMU_MVE_INT_MAC_SPEC 0x0229
| MVE multiply or multiply-accumulate instruction speculatively executed.
#define | ARM_PMU_MVE_INT_RETIRED 0x0224
| MVE integer instruction architecturally executed.
#define | ARM_PMU_MVE_INT_SPEC 0x0225
| MVE integer instruction speculatively executed.
#define | ARM_PMU_MVE_LD_CONTIG_RETIRED 0x0248
| MVE contiguous load instruction architecturally executed.
#define | ARM_PMU_MVE_LD_CONTIG_SPEC 0x0249
| MVE contiguous load instruction speculatively executed.
#define | ARM_PMU_MVE_LD_MULTI_RETIRED 0x0260
| MVE memory load instruction targeting multiple registers architecturally executed.
#define | ARM_PMU_MVE_LD_MULTI_SPEC 0x0261
| MVE memory load instruction targeting multiple registers speculatively executed.
#define | ARM_PMU_MVE_LD_NONCONTIG_RETIRED 0x0254
| MVE non-contiguous load instruction architecturally executed.
#define | ARM_PMU_MVE_LD_NONCONTIG_SPEC 0x0255
| MVE non-contiguous load instruction speculatively executed.
#define | ARM_PMU_MVE_LD_RETIRED 0x023C
| MVE load instruction architecturally executed.
#define | ARM_PMU_MVE_LD_SPEC 0x023D
| MVE load instruction speculatively executed.
#define | ARM_PMU_MVE_LD_UNALIGNED_RETIRED 0x0290
| MVE unaligned load instruction architecturally executed.
#define | ARM_PMU_MVE_LD_UNALIGNED_SPEC 0x0291
| MVE unaligned load instruction speculatively executed.
#define | ARM_PMU_MVE_LDST_CONTIG_RETIRED 0x0244
| MVE contiguous load or store instruction architecturally executed.
#define | ARM_PMU_MVE_LDST_CONTIG_SPEC 0x0245
| MVE contiguous load or store instruction speculatively executed.
#define | ARM_PMU_MVE_LDST_MULTI_RETIRED 0x025C
| MVE memory instruction targeting multiple registers architecturally executed.
#define | ARM_PMU_MVE_LDST_MULTI_SPEC 0x025D
| MVE memory instruction targeting multiple registers speculatively executed.
#define | ARM_PMU_MVE_LDST_NONCONTIG_RETIRED 0x0250
| MVE non-contiguous load or store instruction architecturally executed.
#define | ARM_PMU_MVE_LDST_NONCONTIG_SPEC 0x0251
| MVE non-contiguous load or store instruction speculatively executed.
#define | ARM_PMU_MVE_LDST_RETIRED 0x0238
| MVE load or store instruction architecturally executed.
#define | ARM_PMU_MVE_LDST_SPEC 0x0239
| MVE load or store instruction speculatively executed.
#define | ARM_PMU_MVE_LDST_UNALIGNED_NONCONTIG_RETIRED 0x0298
| MVE unaligned noncontiguous load or store instruction architecturally executed.
#define | ARM_PMU_MVE_LDST_UNALIGNED_NONCONTIG_SPEC 0x0299
| MVE unaligned noncontiguous load or store instruction speculatively executed.
#define | ARM_PMU_MVE_LDST_UNALIGNED_RETIRED 0x028C
| MVE unaligned memory load or store instruction architecturally executed.
#define | ARM_PMU_MVE_LDST_UNALIGNED_SPEC 0x028D
| MVE unaligned memory load or store instruction speculatively executed.
#define | ARM_PMU_MVE_PRED 0x02B8
| Cycles where one or more predicated beats architecturally executed.
#define | ARM_PMU_MVE_ST_CONTIG_RETIRED 0x024C
| MVE contiguous store instruction architecturally executed.
#define | ARM_PMU_MVE_ST_CONTIG_SPEC 0x024D
| MVE contiguous store instruction speculatively executed.
#define | ARM_PMU_MVE_ST_MULTI_RETIRED 0x0261
| MVE memory store instruction targeting multiple registers architecturally executed.
#define | ARM_PMU_MVE_ST_MULTI_SPEC 0x0265
| MVE memory store instruction targeting multiple registers speculatively executed.
#define | ARM_PMU_MVE_ST_NONCONTIG_RETIRED 0x0258
| MVE non-contiguous store instruction architecturally executed.
#define | ARM_PMU_MVE_ST_NONCONTIG_SPEC 0x0259
| MVE non-contiguous store instruction speculatively executed.
#define | ARM_PMU_MVE_ST_RETIRED 0x0240
| MVE store instruction architecturally executed.
#define | ARM_PMU_MVE_ST_SPEC 0x0241
| MVE store instruction speculatively executed.
#define | ARM_PMU_MVE_ST_UNALIGNED_RETIRED 0x0294
| MVE unaligned store instruction architecturally executed.
#define | ARM_PMU_MVE_ST_UNALIGNED_SPEC 0x0295
| MVE unaligned store instruction speculatively executed.
#define | ARM_PMU_MVE_STALL 0x02CC
| Stall cycles caused by an MVE instruction.
#define | ARM_PMU_MVE_STALL_BREAK 0x02D3
| Stall cycles caused by an MVE chain break.
#define | ARM_PMU_MVE_STALL_DEPENDENCY 0x02D4
| Stall cycles caused by MVE register dependency.
#define | ARM_PMU_MVE_STALL_RESOURCE 0x02CD
| Stall cycles caused by an MVE instruction because of resource conflicts.
#define | ARM_PMU_MVE_STALL_RESOURCE_FP 0x02CF
| Stall cycles caused by an MVE instruction because of floating-point resource conflicts.
#define | ARM_PMU_MVE_STALL_RESOURCE_INT 0x02D0
| Stall cycles caused by an MVE instruction because of integer resource conflicts.
#define | ARM_PMU_MVE_STALL_RESOURCE_MEM 0x02CE
| Stall cycles caused by an MVE instruction because of memory resource conflicts.
#define | ARM_PMU_MVE_VREDUCE_FP_RETIRED 0x02A4
| MVE floating-point vector reduction instruction architecturally executed.
#define | ARM_PMU_MVE_VREDUCE_FP_SPEC 0x02A5
| MVE floating-point vector reduction instruction speculatively executed.
#define | ARM_PMU_MVE_VREDUCE_INT_RETIRED 0x02A8
| MVE integer vector reduction instruction architecturally executed.
#define | ARM_PMU_MVE_VREDUCE_INT_SPEC 0x02A9
| MVE integer vector reduction instruction speculatively executed.
#define | ARM_PMU_MVE_VREDUCE_RETIRED 0x02A0
| MVE vector reduction instruction architecturally executed.
#define | ARM_PMU_MVE_VREDUCE_SPEC 0x02A1
| MVE vector reduction instruction speculatively executed.
#define | ARM_PMU_OP_COMPLETE 0x003A
| Operation retired.
#define | ARM_PMU_OP_SPEC 0x003B
| Operation speculatively executed.
#define | ARM_PMU_PC_WRITE_RETIRED 0x000C
| Software change to the Program Counter (PC). Instruction is architecturally executed and condition code check pass.
#define | ARM_PMU_SE_CALL_NS 0x0115
| Call to non-secure function, resulting in Security state change.
#define | ARM_PMU_SE_CALL_S 0x0114
| Call to secure function, resulting in Security state change.
#define | ARM_PMU_ST_RETIRED 0x0007
| Memory-writing instruction architecturally executed and condition code check pass.
#define | ARM_PMU_STALL 0x003C
| Stall cycle for instruction or operation not sent for execution.
#define | ARM_PMU_STALL_BACKEND 0x0024
| No operation issued because of the backend.
#define | ARM_PMU_STALL_FRONTEND 0x0023
| No operation issued because of the frontend.
#define | ARM_PMU_STALL_OP 0x003F
| Instruction or operation slots not occupied each cycle.
#define | ARM_PMU_STALL_OP_BACKEND 0x003D
| Stall cycle for instruction or operation not sent for execution due to pipeline backend.
#define | ARM_PMU_STALL_OP_FRONTEND 0x003E
| Stall cycle for instruction or operation not sent for execution due to pipeline frontend.
#define | ARM_PMU_SW_INCR 0x0000
| Software update to the PMU_SWINC register, architecturally executed and condition code check pass.
#define | ARM_PMU_TRCEXTOUT0 0x4010
| ETM external output 0.
#define | ARM_PMU_TRCEXTOUT1 0x4011
| ETM external output 1.
#define | ARM_PMU_TRCEXTOUT2 0x4012
| ETM external output 2.
#define | ARM_PMU_TRCEXTOUT3 0x4013
| ETM external output 3.
#define | ARM_PMU_UNALIGNED_LDST_RETIRED 0x000F
| Unaligned memory memory-reading or memory-writing instruction architecturally executed and condition code check pass.

## Description

IDs for Armv8.1-M architecture defined events.

These events are available on all Armv8.1-M devices including a PMU.

## Macro Definition Documentation

## ◆ ARM_PMU_BF_CANCEL

#define ARM_PMU_BF_CANCEL 0x0109

Branch future instruction not taken.

## ◆ ARM_PMU_BF_RETIRED

#define ARM_PMU_BF_RETIRED 0x0104

Branch future instruction architecturally executed and condition code check pass.

## ◆ ARM_PMU_BF_SPEC

#define ARM_PMU_BF_SPEC 0x0105

Branch future instruction speculatively executed and condition code check pass.

## ◆ ARM_PMU_BR_IMMED_RETIRED

#define ARM_PMU_BR_IMMED_RETIRED 0x000D

Immediate branch architecturally executed.

## ◆ ARM_PMU_BR_MIS_PRED

#define ARM_PMU_BR_MIS_PRED 0x0010

Mispredicted or not predicted branch speculatively executed.

## ◆ ARM_PMU_BR_MIS_PRED_RETIRED

#define ARM_PMU_BR_MIS_PRED_RETIRED 0x0022

Mispredicted branch instruction architecturally executed.

## ◆ ARM_PMU_BR_PRED

#define ARM_PMU_BR_PRED 0x0012

Predictable branch speculatively executed.

## ◆ ARM_PMU_BR_RETIRED

#define ARM_PMU_BR_RETIRED 0x0021

Branch instruction architecturally executed.

## ◆ ARM_PMU_BR_RETURN_RETIRED

#define ARM_PMU_BR_RETURN_RETIRED 0x000E

Function return instruction architecturally executed and the condition code check pass.

## ◆ ARM_PMU_BUS_ACCESS

#define ARM_PMU_BUS_ACCESS 0x0019

Bus access.

## ◆ ARM_PMU_BUS_CYCLES

#define ARM_PMU_BUS_CYCLES 0x001D

Bus cycles.

## ◆ ARM_PMU_CHAIN

#define ARM_PMU_CHAIN 0x001E

For an odd numbered counter, increment when an overflow occurs on the preceding even-numbered counter on the same PE.

## ◆ ARM_PMU_CPU_CYCLES

#define ARM_PMU_CPU_CYCLES 0x0011

Cycle.

## ◆ ARM_PMU_CTI_TRIGOUT4

#define ARM_PMU_CTI_TRIGOUT4 0x4018

Cross-trigger Interface output trigger 4.

## ◆ ARM_PMU_CTI_TRIGOUT5

#define ARM_PMU_CTI_TRIGOUT5 0x4019

Cross-trigger Interface output trigger 5.

## ◆ ARM_PMU_CTI_TRIGOUT6

#define ARM_PMU_CTI_TRIGOUT6 0x401A

Cross-trigger Interface output trigger 6.

## ◆ ARM_PMU_CTI_TRIGOUT7

#define ARM_PMU_CTI_TRIGOUT7 0x401B

Cross-trigger Interface output trigger 7.

## ◆ ARM_PMU_DTCM_ACCESS

#define ARM_PMU_DTCM_ACCESS 0x4008

Data TCM access.

## ◆ ARM_PMU_DWT_CMPMATCH0

#define ARM_PMU_DWT_CMPMATCH0 0x0118

DWT comparator 0 match.

## ◆ ARM_PMU_DWT_CMPMATCH1

#define ARM_PMU_DWT_CMPMATCH1 0x0119

DWT comparator 1 match.

## ◆ ARM_PMU_DWT_CMPMATCH2

#define ARM_PMU_DWT_CMPMATCH2 0x011A

DWT comparator 2 match.

## ◆ ARM_PMU_DWT_CMPMATCH3

#define ARM_PMU_DWT_CMPMATCH3 0x011B

DWT comparator 3 match.

## ◆ ARM_PMU_EXC_RETURN

#define ARM_PMU_EXC_RETURN 0x000A

Exception return instruction architecturally executed and the condition code check pass.

## ◆ ARM_PMU_EXC_TAKEN

#define ARM_PMU_EXC_TAKEN 0x0009

Exception entry.

## ◆ ARM_PMU_INST_RETIRED

#define ARM_PMU_INST_RETIRED 0x0008

Instruction architecturally executed.

## ◆ ARM_PMU_INST_SPEC

#define ARM_PMU_INST_SPEC 0x001B

Instruction speculatively executed.

## ◆ ARM_PMU_ITCM_ACCESS

#define ARM_PMU_ITCM_ACCESS 0x4007

Instruction TCM access.

## ◆ ARM_PMU_L1D_CACHE

#define ARM_PMU_L1D_CACHE 0x0004

L1 D-Cache access.

## ◆ ARM_PMU_L1D_CACHE_ALLOCATE

#define ARM_PMU_L1D_CACHE_ALLOCATE 0x001F

Level 1 data cache allocation without refill.

## ◆ ARM_PMU_L1D_CACHE_MISS_RD

#define ARM_PMU_L1D_CACHE_MISS_RD 0x0039

Level 1 data cache read miss.

## ◆ ARM_PMU_L1D_CACHE_RD

#define ARM_PMU_L1D_CACHE_RD 0x0040

Level 1 data cache read.

## ◆ ARM_PMU_L1D_CACHE_REFILL

#define ARM_PMU_L1D_CACHE_REFILL 0x0003

L1 D-Cache refill.

## ◆ ARM_PMU_L1D_CACHE_WB

#define ARM_PMU_L1D_CACHE_WB 0x0015

Level 1 data cache write-back.

## ◆ ARM_PMU_L1I_CACHE

#define ARM_PMU_L1I_CACHE 0x0014

Level 1 instruction cache access.

## ◆ ARM_PMU_L1I_CACHE_REFILL

#define ARM_PMU_L1I_CACHE_REFILL 0x0001

L1 I-Cache refill.

## ◆ ARM_PMU_L2D_CACHE

#define ARM_PMU_L2D_CACHE 0x0016

Level 2 data cache access.

## ◆ ARM_PMU_L2D_CACHE_ALLOCATE

#define ARM_PMU_L2D_CACHE_ALLOCATE 0x0020

Level 2 data cache allocation without refill.

## ◆ ARM_PMU_L2D_CACHE_REFILL

#define ARM_PMU_L2D_CACHE_REFILL 0x0017

Level 2 data cache refill.

## ◆ ARM_PMU_L2D_CACHE_WB

#define ARM_PMU_L2D_CACHE_WB 0x0018

Level 2 data cache write-back.

## ◆ ARM_PMU_L2I_CACHE

#define ARM_PMU_L2I_CACHE 0x0027

Level 2 instruction cache access.

## ◆ ARM_PMU_L2I_CACHE_REFILL

#define ARM_PMU_L2I_CACHE_REFILL 0x0028

Level 2 instruction cache refill.

## ◆ ARM_PMU_L3D_CACHE

#define ARM_PMU_L3D_CACHE 0x002B

Level 3 data cache access.

## ◆ ARM_PMU_L3D_CACHE_ALLOCATE

#define ARM_PMU_L3D_CACHE_ALLOCATE 0x0029

Level 3 data cache allocation without refill.

## ◆ ARM_PMU_L3D_CACHE_REFILL

#define ARM_PMU_L3D_CACHE_REFILL 0x002A

Level 3 data cache refill.

## ◆ ARM_PMU_L3D_CACHE_WB

#define ARM_PMU_L3D_CACHE_WB 0x002C

Level 3 data cache write-back.

## ◆ ARM_PMU_LD_RETIRED

#define ARM_PMU_LD_RETIRED 0x0006

Memory-reading instruction architecturally executed and condition code check pass.

## ◆ ARM_PMU_LE_CANCEL

#define ARM_PMU_LE_CANCEL 0x0108

Loop end instruction not taken.

## ◆ ARM_PMU_LE_RETIRED

#define ARM_PMU_LE_RETIRED 0x0100

Loop end instruction executed.

## ◆ ARM_PMU_LE_SPEC

#define ARM_PMU_LE_SPEC 0x0101

Loop end instruction speculatively executed.

## ◆ ARM_PMU_LL_CACHE_MISS_RD

#define ARM_PMU_LL_CACHE_MISS_RD 0x0037

Last level data cache read miss.

## ◆ ARM_PMU_LL_CACHE_RD

#define ARM_PMU_LL_CACHE_RD 0x0036

Last level data cache read.

## ◆ ARM_PMU_MEM_ACCESS

#define ARM_PMU_MEM_ACCESS 0x0013

Data memory access.

## ◆ ARM_PMU_MEMORY_ERROR

#define ARM_PMU_MEMORY_ERROR 0x001A

Local memory error.

## ◆ ARM_PMU_MVE_FP_HP_RETIRED

#define ARM_PMU_MVE_FP_HP_RETIRED 0x0208

MVE half-precision floating-point instruction architecturally executed.

## ◆ ARM_PMU_MVE_FP_HP_SPEC

#define ARM_PMU_MVE_FP_HP_SPEC 0x0209

MVE half-precision floating-point instruction speculatively executed.

## ◆ ARM_PMU_MVE_FP_MAC_RETIRED

#define ARM_PMU_MVE_FP_MAC_RETIRED 0x0214

MVE floating-point multiply or multiply-accumulate instruction architecturally executed.

## ◆ ARM_PMU_MVE_FP_MAC_SPEC

#define ARM_PMU_MVE_FP_MAC_SPEC 0x0215

MVE floating-point multiply or multiply-accumulate instruction speculatively executed.

## ◆ ARM_PMU_MVE_FP_RETIRED

#define ARM_PMU_MVE_FP_RETIRED 0x0204

MVE floating-point instruction architecturally executed.

## ◆ ARM_PMU_MVE_FP_SP_RETIRED

#define ARM_PMU_MVE_FP_SP_RETIRED 0x020C

MVE single-precision floating-point instruction architecturally executed.

## ◆ ARM_PMU_MVE_FP_SP_SPEC

#define ARM_PMU_MVE_FP_SP_SPEC 0x020D

MVE single-precision floating-point instruction speculatively executed.

## ◆ ARM_PMU_MVE_FP_SPEC

#define ARM_PMU_MVE_FP_SPEC 0x0205

MVE floating-point instruction speculatively executed.

## ◆ ARM_PMU_MVE_INST_RETIRED

#define ARM_PMU_MVE_INST_RETIRED 0x0200

MVE instruction architecturally executed.

## ◆ ARM_PMU_MVE_INST_SPEC

#define ARM_PMU_MVE_INST_SPEC 0x0201

MVE instruction speculatively executed.

## ◆ ARM_PMU_MVE_INT_MAC_RETIRED

#define ARM_PMU_MVE_INT_MAC_RETIRED 0x0228

MVE multiply or multiply-accumulate instruction architecturally executed.

## ◆ ARM_PMU_MVE_INT_MAC_SPEC

#define ARM_PMU_MVE_INT_MAC_SPEC 0x0229

MVE multiply or multiply-accumulate instruction speculatively executed.

## ◆ ARM_PMU_MVE_INT_RETIRED

#define ARM_PMU_MVE_INT_RETIRED 0x0224

MVE integer instruction architecturally executed.

## ◆ ARM_PMU_MVE_INT_SPEC

#define ARM_PMU_MVE_INT_SPEC 0x0225

MVE integer instruction speculatively executed.

## ◆ ARM_PMU_MVE_LD_CONTIG_RETIRED

#define ARM_PMU_MVE_LD_CONTIG_RETIRED 0x0248

MVE contiguous load instruction architecturally executed.

## ◆ ARM_PMU_MVE_LD_CONTIG_SPEC

#define ARM_PMU_MVE_LD_CONTIG_SPEC 0x0249

MVE contiguous load instruction speculatively executed.

## ◆ ARM_PMU_MVE_LD_MULTI_RETIRED

#define ARM_PMU_MVE_LD_MULTI_RETIRED 0x0260

MVE memory load instruction targeting multiple registers architecturally executed.

## ◆ ARM_PMU_MVE_LD_MULTI_SPEC

#define ARM_PMU_MVE_LD_MULTI_SPEC 0x0261

MVE memory load instruction targeting multiple registers speculatively executed.

## ◆ ARM_PMU_MVE_LD_NONCONTIG_RETIRED

#define ARM_PMU_MVE_LD_NONCONTIG_RETIRED 0x0254

MVE non-contiguous load instruction architecturally executed.

## ◆ ARM_PMU_MVE_LD_NONCONTIG_SPEC

#define ARM_PMU_MVE_LD_NONCONTIG_SPEC 0x0255

MVE non-contiguous load instruction speculatively executed.

## ◆ ARM_PMU_MVE_LD_RETIRED

#define ARM_PMU_MVE_LD_RETIRED 0x023C

MVE load instruction architecturally executed.

## ◆ ARM_PMU_MVE_LD_SPEC

#define ARM_PMU_MVE_LD_SPEC 0x023D

MVE load instruction speculatively executed.

## ◆ ARM_PMU_MVE_LD_UNALIGNED_RETIRED

#define ARM_PMU_MVE_LD_UNALIGNED_RETIRED 0x0290

MVE unaligned load instruction architecturally executed.

## ◆ ARM_PMU_MVE_LD_UNALIGNED_SPEC

#define ARM_PMU_MVE_LD_UNALIGNED_SPEC 0x0291

MVE unaligned load instruction speculatively executed.

## ◆ ARM_PMU_MVE_LDST_CONTIG_RETIRED

#define ARM_PMU_MVE_LDST_CONTIG_RETIRED 0x0244

MVE contiguous load or store instruction architecturally executed.

## ◆ ARM_PMU_MVE_LDST_CONTIG_SPEC

#define ARM_PMU_MVE_LDST_CONTIG_SPEC 0x0245

MVE contiguous load or store instruction speculatively executed.

## ◆ ARM_PMU_MVE_LDST_MULTI_RETIRED

#define ARM_PMU_MVE_LDST_MULTI_RETIRED 0x025C

MVE memory instruction targeting multiple registers architecturally executed.

## ◆ ARM_PMU_MVE_LDST_MULTI_SPEC

#define ARM_PMU_MVE_LDST_MULTI_SPEC 0x025D

MVE memory instruction targeting multiple registers speculatively executed.

## ◆ ARM_PMU_MVE_LDST_NONCONTIG_RETIRED

#define ARM_PMU_MVE_LDST_NONCONTIG_RETIRED 0x0250

MVE non-contiguous load or store instruction architecturally executed.

## ◆ ARM_PMU_MVE_LDST_NONCONTIG_SPEC

#define ARM_PMU_MVE_LDST_NONCONTIG_SPEC 0x0251

MVE non-contiguous load or store instruction speculatively executed.

## ◆ ARM_PMU_MVE_LDST_RETIRED

#define ARM_PMU_MVE_LDST_RETIRED 0x0238

MVE load or store instruction architecturally executed.

## ◆ ARM_PMU_MVE_LDST_SPEC

#define ARM_PMU_MVE_LDST_SPEC 0x0239

MVE load or store instruction speculatively executed.

## ◆ ARM_PMU_MVE_LDST_UNALIGNED_NONCONTIG_RETIRED

#define ARM_PMU_MVE_LDST_UNALIGNED_NONCONTIG_RETIRED 0x0298

MVE unaligned noncontiguous load or store instruction architecturally executed.

## ◆ ARM_PMU_MVE_LDST_UNALIGNED_NONCONTIG_SPEC

#define ARM_PMU_MVE_LDST_UNALIGNED_NONCONTIG_SPEC 0x0299

MVE unaligned noncontiguous load or store instruction speculatively executed.

## ◆ ARM_PMU_MVE_LDST_UNALIGNED_RETIRED

#define ARM_PMU_MVE_LDST_UNALIGNED_RETIRED 0x028C

MVE unaligned memory load or store instruction architecturally executed.

## ◆ ARM_PMU_MVE_LDST_UNALIGNED_SPEC

#define ARM_PMU_MVE_LDST_UNALIGNED_SPEC 0x028D

MVE unaligned memory load or store instruction speculatively executed.

## ◆ ARM_PMU_MVE_PRED

#define ARM_PMU_MVE_PRED 0x02B8

Cycles where one or more predicated beats architecturally executed.

## ◆ ARM_PMU_MVE_ST_CONTIG_RETIRED

#define ARM_PMU_MVE_ST_CONTIG_RETIRED 0x024C

MVE contiguous store instruction architecturally executed.

## ◆ ARM_PMU_MVE_ST_CONTIG_SPEC

#define ARM_PMU_MVE_ST_CONTIG_SPEC 0x024D

MVE contiguous store instruction speculatively executed.

## ◆ ARM_PMU_MVE_ST_MULTI_RETIRED

#define ARM_PMU_MVE_ST_MULTI_RETIRED 0x0261

MVE memory store instruction targeting multiple registers architecturally executed.

## ◆ ARM_PMU_MVE_ST_MULTI_SPEC

#define ARM_PMU_MVE_ST_MULTI_SPEC 0x0265

MVE memory store instruction targeting multiple registers speculatively executed.

## ◆ ARM_PMU_MVE_ST_NONCONTIG_RETIRED

#define ARM_PMU_MVE_ST_NONCONTIG_RETIRED 0x0258

MVE non-contiguous store instruction architecturally executed.

## ◆ ARM_PMU_MVE_ST_NONCONTIG_SPEC

#define ARM_PMU_MVE_ST_NONCONTIG_SPEC 0x0259

MVE non-contiguous store instruction speculatively executed.

## ◆ ARM_PMU_MVE_ST_RETIRED

#define ARM_PMU_MVE_ST_RETIRED 0x0240

MVE store instruction architecturally executed.

## ◆ ARM_PMU_MVE_ST_SPEC

#define ARM_PMU_MVE_ST_SPEC 0x0241

MVE store instruction speculatively executed.

## ◆ ARM_PMU_MVE_ST_UNALIGNED_RETIRED

#define ARM_PMU_MVE_ST_UNALIGNED_RETIRED 0x0294

MVE unaligned store instruction architecturally executed.

## ◆ ARM_PMU_MVE_ST_UNALIGNED_SPEC

#define ARM_PMU_MVE_ST_UNALIGNED_SPEC 0x0295

MVE unaligned store instruction speculatively executed.

## ◆ ARM_PMU_MVE_STALL

#define ARM_PMU_MVE_STALL 0x02CC

Stall cycles caused by an MVE instruction.

## ◆ ARM_PMU_MVE_STALL_BREAK

#define ARM_PMU_MVE_STALL_BREAK 0x02D3

Stall cycles caused by an MVE chain break.

## ◆ ARM_PMU_MVE_STALL_DEPENDENCY

#define ARM_PMU_MVE_STALL_DEPENDENCY 0x02D4

Stall cycles caused by MVE register dependency.

## ◆ ARM_PMU_MVE_STALL_RESOURCE

#define ARM_PMU_MVE_STALL_RESOURCE 0x02CD

Stall cycles caused by an MVE instruction because of resource conflicts.

## ◆ ARM_PMU_MVE_STALL_RESOURCE_FP

#define ARM_PMU_MVE_STALL_RESOURCE_FP 0x02CF

Stall cycles caused by an MVE instruction because of floating-point resource conflicts.

## ◆ ARM_PMU_MVE_STALL_RESOURCE_INT

#define ARM_PMU_MVE_STALL_RESOURCE_INT 0x02D0

Stall cycles caused by an MVE instruction because of integer resource conflicts.

## ◆ ARM_PMU_MVE_STALL_RESOURCE_MEM

#define ARM_PMU_MVE_STALL_RESOURCE_MEM 0x02CE

Stall cycles caused by an MVE instruction because of memory resource conflicts.

## ◆ ARM_PMU_MVE_VREDUCE_FP_RETIRED

#define ARM_PMU_MVE_VREDUCE_FP_RETIRED 0x02A4

MVE floating-point vector reduction instruction architecturally executed.

## ◆ ARM_PMU_MVE_VREDUCE_FP_SPEC

#define ARM_PMU_MVE_VREDUCE_FP_SPEC 0x02A5

MVE floating-point vector reduction instruction speculatively executed.

## ◆ ARM_PMU_MVE_VREDUCE_INT_RETIRED

#define ARM_PMU_MVE_VREDUCE_INT_RETIRED 0x02A8

MVE integer vector reduction instruction architecturally executed.

## ◆ ARM_PMU_MVE_VREDUCE_INT_SPEC

#define ARM_PMU_MVE_VREDUCE_INT_SPEC 0x02A9

MVE integer vector reduction instruction speculatively executed.

## ◆ ARM_PMU_MVE_VREDUCE_RETIRED

#define ARM_PMU_MVE_VREDUCE_RETIRED 0x02A0

MVE vector reduction instruction architecturally executed.

## ◆ ARM_PMU_MVE_VREDUCE_SPEC

#define ARM_PMU_MVE_VREDUCE_SPEC 0x02A1

MVE vector reduction instruction speculatively executed.

## ◆ ARM_PMU_OP_COMPLETE

#define ARM_PMU_OP_COMPLETE 0x003A

Operation retired.

## ◆ ARM_PMU_OP_SPEC

#define ARM_PMU_OP_SPEC 0x003B

Operation speculatively executed.

## ◆ ARM_PMU_PC_WRITE_RETIRED

#define ARM_PMU_PC_WRITE_RETIRED 0x000C

Software change to the Program Counter (PC). Instruction is architecturally executed and condition code check pass.

## ◆ ARM_PMU_SE_CALL_NS

#define ARM_PMU_SE_CALL_NS 0x0115

Call to non-secure function, resulting in Security state change.

## ◆ ARM_PMU_SE_CALL_S

#define ARM_PMU_SE_CALL_S 0x0114

Call to secure function, resulting in Security state change.

## ◆ ARM_PMU_ST_RETIRED

#define ARM_PMU_ST_RETIRED 0x0007

Memory-writing instruction architecturally executed and condition code check pass.

## ◆ ARM_PMU_STALL

#define ARM_PMU_STALL 0x003C

Stall cycle for instruction or operation not sent for execution.

## ◆ ARM_PMU_STALL_BACKEND

#define ARM_PMU_STALL_BACKEND 0x0024

No operation issued because of the backend.

## ◆ ARM_PMU_STALL_FRONTEND

#define ARM_PMU_STALL_FRONTEND 0x0023

No operation issued because of the frontend.

## ◆ ARM_PMU_STALL_OP

#define ARM_PMU_STALL_OP 0x003F

Instruction or operation slots not occupied each cycle.

## ◆ ARM_PMU_STALL_OP_BACKEND

#define ARM_PMU_STALL_OP_BACKEND 0x003D

Stall cycle for instruction or operation not sent for execution due to pipeline backend.

## ◆ ARM_PMU_STALL_OP_FRONTEND

#define ARM_PMU_STALL_OP_FRONTEND 0x003E

Stall cycle for instruction or operation not sent for execution due to pipeline frontend.

## ◆ ARM_PMU_SW_INCR

#define ARM_PMU_SW_INCR 0x0000

Software update to the PMU_SWINC register, architecturally executed and condition code check pass.

## ◆ ARM_PMU_TRCEXTOUT0

#define ARM_PMU_TRCEXTOUT0 0x4010

ETM external output 0.

## ◆ ARM_PMU_TRCEXTOUT1

#define ARM_PMU_TRCEXTOUT1 0x4011

ETM external output 1.

## ◆ ARM_PMU_TRCEXTOUT2

#define ARM_PMU_TRCEXTOUT2 0x4012

ETM external output 2.

## ◆ ARM_PMU_TRCEXTOUT3

#define ARM_PMU_TRCEXTOUT3 0x4013

ETM external output 3.

## ◆ ARM_PMU_UNALIGNED_LDST_RETIRED

#define ARM_PMU_UNALIGNED_LDST_RETIRED 0x000F

Unaligned memory memory-reading or memory-writing instruction architecturally executed and condition code check pass.