| CMSIS-Driver Peripheral Interface for Middleware and Application Code |

Loading...
Searching...
No Matches
Macros
I2C Address Flags
I2C Interface

Specify address flags. More...

## Macros
#define | ARM_I2C_ADDRESS_10BIT (0x0400UL)
| 10-bit address flag
#define | ARM_I2C_ADDRESS_GC (0x8000UL)
| General Call flag.

## Description

Specify address flags.

Specifies the address type for the functions ARM_I2C_MasterReceive, ARM_I2C_MasterTransmit and ARM_I2C_OWN_ADDRESS.

## Macro Definition Documentation

## ◆ ARM_I2C_ADDRESS_10BIT

#define ARM_I2C_ADDRESS_10BIT (0x0400UL)

10-bit address flag

See also
  ARM_I2C_OWN_ADDRESS
  ARM_I2C_MasterTransmit
  ARM_I2C_MasterReceive

## ◆ ARM_I2C_ADDRESS_GC

#define ARM_I2C_ADDRESS_GC (0x8000UL)

General Call flag.

See also
  ARM_I2C_OWN_ADDRESS