| CMSIS-Driver Peripheral Interface for Middleware and Application Code |

Loading...
Searching...
No Matches
Macros
USB Endpoint Type
USB Interface

USB Endpoint Type definitions. More...

## Macros
#define | ARM_USB_ENDPOINT_CONTROL (0U)
| Control Endpoint.
#define | ARM_USB_ENDPOINT_ISOCHRONOUS (1U)
| Isochronous Endpoint.
#define | ARM_USB_ENDPOINT_BULK (2U)
| Bulk Endpoint.
#define | ARM_USB_ENDPOINT_INTERRUPT (3U)
| Interrupt Endpoint.

## Description

USB Endpoint Type definitions.

The following USB Endpoint Type values are defined:

## Macro Definition Documentation

## ◆ ARM_USB_ENDPOINT_CONTROL

#define ARM_USB_ENDPOINT_CONTROL (0U)

Control Endpoint.

## ◆ ARM_USB_ENDPOINT_ISOCHRONOUS

#define ARM_USB_ENDPOINT_ISOCHRONOUS (1U)

Isochronous Endpoint.

## ◆ ARM_USB_ENDPOINT_BULK

#define ARM_USB_ENDPOINT_BULK (2U)

Bulk Endpoint.

## ◆ ARM_USB_ENDPOINT_INTERRUPT

#define ARM_USB_ENDPOINT_INTERRUPT (3U)

Interrupt Endpoint.