| CMSIS-Driver Peripheral Interface for Middleware and Application Code |

Loading...
Searching...
No Matches
Functions
Driver_NAND.c File Reference

## Functions
ARM_DRIVER_VERSION | ARM_NAND_GetVersion (void)
| Get driver version.
ARM_NAND_CAPABILITIES | ARM_NAND_GetCapabilities (void)
| Get driver capabilities.
int32_t | ARM_NAND_Initialize (ARM_NAND_SignalEvent_t cb_event)
| Initialize the NAND Interface.
int32_t | ARM_NAND_Uninitialize (void)
| De-initialize the NAND Interface.
int32_t | ARM_NAND_PowerControl (ARM_POWER_STATE state)
| Control the NAND interface power.
int32_t | ARM_NAND_DevicePower (uint32_t voltage)
| Set device power supply voltage.
int32_t | ARM_NAND_WriteProtect (uint32_t dev_num, bool enable)
| Control WPn (Write Protect).
int32_t | ARM_NAND_ChipEnable (uint32_t dev_num, bool enable)
| Control CEn (Chip Enable).
int32_t | ARM_NAND_GetDeviceBusy (uint32_t dev_num)
| Get Device Busy pin state.
int32_t | ARM_NAND_SendCommand (uint32_t dev_num, uint8_t cmd)
| Send command to NAND device.
int32_t | ARM_NAND_SendAddress (uint32_t dev_num, uint8_t addr)
| Send address to NAND device.
int32_t | ARM_NAND_ReadData (uint32_t dev_num, void *data, uint32_t cnt, uint32_t mode)
| Read data from NAND device.
int32_t | ARM_NAND_WriteData (uint32_t dev_num, const void *data, uint32_t cnt, uint32_t mode)
| Write data to NAND device.
int32_t | ARM_NAND_ExecuteSequence (uint32_t dev_num, uint32_t code, uint32_t cmd, uint32_t addr_col, uint32_t addr_row, void *data, uint32_t data_cnt, uint8_t *status, uint32_t *count)
| Execute sequence of operations.
int32_t | ARM_NAND_AbortSequence (uint32_t dev_num)
| Abort sequence execution.
int32_t | ARM_NAND_Control (uint32_t dev_num, uint32_t control, uint32_t arg)
| Control NAND Interface.
ARM_NAND_STATUS | ARM_NAND_GetStatus (uint32_t dev_num)
| Get NAND status.
int32_t | ARM_NAND_InquireECC (int32_t index, ARM_NAND_ECC_INFO *info)
| Inquire about available ECC.
void | ARM_NAND_SignalEvent (uint32_t dev_num, uint32_t event)
| Signal NAND event.