| CMSIS-Core (Cortex-A) CMSIS-Core support for Cortex-A processor-based devices |

Loading...
Searching...
No Matches
Content | Functions
Configuration Base Address Register (CBAR)
Core Register Access

Takes the physical base address value of the memory-mapped SCU peripherals at reset from the external signal PERIPHBASE[31:13]. More...

## Content
| CBAR Bits
| Bit position and mask macros.

## Functions
__STATIC_FORCEINLINE uint32_t | __get_CBAR (void)
| Get CBAR.

## Description

Takes the physical base address value of the memory-mapped SCU peripherals at reset from the external signal PERIPHBASE[31:13].

Bits | Name | Function
--- | --- | ---
[31:13] | PERIPHBASE | Peripheral base address.
[12:0] | - | Read as zero.

Consider __get_CBAR to access this register.

## Function Documentation

## ◆ __get_CBAR()

__STATIC_INLINE uint32_t __get_CBAR | ( | void |  | ) |

Get CBAR.

Returns
  Configuration Base Address register value

This function returns the value of the Configuration Base Address register.