| CMSIS-Driver Peripheral Interface for Middleware and Application Code |

Loading...
Searching...
No Matches

### - g -

- general_call : ARM_I2C_STATUS
- GetBlock : ARM_DRIVER_STORAGE
- GetCapabilities : ARM_DRIVER_CAN, ARM_DRIVER_ETH_MAC, ARM_DRIVER_FLASH, ARM_DRIVER_I2C, ARM_DRIVER_MCI, ARM_DRIVER_NAND, ARM_DRIVER_SAI, ARM_DRIVER_SPI, ARM_DRIVER_STORAGE, ARM_DRIVER_USART, ARM_DRIVER_USBD, ARM_DRIVER_USBH, ARM_DRIVER_USBH_HCI, ARM_DRIVER_WIFI
- GetClock : ARM_DRIVER_CAN
- GetDataCount : ARM_DRIVER_I2C, ARM_DRIVER_SPI
- GetDeviceBusy : ARM_DRIVER_NAND
- GetFrameNumber : ARM_DRIVER_USBD, ARM_DRIVER_USBH
- GetInfo : ARM_DRIVER_FLASH, ARM_DRIVER_STORAGE
- GetInput : ARM_DRIVER_GPIO
- GetLinkInfo : ARM_DRIVER_ETH_PHY
- GetLinkState : ARM_DRIVER_ETH_PHY
- GetMacAddress : ARM_DRIVER_ETH_MAC
- GetModemStatus : ARM_DRIVER_USART
- GetModuleInfo : ARM_DRIVER_WIFI
- GetNetInfo : ARM_DRIVER_WIFI
- GetNextBlock : ARM_DRIVER_STORAGE
- GetOption : ARM_DRIVER_WIFI
- GetRxCount : ARM_DRIVER_SAI, ARM_DRIVER_USART
- GetRxFrameSize : ARM_DRIVER_ETH_MAC
- GetRxFrameTime : ARM_DRIVER_ETH_MAC
- GetStatus : ARM_DRIVER_CAN, ARM_DRIVER_FLASH, ARM_DRIVER_I2C, ARM_DRIVER_MCI, ARM_DRIVER_NAND, ARM_DRIVER_SAI, ARM_DRIVER_SPI, ARM_DRIVER_STORAGE, ARM_DRIVER_USART
- GetTxCount : ARM_DRIVER_SAI, ARM_DRIVER_USART
- GetTxFrameTime : ARM_DRIVER_ETH_MAC
- GetVersion : ARM_DRIVER_CAN, ARM_DRIVER_ETH_MAC, ARM_DRIVER_ETH_PHY, ARM_DRIVER_FLASH, ARM_DRIVER_I2C, ARM_DRIVER_MCI, ARM_DRIVER_NAND, ARM_DRIVER_SAI, ARM_DRIVER_SPI, ARM_DRIVER_STORAGE, ARM_DRIVER_USART, ARM_DRIVER_USBD, ARM_DRIVER_USBH, ARM_DRIVER_USBH_HCI, ARM_DRIVER_WIFI