| CMSIS-Driver Peripheral Interface for Middleware and Application Code |

Loading...
Searching...
No Matches
Macros
Flash Events
Flash Interface

The Flash driver generates call back events that are notified via the function ARM_Flash_SignalEvent. More...

## Macros
#define | ARM_FLASH_EVENT_READY (1UL << 0)
| Flash Ready.
#define | ARM_FLASH_EVENT_ERROR (1UL << 1)
| Read/Program/Erase Error.

## Description

The Flash driver generates call back events that are notified via the function ARM_Flash_SignalEvent.

This section provides the event values for the ARM_Flash_SignalEvent callback function.

The following call back notification events are generated:

## Macro Definition Documentation

## ◆ ARM_FLASH_EVENT_READY

#define ARM_FLASH_EVENT_READY (1UL << 0)

Flash Ready.

## ◆ ARM_FLASH_EVENT_ERROR

#define ARM_FLASH_EVENT_ERROR (1UL << 1)

Read/Program/Erase Error.