CMSIS-Driver: USART Control Codes

| CMSIS-Driver Version 2.05 Peripheral Interface for Middleware and Application Code

- Main Page
- Usage and Description
- Reference

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Content
USART Control Codes
USART Interface

Many parameters of the USART driver are configured using the ARM_USART_Control function. More...

## Content
| USART Mode Control
| Specify USART mode.
| USART Miscellaneous Control
| Specifies additional miscellaneous controls.
| USART Data Bits
| Defines the number of data bits.
| USART Parity Bit
| Defines the parity bit.
| USART Stop Bits
| Defines the number of stop bits.
| USART Flow Control
| Specifies RTS/CTS flow control.
| USART Clock Polarity
| Defines the clock polarity for the synchronous mode.
| USART Clock Phase
| Defines the clock phase for the synchronous mode.

## Description

Many parameters of the USART driver are configured using the ARM_USART_Control function.

The various USART control codes define:

- USART Mode Control specifies USART mode
- USART Data Bits defines the number of data bits
- USART Parity Bit defines the parity bit
- USART Stop Bits defines the number of stop bits
- USART Flow Control specifies RTS/CTS flow control
- USART Clock Polarity defines the clock polarity for the synchronous mode
- USART Clock Phase defines the clock phase for the synchronous mode
- USART Miscellaneous Control specifies additional miscellaneous controls

Refer to the ARM_USART_Control function for further details.