CMSIS-DAP: General Commands

| CMSIS-DAP Version 1.2.0 (Proposal) Interface Firmware for CoreSight Debug Access Port

- Main Page
- Usage and Description
- Reference

All Functions Groups Pages
Content
General Commands
CMSIS-DAP Commands

Information and Control commands for the CMSIS-DAP Debug Unit. More...

## Content
| DAP_Info
| Get Information about CMSIS-DAP Debug Unit.
| DAP_HostStatus
| Sent status information of the debugger to Debug Unit.
| DAP_Connect
| Connect to Device and selected DAP mode.
| DAP_Disconnect
| Disconnect from active Debug Port.
| DAP_WriteABORT
| Write ABORT Register.
| DAP_Delay
| Wait for specified delay.
| DAP_ResetTarget
| Reset Target with Device specific sequence.

## Description

Information and Control commands for the CMSIS-DAP Debug Unit.

The General Commands allow to:

- Connect, disconnect, and identify the Debug Unit.
- Control the Status LEDs of the Debug Unit.
- Issue and hardware reset to the connected Device.
- Terminate previous CMSIS-DAP Commands.
- Wait for a specified time.