CMSIS-Driver: Globals

| CMSIS-Driver Version 2.05 Peripheral Interface for Middleware and Application Code

- Main Page
- Usage and Description
- Reference

- All
- Functions
- Typedefs
- Enumerations
- Enumerator
- Macros

- _
- c
- d
- e
- f
- i
- m
- n
- r
- s
- u

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages

### - s -

- ARM_SAI_ABORT_RECEIVE : Driver_SAI.h
- ARM_SAI_ABORT_SEND : Driver_SAI.h
- ARM_SAI_API_VERSION : Driver_SAI.h
- ARM_SAI_ASYNCHRONOUS : Driver_SAI.h
- ARM_SAI_AUDIO_FREQ_Msk : Driver_SAI.h
- ARM_SAI_BIT_ORDER_Msk : Driver_SAI.h
- ARM_SAI_BIT_ORDER_Pos : Driver_SAI.h
- ARM_SAI_CLOCK_POLARITY_0 : Driver_SAI.h
- ARM_SAI_CLOCK_POLARITY_1 : Driver_SAI.h
- ARM_SAI_CLOCK_POLARITY_Msk : Driver_SAI.h
- ARM_SAI_CLOCK_POLARITY_Pos : Driver_SAI.h
- ARM_SAI_COMPANDING_A_LAW : Driver_SAI.h
- ARM_SAI_COMPANDING_Msk : Driver_SAI.h
- ARM_SAI_COMPANDING_NONE : Driver_SAI.h
- ARM_SAI_COMPANDING_Pos : Driver_SAI.h
- ARM_SAI_COMPANDING_U_LAW : Driver_SAI.h
- ARM_SAI_CONFIGURE_RX : Driver_SAI.h
- ARM_SAI_CONFIGURE_TX : Driver_SAI.h
- ARM_SAI_CONTROL_Msk : Driver_SAI.h
- ARM_SAI_CONTROL_RX : Driver_SAI.h
- ARM_SAI_CONTROL_TX : Driver_SAI.h
- ARM_SAI_DATA_SIZE : Driver_SAI.h
- ARM_SAI_DATA_SIZE_Msk : Driver_SAI.h
- ARM_SAI_DATA_SIZE_Pos : Driver_SAI.h
- ARM_SAI_ERROR_AUDIO_FREQ : Driver_SAI.h
- ARM_SAI_ERROR_BIT_ORDER : Driver_SAI.h
- ARM_SAI_ERROR_CLOCK_POLARITY : Driver_SAI.h
- ARM_SAI_ERROR_COMPANDING : Driver_SAI.h
- ARM_SAI_ERROR_DATA_SIZE : Driver_SAI.h
- ARM_SAI_ERROR_FRAME_LENGHT : Driver_SAI.h
- ARM_SAI_ERROR_FRAME_SYNC_EARLY : Driver_SAI.h
- ARM_SAI_ERROR_FRAME_SYNC_POLARITY : Driver_SAI.h
- ARM_SAI_ERROR_FRAME_SYNC_WIDTH : Driver_SAI.h
- ARM_SAI_ERROR_MCLK_PIN : Driver_SAI.h
- ARM_SAI_ERROR_MCLK_PRESCALER : Driver_SAI.h
- ARM_SAI_ERROR_MONO_MODE : Driver_SAI.h
- ARM_SAI_ERROR_PROTOCOL : Driver_SAI.h
- ARM_SAI_ERROR_SLOT_COUNT : Driver_SAI.h
- ARM_SAI_ERROR_SLOT_OFFESET : Driver_SAI.h
- ARM_SAI_ERROR_SLOT_SIZE : Driver_SAI.h
- ARM_SAI_ERROR_SYNCHRONIZATION : Driver_SAI.h
- ARM_SAI_EVENT_FRAME_ERROR : Driver_SAI.h
- ARM_SAI_EVENT_RECEIVE_COMPLETE : Driver_SAI.h
- ARM_SAI_EVENT_RX_OVERFLOW : Driver_SAI.h
- ARM_SAI_EVENT_SEND_COMPLETE : Driver_SAI.h
- ARM_SAI_EVENT_TX_UNDERFLOW : Driver_SAI.h
- ARM_SAI_FRAME_LENGTH : Driver_SAI.h
- ARM_SAI_FRAME_LENGTH_Msk : Driver_SAI.h
- ARM_SAI_FRAME_LENGTH_Pos : Driver_SAI.h
- ARM_SAI_FRAME_SYNC_EARLY : Driver_SAI.h
- ARM_SAI_FRAME_SYNC_POLARITY_HIGH : Driver_SAI.h
- ARM_SAI_FRAME_SYNC_POLARITY_LOW : Driver_SAI.h
- ARM_SAI_FRAME_SYNC_POLARITY_Msk : Driver_SAI.h
- ARM_SAI_FRAME_SYNC_POLARITY_Pos : Driver_SAI.h
- ARM_SAI_FRAME_SYNC_WIDTH : Driver_SAI.h
- ARM_SAI_FRAME_SYNC_WIDTH_Msk : Driver_SAI.h
- ARM_SAI_FRAME_SYNC_WIDTH_Pos : Driver_SAI.h
- ARM_SAI_LSB_FIRST : Driver_SAI.h
- ARM_SAI_MASK_SLOTS_RX : Driver_SAI.h
- ARM_SAI_MASK_SLOTS_TX : Driver_SAI.h
- ARM_SAI_MCLK_PIN_INACTIVE : Driver_SAI.h
- ARM_SAI_MCLK_PIN_INPUT : Driver_SAI.h
- ARM_SAI_MCLK_PIN_Msk : Driver_SAI.h
- ARM_SAI_MCLK_PIN_OUTPUT : Driver_SAI.h
- ARM_SAI_MCLK_PIN_Pos : Driver_SAI.h
- ARM_SAI_MCLK_PRESCALER : Driver_SAI.h
- ARM_SAI_MCLK_PRESCALER_Msk : Driver_SAI.h
- ARM_SAI_MCLK_PRESCALER_Pos : Driver_SAI.h
- ARM_SAI_MODE_MASTER : Driver_SAI.h
- ARM_SAI_MODE_Msk : Driver_SAI.h
- ARM_SAI_MODE_Pos : Driver_SAI.h
- ARM_SAI_MODE_SLAVE : Driver_SAI.h
- ARM_SAI_MONO_MODE : Driver_SAI.h
- ARM_SAI_MSB_FIRST : Driver_SAI.h
- ARM_SAI_PROTOCOL_AC97 : Driver_SAI.h
- ARM_SAI_PROTOCOL_I2S : Driver_SAI.h
- ARM_SAI_PROTOCOL_LSB_JUSTIFIED : Driver_SAI.h
- ARM_SAI_PROTOCOL_MSB_JUSTIFIED : Driver_SAI.h
- ARM_SAI_PROTOCOL_Msk : Driver_SAI.h
- ARM_SAI_PROTOCOL_PCM_LONG : Driver_SAI.h
- ARM_SAI_PROTOCOL_PCM_SHORT : Driver_SAI.h
- ARM_SAI_PROTOCOL_Pos : Driver_SAI.h
- ARM_SAI_PROTOCOL_USER : Driver_SAI.h
- ARM_SAI_SLOT_COUNT : Driver_SAI.h
- ARM_SAI_SLOT_COUNT_Msk : Driver_SAI.h
- ARM_SAI_SLOT_COUNT_Pos : Driver_SAI.h
- ARM_SAI_SLOT_OFFSET : Driver_SAI.h
- ARM_SAI_SLOT_OFFSET_Msk : Driver_SAI.h
- ARM_SAI_SLOT_OFFSET_Pos : Driver_SAI.h
- ARM_SAI_SLOT_SIZE_16 : Driver_SAI.h
- ARM_SAI_SLOT_SIZE_32 : Driver_SAI.h
- ARM_SAI_SLOT_SIZE_DEFAULT : Driver_SAI.h
- ARM_SAI_SLOT_SIZE_Msk : Driver_SAI.h
- ARM_SAI_SLOT_SIZE_Pos : Driver_SAI.h
- ARM_SAI_SYNCHRONIZATION_Msk : Driver_SAI.h
- ARM_SAI_SYNCHRONIZATION_Pos : Driver_SAI.h
- ARM_SAI_SYNCHRONOUS : Driver_SAI.h
- ARM_SPI_ABORT_TRANSFER : Driver_SPI.h
- ARM_SPI_API_VERSION : Driver_SPI.h
- ARM_SPI_BIT_ORDER_Msk : Driver_SPI.h
- ARM_SPI_BIT_ORDER_Pos : Driver_SPI.h
- ARM_SPI_CONTROL_Msk : Driver_SPI.h
- ARM_SPI_CONTROL_Pos : Driver_SPI.h
- ARM_SPI_CONTROL_SS : Driver_SPI.h
- ARM_SPI_CPOL0_CPHA0 : Driver_SPI.h
- ARM_SPI_CPOL0_CPHA1 : Driver_SPI.h
- ARM_SPI_CPOL1_CPHA0 : Driver_SPI.h
- ARM_SPI_CPOL1_CPHA1 : Driver_SPI.h
- ARM_SPI_DATA_BITS : Driver_SPI.h
- ARM_SPI_DATA_BITS_Msk : Driver_SPI.h
- ARM_SPI_DATA_BITS_Pos : Driver_SPI.h
- ARM_SPI_ERROR_BIT_ORDER : Driver_SPI.h
- ARM_SPI_ERROR_DATA_BITS : Driver_SPI.h
- ARM_SPI_ERROR_FRAME_FORMAT : Driver_SPI.h
- ARM_SPI_ERROR_MODE : Driver_SPI.h
- ARM_SPI_ERROR_SS_MODE : Driver_SPI.h
- ARM_SPI_EVENT_DATA_LOST : Driver_SPI.h
- ARM_SPI_EVENT_MODE_FAULT : Driver_SPI.h
- ARM_SPI_EVENT_TRANSFER_COMPLETE : Driver_SPI.h
- ARM_SPI_FRAME_FORMAT_Msk : Driver_SPI.h
- ARM_SPI_FRAME_FORMAT_Pos : Driver_SPI.h
- ARM_SPI_GET_BUS_SPEED : Driver_SPI.h
- ARM_SPI_LSB_MSB : Driver_SPI.h
- ARM_SPI_MICROWIRE : Driver_SPI.h
- ARM_SPI_MODE_INACTIVE : Driver_SPI.h
- ARM_SPI_MODE_MASTER : Driver_SPI.h
- ARM_SPI_MODE_MASTER_SIMPLEX : Driver_SPI.h
- ARM_SPI_MODE_SLAVE : Driver_SPI.h
- ARM_SPI_MODE_SLAVE_SIMPLEX : Driver_SPI.h
- ARM_SPI_MSB_LSB : Driver_SPI.h
- ARM_SPI_SET_BUS_SPEED : Driver_SPI.h
- ARM_SPI_SET_DEFAULT_TX_VALUE : Driver_SPI.h
- ARM_SPI_SS_ACTIVE : Driver_SPI.h
- ARM_SPI_SS_INACTIVE : Driver_SPI.h
- ARM_SPI_SS_MASTER_HW_INPUT : Driver_SPI.h
- ARM_SPI_SS_MASTER_HW_OUTPUT : Driver_SPI.h
- ARM_SPI_SS_MASTER_MODE_Msk : Driver_SPI.h
- ARM_SPI_SS_MASTER_MODE_Pos : Driver_SPI.h
- ARM_SPI_SS_MASTER_SW : Driver_SPI.h
- ARM_SPI_SS_MASTER_UNUSED : Driver_SPI.h
- ARM_SPI_SS_SLAVE_HW : Driver_SPI.h
- ARM_SPI_SS_SLAVE_MODE_Msk : Driver_SPI.h
- ARM_SPI_SS_SLAVE_MODE_Pos : Driver_SPI.h
- ARM_SPI_SS_SLAVE_SW : Driver_SPI.h
- ARM_SPI_TI_SSI : Driver_SPI.h
- ARM_STORAGE_API_VERSION : Driver_Storage.h
- ARM_STORAGE_ERROR_NOT_ERASABLE : Driver_Storage.h
- ARM_STORAGE_ERROR_NOT_PROGRAMMABLE : Driver_Storage.h
- ARM_STORAGE_ERROR_PROTECTED : Driver_Storage.h
- ARM_STORAGE_INVALID_ADDRESS : Driver_Storage.h
- ARM_STORAGE_INVALID_OFFSET : Driver_Storage.h
- ARM_STORAGE_PROGRAM_CYCLES_INFINITE : Driver_Storage.h
- ARM_STORAGE_PROGRAMMABILITY_ERASABLE : Driver_Storage.h
- ARM_STORAGE_PROGRAMMABILITY_RAM : Driver_Storage.h
- ARM_STORAGE_PROGRAMMABILITY_ROM : Driver_Storage.h
- ARM_STORAGE_PROGRAMMABILITY_WORM : Driver_Storage.h
- ARM_STORAGE_VALID_BLOCK : Driver_Storage.h