CMSIS-Driver: Driver_USBH.c File Reference

| CMSIS-Driver Version 2.05 Peripheral Interface for Middleware and Application Code

- Main Page
- Usage and Description
- Reference

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Functions
Driver_USBH.c File Reference

## Functions
ARM_DRIVER_VERSION | ARM_USBH_GetVersion (void)
| Get driver version. More...
ARM_USBH_CAPABILITIES | ARM_USBH_GetCapabilities (void)
| Get driver capabilities. More...
int32_t | ARM_USBH_Initialize (ARM_USBH_SignalPortEvent_t cb_port_event, ARM_USBH_SignalPipeEvent_t cb_pipe_event)
| Initialize USB Host Interface. More...
int32_t | ARM_USBH_Uninitialize (void)
| De-initialize USB Host Interface. More...
int32_t | ARM_USBH_PowerControl (ARM_POWER_STATE state)
| Control USB Host Interface Power. More...
int32_t | ARM_USBH_PortVbusOnOff (uint8_t port, bool vbus)
| Root HUB Port VBUS on/off. More...
int32_t | ARM_USBH_PortReset (uint8_t port)
| Do Root HUB Port Reset. More...
int32_t | ARM_USBH_PortSuspend (uint8_t port)
| Suspend Root HUB Port (stop generating SOFs). More...
int32_t | ARM_USBH_PortResume (uint8_t port)
| Resume Root HUB Port (start generating SOFs). More...
ARM_USBH_PORT_STATE | ARM_USBH_PortGetState (uint8_t port)
| Get current Root HUB Port State. More...
ARM_USBH_PIPE_HANDLE | ARM_USBH_PipeCreate (uint8_t dev_addr, uint8_t dev_speed, uint8_t hub_addr, uint8_t hub_port, uint8_t ep_addr, uint8_t ep_type, uint16_t ep_max_packet_size, uint8_t ep_interval)
| Create Pipe in System. More...
int32_t | ARM_USBH_PipeModify (ARM_USBH_PIPE_HANDLE pipe_hndl, uint8_t dev_addr, uint8_t dev_speed, uint8_t hub_addr, uint8_t hub_port, uint16_t ep_max_packet_size)
| Modify Pipe in System. More...
int32_t | ARM_USBH_PipeDelete (ARM_USBH_PIPE_HANDLE pipe_hndl)
| Delete Pipe from System. More...
int32_t | ARM_USBH_PipeReset (ARM_USBH_PIPE_HANDLE pipe_hndl)
| Reset Pipe. More...
int32_t | ARM_USBH_PipeTransfer (ARM_USBH_PIPE_HANDLE pipe_hndl, uint32_t packet, uint8_t *data, uint32_t num)
| Transfer packets through USB Pipe. More...
uint32_t | ARM_USBH_PipeTransferGetResult (ARM_USBH_PIPE_HANDLE pipe_hndl)
| Get result of USB Pipe transfer. More...
int32_t | ARM_USBH_PipeTransferAbort (ARM_USBH_PIPE_HANDLE pipe_hndl)
| Abort current USB Pipe transfer. More...
uint16_t | ARM_USBH_GetFrameNumber (void)
| Get current USB Frame Number. More...
void | ARM_USBH_SignalPortEvent (uint8_t port, uint32_t event)
| Signal Root HUB Port Event. More...
void | ARM_USBH_SignalPipeEvent (ARM_USBH_PIPE_HANDLE pipe_hndl, uint32_t event)
| Signal Pipe Event. More...
ARM_DRIVER_VERSION | ARM_USBH_HCI_GetVersion (void)
| Get USB Host HCI (OHCI/EHCI) driver version. More...
ARM_USBH_HCI_CAPABILITIES | ARM_USBH_HCI_GetCapabilities (void)
| Get driver capabilities. More...
int32_t | ARM_USBH_HCI_Initialize (ARM_USBH_HCI_Interrupt_t *cb_interrupt)
| Initialize USB Host HCI (OHCI/EHCI) Interface. More...
int32_t | ARM_USBH_HCI_Uninitialize (void)
| De-initialize USB Host HCI (OHCI/EHCI) Interface. More...
int32_t | ARM_USBH_HCI_PowerControl (ARM_POWER_STATE state)
| Control USB Host HCI (OHCI/EHCI) Interface Power. More...
int32_t | ARM_USBH_HCI_PortVbusOnOff (uint8_t port, bool vbus)
| USB Host HCI (OHCI/EHCI) Root HUB Port VBUS on/off. More...
void | ARM_USBH_HCI_Interrupt (void)
| USB Host HCI Interrupt Handler. More...