CMSIS-Driver: Data Fields - Variables

| CMSIS-Driver Version 2.05 Peripheral Interface for Middleware and Application Code

- Main Page
- Usage and Description
- Reference

- Data Structures
- Data Structure Index
- Data Fields

- All
- Variables

- a
- b
- c
- d
- e
- f
- g
- h
- i
- l
- m
- n
- o
- p
- r
- s
- t
- u
- v
- w

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages

### - u -

- uhs_ddr50 : ARM_MCI_CAPABILITIES
- uhs_driver_type_a : ARM_MCI_CAPABILITIES
- uhs_driver_type_c : ARM_MCI_CAPABILITIES
- uhs_driver_type_d : ARM_MCI_CAPABILITIES
- uhs_sdr104 : ARM_MCI_CAPABILITIES
- uhs_sdr50 : ARM_MCI_CAPABILITIES
- uhs_signaling : ARM_MCI_CAPABILITIES
- uhs_tuning : ARM_MCI_CAPABILITIES
- Uninitialize : ARM_DRIVER_CAN , ARM_DRIVER_ETH_MAC , ARM_DRIVER_ETH_PHY , ARM_DRIVER_FLASH , ARM_DRIVER_I2C , ARM_DRIVER_MCI , ARM_DRIVER_NAND , ARM_DRIVER_SAI , ARM_DRIVER_SPI , ARM_DRIVER_STORAGE , ARM_DRIVER_USART , ARM_DRIVER_USBD , ARM_DRIVER_USBH , ARM_DRIVER_USBH_HCI
- unit_state : ARM_CAN_STATUS