| M480 BSP V3.05.001 The Board Support Package for M480 Series

Data Structures
acmp_reg.h File Reference

ACMP register definition header file. More...

Go to the source code of this file.

## Data Structures
struct | ACMP_T

## Macros
#define | ACMP_CTL_ACMPEN_Pos (0)
#define | ACMP_CTL_ACMPEN_Msk (0x1ul << ACMP_CTL_ACMPEN_Pos)
#define | ACMP_CTL_ACMPIE_Pos (1)
#define | ACMP_CTL_ACMPIE_Msk (0x1ul << ACMP_CTL_ACMPIE_Pos)
#define | ACMP_CTL_ACMPOINV_Pos (3)
#define | ACMP_CTL_ACMPOINV_Msk (0x1ul << ACMP_CTL_ACMPOINV_Pos)
#define | ACMP_CTL_NEGSEL_Pos (4)
#define | ACMP_CTL_NEGSEL_Msk (0x3ul << ACMP_CTL_NEGSEL_Pos)
#define | ACMP_CTL_POSSEL_Pos (6)
#define | ACMP_CTL_POSSEL_Msk (0x3ul << ACMP_CTL_POSSEL_Pos)
#define | ACMP_CTL_INTPOL_Pos (8)
#define | ACMP_CTL_INTPOL_Msk (0x3ul << ACMP_CTL_INTPOL_Pos)
#define | ACMP_CTL_OUTSEL_Pos (12)
#define | ACMP_CTL_OUTSEL_Msk (0x1ul << ACMP_CTL_OUTSEL_Pos)
#define | ACMP_CTL_FILTSEL_Pos (13)
#define | ACMP_CTL_FILTSEL_Msk (0x7ul << ACMP_CTL_FILTSEL_Pos)
#define | ACMP_CTL_WKEN_Pos (16)
#define | ACMP_CTL_WKEN_Msk (0x1ul << ACMP_CTL_WKEN_Pos)
#define | ACMP_CTL_WLATEN_Pos (17)
#define | ACMP_CTL_WLATEN_Msk (0x1ul << ACMP_CTL_WLATEN_Pos)
#define | ACMP_CTL_WCMPSEL_Pos (18)
#define | ACMP_CTL_WCMPSEL_Msk (0x1ul << ACMP_CTL_WCMPSEL_Pos)
#define | ACMP_CTL_HYSSEL_Pos (24)
#define | ACMP_CTL_HYSSEL_Msk (0x3ul << ACMP_CTL_HYSSEL_Pos)
#define | ACMP_CTL_MODESEL_Pos (28)
#define | ACMP_CTL_MODESEL_Msk (0x3ul << ACMP_CTL_MODESEL_Pos)
#define | ACMP_STATUS_ACMPIF0_Pos (0)
#define | ACMP_STATUS_ACMPIF0_Msk (0x1ul << ACMP_STATUS_ACMPIF0_Pos)
#define | ACMP_STATUS_ACMPIF1_Pos (1)
#define | ACMP_STATUS_ACMPIF1_Msk (0x1ul << ACMP_STATUS_ACMPIF1_Pos)
#define | ACMP_STATUS_ACMPO0_Pos (4)
#define | ACMP_STATUS_ACMPO0_Msk (0x1ul << ACMP_STATUS_ACMPO0_Pos)
#define | ACMP_STATUS_ACMPO1_Pos (5)
#define | ACMP_STATUS_ACMPO1_Msk (0x1ul << ACMP_STATUS_ACMPO1_Pos)
#define | ACMP_STATUS_WKIF0_Pos (8)
#define | ACMP_STATUS_WKIF0_Msk (0x1ul << ACMP_STATUS_WKIF0_Pos)
#define | ACMP_STATUS_WKIF1_Pos (9)
#define | ACMP_STATUS_WKIF1_Msk (0x1ul << ACMP_STATUS_WKIF1_Pos)
#define | ACMP_STATUS_ACMPS0_Pos (12)
#define | ACMP_STATUS_ACMPS0_Msk (0x1ul << ACMP_STATUS_ACMPS0_Pos)
#define | ACMP_STATUS_ACMPS1_Pos (13)
#define | ACMP_STATUS_ACMPS1_Msk (0x1ul << ACMP_STATUS_ACMPS1_Pos)
#define | ACMP_STATUS_ACMPWO_Pos (16)
#define | ACMP_STATUS_ACMPWO_Msk (0x1ul << ACMP_STATUS_ACMPWO_Pos)
#define | ACMP_VREF_CRVCTL_Pos (0)
#define | ACMP_VREF_CRVCTL_Msk (0xful << ACMP_VREF_CRVCTL_Pos)
#define | ACMP_VREF_CRVSSEL_Pos (6)
#define | ACMP_VREF_CRVSSEL_Msk (0x1ul << ACMP_VREF_CRVSSEL_Pos)

## Detailed Description

ACMP register definition header file.

Version
  V1.00 SPDX-License-Identifier: Apache-2.0

Copyright
  (C) 2017-2020 Nuvoton Technology Corp. All rights reserved.

Definition in file acmp_reg.h.