| M480 BSP V3.05.001 The Board Support Package for M480 Series

Macros
QSPI Exported Constants
Standard Driver » QSPI Driver

## Macros
#define | QSPI_MODE_0
#define | QSPI_MODE_1
#define | QSPI_MODE_2
#define | QSPI_MODE_3
#define | QSPI_SLAVE
#define | QSPI_MASTER
#define | QSPI_SS
#define | QSPI_SS_ACTIVE_HIGH
#define | QSPI_SS_ACTIVE_LOW
#define | QSPI_UNIT_INT_MASK
#define | QSPI_SSACT_INT_MASK
#define | QSPI_SSINACT_INT_MASK
#define | QSPI_SLVUR_INT_MASK
#define | QSPI_SLVBE_INT_MASK
#define | QSPI_TXUF_INT_MASK
#define | QSPI_FIFO_TXTH_INT_MASK
#define | QSPI_FIFO_RXTH_INT_MASK
#define | QSPI_FIFO_RXOV_INT_MASK
#define | QSPI_FIFO_RXTO_INT_MASK
#define | QSPI_BUSY_MASK
#define | QSPI_RX_EMPTY_MASK
#define | QSPI_RX_FULL_MASK
#define | QSPI_TX_EMPTY_MASK
#define | QSPI_TX_FULL_MASK
#define | QSPI_TXRX_RESET_MASK
#define | QSPI_QSPIEN_STS_MASK
#define | QSPI_SSLINE_STS_MASK

## Detailed Description

## Macro Definition Documentation

## ◆ QSPI_BUSY_MASK

#define QSPI_BUSY_MASK

Busy status mask

Definition at line 55 of file qspi.h.

## ◆ QSPI_FIFO_RXOV_INT_MASK

#define QSPI_FIFO_RXOV_INT_MASK

FIFO RX overrun interrupt mask

Definition at line 51 of file qspi.h.

## ◆ QSPI_FIFO_RXTH_INT_MASK

#define QSPI_FIFO_RXTH_INT_MASK

FIFO RX threshold interrupt mask

Definition at line 50 of file qspi.h.

## ◆ QSPI_FIFO_RXTO_INT_MASK

#define QSPI_FIFO_RXTO_INT_MASK

FIFO RX time-out interrupt mask

Definition at line 52 of file qspi.h.

## ◆ QSPI_FIFO_TXTH_INT_MASK

#define QSPI_FIFO_TXTH_INT_MASK

FIFO TX threshold interrupt mask

Definition at line 49 of file qspi.h.

## ◆ QSPI_MASTER

#define QSPI_MASTER

Set as master

Definition at line 36 of file qspi.h.

## ◆ QSPI_MODE_0

#define QSPI_MODE_0

CLKPOL=0; RXNEG=0; TXNEG=1

Definition at line 30 of file qspi.h.

## ◆ QSPI_MODE_1

#define QSPI_MODE_1

CLKPOL=0; RXNEG=1; TXNEG=0

Definition at line 31 of file qspi.h.

## ◆ QSPI_MODE_2

#define QSPI_MODE_2

CLKPOL=1; RXNEG=1; TXNEG=0

Definition at line 32 of file qspi.h.

## ◆ QSPI_MODE_3

#define QSPI_MODE_3

CLKPOL=1; RXNEG=0; TXNEG=1

Definition at line 33 of file qspi.h.

## ◆ QSPI_QSPIEN_STS_MASK

#define QSPI_QSPIEN_STS_MASK

QSPIEN status mask

Definition at line 61 of file qspi.h.

## ◆ QSPI_RX_EMPTY_MASK

#define QSPI_RX_EMPTY_MASK

RX empty status mask

Definition at line 56 of file qspi.h.

## ◆ QSPI_RX_FULL_MASK

#define QSPI_RX_FULL_MASK

RX full status mask

Definition at line 57 of file qspi.h.

## ◆ QSPI_SLAVE

#define QSPI_SLAVE

Set as slave

Definition at line 35 of file qspi.h.

## ◆ QSPI_SLVBE_INT_MASK

#define QSPI_SLVBE_INT_MASK

Slave bit count error interrupt mask

Definition at line 47 of file qspi.h.

## ◆ QSPI_SLVUR_INT_MASK

#define QSPI_SLVUR_INT_MASK

Slave under run interrupt mask

Definition at line 46 of file qspi.h.

## ◆ QSPI_SS

#define QSPI_SS

Set SS

Definition at line 38 of file qspi.h.

## ◆ QSPI_SS_ACTIVE_HIGH

#define QSPI_SS_ACTIVE_HIGH

SS active high

Definition at line 39 of file qspi.h.

## ◆ QSPI_SS_ACTIVE_LOW

#define QSPI_SS_ACTIVE_LOW

SS active low

Definition at line 40 of file qspi.h.

## ◆ QSPI_SSACT_INT_MASK

#define QSPI_SSACT_INT_MASK

Slave selection signal active interrupt mask

Definition at line 44 of file qspi.h.

## ◆ QSPI_SSINACT_INT_MASK

#define QSPI_SSINACT_INT_MASK

Slave selection signal inactive interrupt mask

Definition at line 45 of file qspi.h.

## ◆ QSPI_SSLINE_STS_MASK

#define QSPI_SSLINE_STS_MASK

QSPIx_SS line status mask

Definition at line 62 of file qspi.h.

## ◆ QSPI_TX_EMPTY_MASK

#define QSPI_TX_EMPTY_MASK

TX empty status mask

Definition at line 58 of file qspi.h.

## ◆ QSPI_TX_FULL_MASK

#define QSPI_TX_FULL_MASK

TX full status mask

Definition at line 59 of file qspi.h.

## ◆ QSPI_TXRX_RESET_MASK

#define QSPI_TXRX_RESET_MASK

TX or RX reset status mask

Definition at line 60 of file qspi.h.

## ◆ QSPI_TXUF_INT_MASK

#define QSPI_TXUF_INT_MASK

Slave TX underflow interrupt mask

Definition at line 48 of file qspi.h.

## ◆ QSPI_UNIT_INT_MASK

#define QSPI_UNIT_INT_MASK

Unit transfer interrupt mask

Definition at line 43 of file qspi.h.