| M480 BSP V3.05.001 The Board Support Package for M480 Series

Macros
PDMA Exported Constants
Standard Driver » PDMA Driver

## Macros
#define | PDMA_CH_MAX
#define | PDMA_OP_STOP
#define | PDMA_OP_BASIC
#define | PDMA_OP_SCATTER
#define | PDMA_WIDTH_8
#define | PDMA_WIDTH_16
#define | PDMA_WIDTH_32
#define | PDMA_SAR_INC
#define | PDMA_SAR_FIX
#define | PDMA_DAR_INC
#define | PDMA_DAR_FIX
#define | PDMA_REQ_SINGLE
#define | PDMA_REQ_BURST
#define | PDMA_BURST_128
#define | PDMA_BURST_64
#define | PDMA_BURST_32
#define | PDMA_BURST_16
#define | PDMA_BURST_8
#define | PDMA_BURST_4
#define | PDMA_BURST_2
#define | PDMA_BURST_1
#define | PDMA_TBINTDIS_ENABLE
#define | PDMA_TBINTDIS_DISABLE
#define | PDMA_MEM
#define | PDMA_USB_TX
#define | PDMA_USB_RX
#define | PDMA_UART0_TX
#define | PDMA_UART0_RX
#define | PDMA_UART1_TX
#define | PDMA_UART1_RX
#define | PDMA_UART2_TX
#define | PDMA_UART2_RX
#define | PDMA_UART3_TX
#define | PDMA_UART3_RX
#define | PDMA_UART4_TX
#define | PDMA_UART4_RX
#define | PDMA_UART5_TX
#define | PDMA_UART5_RX
#define | PDMA_USCI0_TX
#define | PDMA_USCI0_RX
#define | PDMA_USCI1_TX
#define | PDMA_USCI1_RX
#define | PDMA_QSPI0_TX
#define | PDMA_QSPI0_RX
#define | PDMA_SPI0_TX
#define | PDMA_SPI0_RX
#define | PDMA_SPI1_TX
#define | PDMA_SPI1_RX
#define | PDMA_SPI2_TX
#define | PDMA_SPI2_RX
#define | PDMA_SPI3_TX
#define | PDMA_SPI3_RX
#define | PDMA_QSPI1_TX
#define | PDMA_QSPI1_RX
#define | PDMA_EPWM0_P1_RX
#define | PDMA_EPWM0_P2_RX
#define | PDMA_EPWM0_P3_RX
#define | PDMA_EPWM1_P1_RX
#define | PDMA_EPWM1_P2_RX
#define | PDMA_EPWM1_P3_RX
#define | PDMA_I2C0_TX
#define | PDMA_I2C0_RX
#define | PDMA_I2C1_TX
#define | PDMA_I2C1_RX
#define | PDMA_I2C2_TX
#define | PDMA_I2C2_RX
#define | PDMA_I2S0_TX
#define | PDMA_I2S0_RX
#define | PDMA_TMR0
#define | PDMA_TMR1
#define | PDMA_TMR2
#define | PDMA_TMR3
#define | PDMA_EADC0_RX
#define | PDMA_DAC0_TX
#define | PDMA_DAC1_TX
#define | PDMA_EPWM0_CH0_TX
#define | PDMA_EPWM0_CH1_TX
#define | PDMA_EPWM0_CH2_TX
#define | PDMA_EPWM0_CH3_TX
#define | PDMA_EPWM0_CH4_TX
#define | PDMA_EPWM0_CH5_TX
#define | PDMA_EPWM1_CH0_TX
#define | PDMA_EPWM1_CH1_TX
#define | PDMA_EPWM1_CH2_TX
#define | PDMA_EPWM1_CH3_TX
#define | PDMA_EPWM1_CH4_TX
#define | PDMA_EPWM1_CH5_TX
#define | PDMA_UART6_TX
#define | PDMA_UART6_RX
#define | PDMA_UART7_TX
#define | PDMA_UART7_RX
#define | PDMA_EADC1_RX
#define | PDMA_INT_TRANS_DONE
#define | PDMA_INT_TEMPTY
#define | PDMA_INT_TIMEOUT

## Detailed Description

## Macro Definition Documentation

## ◆ PDMA_BURST_1

#define PDMA_BURST_1

DMA Burst 1 Transfers

Definition at line 66 of file pdma.h.

## ◆ PDMA_BURST_128

#define PDMA_BURST_128

DMA Burst 128 Transfers

Definition at line 59 of file pdma.h.

## ◆ PDMA_BURST_16

#define PDMA_BURST_16

DMA Burst 16 Transfers

Definition at line 62 of file pdma.h.

## ◆ PDMA_BURST_2

#define PDMA_BURST_2

DMA Burst 2 Transfers

Definition at line 65 of file pdma.h.

## ◆ PDMA_BURST_32

#define PDMA_BURST_32

DMA Burst 32 Transfers

Definition at line 61 of file pdma.h.

## ◆ PDMA_BURST_4

#define PDMA_BURST_4

DMA Burst 4 Transfers

Definition at line 64 of file pdma.h.

## ◆ PDMA_BURST_64

#define PDMA_BURST_64

DMA Burst 64 Transfers

Definition at line 60 of file pdma.h.

## ◆ PDMA_BURST_8

#define PDMA_BURST_8

DMA Burst 8 Transfers

Definition at line 63 of file pdma.h.

## ◆ PDMA_CH_MAX

#define PDMA_CH_MAX

Specify Maximum Channels of PDMA

Definition at line 29 of file pdma.h.

## ◆ PDMA_DAC0_TX

#define PDMA_DAC0_TX

DMA Connect to DAC0_TX

Definition at line 127 of file pdma.h.

## ◆ PDMA_DAC1_TX

#define PDMA_DAC1_TX

DMA Connect to DAC1_TX

Definition at line 128 of file pdma.h.

## ◆ PDMA_DAR_FIX

#define PDMA_DAR_FIX

DMA DAR fix address

Definition at line 51 of file pdma.h.

## ◆ PDMA_DAR_INC

#define PDMA_DAR_INC

DMA DAR increment

Definition at line 50 of file pdma.h.

## ◆ PDMA_EADC0_RX

#define PDMA_EADC0_RX

DMA Connect to EADC0_RX

Definition at line 126 of file pdma.h.

## ◆ PDMA_EADC1_RX

#define PDMA_EADC1_RX

DMA Connect to EADC1_RX

Definition at line 145 of file pdma.h.

## ◆ PDMA_EPWM0_CH0_TX

#define PDMA_EPWM0_CH0_TX

DMA Connect to EPWM0_CH0_TX

Definition at line 129 of file pdma.h.

## ◆ PDMA_EPWM0_CH1_TX

#define PDMA_EPWM0_CH1_TX

DMA Connect to EPWM0_CH1_TX

Definition at line 130 of file pdma.h.

## ◆ PDMA_EPWM0_CH2_TX

#define PDMA_EPWM0_CH2_TX

DMA Connect to EPWM0_CH2_TX

Definition at line 131 of file pdma.h.

## ◆ PDMA_EPWM0_CH3_TX

#define PDMA_EPWM0_CH3_TX

DMA Connect to EPWM0_CH3_TX

Definition at line 132 of file pdma.h.

## ◆ PDMA_EPWM0_CH4_TX

#define PDMA_EPWM0_CH4_TX

DMA Connect to EPWM0_CH4_TX

Definition at line 133 of file pdma.h.

## ◆ PDMA_EPWM0_CH5_TX

#define PDMA_EPWM0_CH5_TX

DMA Connect to EPWM0_CH5_TX

Definition at line 134 of file pdma.h.

## ◆ PDMA_EPWM0_P1_RX

#define PDMA_EPWM0_P1_RX

DMA Connect to EPWM0_P1

Definition at line 108 of file pdma.h.

## ◆ PDMA_EPWM0_P2_RX

#define PDMA_EPWM0_P2_RX

DMA Connect to EPWM0_P2

Definition at line 109 of file pdma.h.

## ◆ PDMA_EPWM0_P3_RX

#define PDMA_EPWM0_P3_RX

DMA Connect to EPWM0_P3

Definition at line 110 of file pdma.h.

## ◆ PDMA_EPWM1_CH0_TX

#define PDMA_EPWM1_CH0_TX

DMA Connect to EPWM1_CH0_TX

Definition at line 135 of file pdma.h.

## ◆ PDMA_EPWM1_CH1_TX

#define PDMA_EPWM1_CH1_TX

DMA Connect to EPWM1_CH1_TX

Definition at line 136 of file pdma.h.

## ◆ PDMA_EPWM1_CH2_TX

#define PDMA_EPWM1_CH2_TX

DMA Connect to EPWM1_CH2_TX

Definition at line 137 of file pdma.h.

## ◆ PDMA_EPWM1_CH3_TX

#define PDMA_EPWM1_CH3_TX

DMA Connect to EPWM1_CH3_TX

Definition at line 138 of file pdma.h.

## ◆ PDMA_EPWM1_CH4_TX

#define PDMA_EPWM1_CH4_TX

DMA Connect to EPWM1_CH4_TX

Definition at line 139 of file pdma.h.

## ◆ PDMA_EPWM1_CH5_TX

#define PDMA_EPWM1_CH5_TX

DMA Connect to EPWM1_CH5_TX

Definition at line 140 of file pdma.h.

## ◆ PDMA_EPWM1_P1_RX

#define PDMA_EPWM1_P1_RX

DMA Connect to EPWM1_P1

Definition at line 111 of file pdma.h.

## ◆ PDMA_EPWM1_P2_RX

#define PDMA_EPWM1_P2_RX

DMA Connect to EPWM1_P2

Definition at line 112 of file pdma.h.

## ◆ PDMA_EPWM1_P3_RX

#define PDMA_EPWM1_P3_RX

DMA Connect to PWM1_P3

Definition at line 113 of file pdma.h.

## ◆ PDMA_I2C0_RX

#define PDMA_I2C0_RX

DMA Connect to I2C0_RX

Definition at line 115 of file pdma.h.

## ◆ PDMA_I2C0_TX

#define PDMA_I2C0_TX

DMA Connect to I2C0_TX

Definition at line 114 of file pdma.h.

## ◆ PDMA_I2C1_RX

#define PDMA_I2C1_RX

DMA Connect to I2C1_RX

Definition at line 117 of file pdma.h.

## ◆ PDMA_I2C1_TX

#define PDMA_I2C1_TX

DMA Connect to I2C1_TX

Definition at line 116 of file pdma.h.

## ◆ PDMA_I2C2_RX

#define PDMA_I2C2_RX

DMA Connect to I2C2_RX

Definition at line 119 of file pdma.h.

## ◆ PDMA_I2C2_TX

#define PDMA_I2C2_TX

DMA Connect to I2C2_TX

Definition at line 118 of file pdma.h.

## ◆ PDMA_I2S0_RX

#define PDMA_I2S0_RX

DMA Connect to I2S0_RX

Definition at line 121 of file pdma.h.

## ◆ PDMA_I2S0_TX

#define PDMA_I2S0_TX

DMA Connect to I2S0_TX

Definition at line 120 of file pdma.h.

## ◆ PDMA_INT_TEMPTY

#define PDMA_INT_TEMPTY

Table Empty Interrupt

Definition at line 150 of file pdma.h.

## ◆ PDMA_INT_TIMEOUT

#define PDMA_INT_TIMEOUT

Timeout Interrupt

Definition at line 151 of file pdma.h.

## ◆ PDMA_INT_TRANS_DONE

#define PDMA_INT_TRANS_DONE

Transfer Done Interrupt

Definition at line 149 of file pdma.h.

## ◆ PDMA_MEM

#define PDMA_MEM

DMA Connect to Memory

Definition at line 77 of file pdma.h.

## ◆ PDMA_OP_BASIC

#define PDMA_OP_BASIC

DMA Basic Mode

Definition at line 35 of file pdma.h.

## ◆ PDMA_OP_SCATTER

#define PDMA_OP_SCATTER

DMA Scatter-gather Mode

Definition at line 36 of file pdma.h.

## ◆ PDMA_OP_STOP

#define PDMA_OP_STOP

DMA Stop Mode

Definition at line 34 of file pdma.h.

## ◆ PDMA_QSPI0_RX

#define PDMA_QSPI0_RX

DMA Connect to QSPI0_RX

Definition at line 97 of file pdma.h.

## ◆ PDMA_QSPI0_TX

#define PDMA_QSPI0_TX

DMA Connect to QSPI0_TX

Definition at line 96 of file pdma.h.

## ◆ PDMA_QSPI1_RX

#define PDMA_QSPI1_RX

DMA Connect to QSPI1_RX

Definition at line 107 of file pdma.h.

## ◆ PDMA_QSPI1_TX

#define PDMA_QSPI1_TX

DMA Connect to QSPI1_TX

Definition at line 106 of file pdma.h.

## ◆ PDMA_REQ_BURST

#define PDMA_REQ_BURST

DMA Burst Request

Definition at line 57 of file pdma.h.

## ◆ PDMA_REQ_SINGLE

#define PDMA_REQ_SINGLE

DMA Single Request

Definition at line 56 of file pdma.h.

## ◆ PDMA_SAR_FIX

#define PDMA_SAR_FIX

DMA SAR fix address

Definition at line 49 of file pdma.h.

## ◆ PDMA_SAR_INC

#define PDMA_SAR_INC

DMA SAR increment

Definition at line 48 of file pdma.h.

## ◆ PDMA_SPI0_RX

#define PDMA_SPI0_RX

DMA Connect to SPI0_RX

Definition at line 99 of file pdma.h.

## ◆ PDMA_SPI0_TX

#define PDMA_SPI0_TX

DMA Connect to SPI0_TX

Definition at line 98 of file pdma.h.

## ◆ PDMA_SPI1_RX

#define PDMA_SPI1_RX

DMA Connect to SPI1_RX

Definition at line 101 of file pdma.h.

## ◆ PDMA_SPI1_TX

#define PDMA_SPI1_TX

DMA Connect to SPI1_TX

Definition at line 100 of file pdma.h.

## ◆ PDMA_SPI2_RX

#define PDMA_SPI2_RX

DMA Connect to SPI2_RX

Definition at line 103 of file pdma.h.

## ◆ PDMA_SPI2_TX

#define PDMA_SPI2_TX

DMA Connect to SPI2_TX

Definition at line 102 of file pdma.h.

## ◆ PDMA_SPI3_RX

#define PDMA_SPI3_RX

DMA Connect to SPI3_RX

Definition at line 105 of file pdma.h.

## ◆ PDMA_SPI3_TX

#define PDMA_SPI3_TX

DMA Connect to SPI3_TX

Definition at line 104 of file pdma.h.

## ◆ PDMA_TBINTDIS_DISABLE

#define PDMA_TBINTDIS_DISABLE

DMA Table Interrupt Disabled

Definition at line 72 of file pdma.h.

## ◆ PDMA_TBINTDIS_ENABLE

#define PDMA_TBINTDIS_ENABLE

DMA Table Interrupt Enabled

Definition at line 71 of file pdma.h.

## ◆ PDMA_TMR0

#define PDMA_TMR0

DMA Connect to TMR0

Definition at line 122 of file pdma.h.

## ◆ PDMA_TMR1

#define PDMA_TMR1

DMA Connect to TMR1

Definition at line 123 of file pdma.h.

## ◆ PDMA_TMR2

#define PDMA_TMR2

DMA Connect to TMR2

Definition at line 124 of file pdma.h.

## ◆ PDMA_TMR3

#define PDMA_TMR3

DMA Connect to TMR3

Definition at line 125 of file pdma.h.

## ◆ PDMA_UART0_RX

#define PDMA_UART0_RX

DMA Connect to UART0_RX

Definition at line 81 of file pdma.h.

## ◆ PDMA_UART0_TX

#define PDMA_UART0_TX

DMA Connect to UART0_TX

Definition at line 80 of file pdma.h.

## ◆ PDMA_UART1_RX

#define PDMA_UART1_RX

DMA Connect to UART1_RX

Definition at line 83 of file pdma.h.

## ◆ PDMA_UART1_TX

#define PDMA_UART1_TX

DMA Connect to UART1_TX

Definition at line 82 of file pdma.h.

## ◆ PDMA_UART2_RX

#define PDMA_UART2_RX

DMA Connect to UART2_RX

Definition at line 85 of file pdma.h.

## ◆ PDMA_UART2_TX

#define PDMA_UART2_TX

DMA Connect to UART2_TX

Definition at line 84 of file pdma.h.

## ◆ PDMA_UART3_RX

#define PDMA_UART3_RX

DMA Connect to UART3_RX

Definition at line 87 of file pdma.h.

## ◆ PDMA_UART3_TX

#define PDMA_UART3_TX

DMA Connect to UART3_TX

Definition at line 86 of file pdma.h.

## ◆ PDMA_UART4_RX

#define PDMA_UART4_RX

DMA Connect to UART4_RX

Definition at line 89 of file pdma.h.

## ◆ PDMA_UART4_TX

#define PDMA_UART4_TX

DMA Connect to UART4_TX

Definition at line 88 of file pdma.h.

## ◆ PDMA_UART5_RX

#define PDMA_UART5_RX

DMA Connect to UART5_RX

Definition at line 91 of file pdma.h.

## ◆ PDMA_UART5_TX

#define PDMA_UART5_TX

DMA Connect to UART5_TX

Definition at line 90 of file pdma.h.

## ◆ PDMA_UART6_RX

#define PDMA_UART6_RX

DMA Connect to UART6_RX

Definition at line 142 of file pdma.h.

## ◆ PDMA_UART6_TX

#define PDMA_UART6_TX

DMA Connect to UART6_TX

Definition at line 141 of file pdma.h.

## ◆ PDMA_UART7_RX

#define PDMA_UART7_RX

DMA Connect to UART7_RX

Definition at line 144 of file pdma.h.

## ◆ PDMA_UART7_TX

#define PDMA_UART7_TX

DMA Connect to UART7_TX

Definition at line 143 of file pdma.h.

## ◆ PDMA_USB_RX

#define PDMA_USB_RX

DMA Connect to USB_RX

Definition at line 79 of file pdma.h.

## ◆ PDMA_USB_TX

#define PDMA_USB_TX

DMA Connect to USB_TX

Definition at line 78 of file pdma.h.

## ◆ PDMA_USCI0_RX

#define PDMA_USCI0_RX

DMA Connect to USCI0_RX

Definition at line 93 of file pdma.h.

## ◆ PDMA_USCI0_TX

#define PDMA_USCI0_TX

DMA Connect to USCI0_TX

Definition at line 92 of file pdma.h.

## ◆ PDMA_USCI1_RX

#define PDMA_USCI1_RX

DMA Connect to USCI1_RX

Definition at line 95 of file pdma.h.

## ◆ PDMA_USCI1_TX

#define PDMA_USCI1_TX

DMA Connect to USCI1_TX

Definition at line 94 of file pdma.h.

## ◆ PDMA_WIDTH_16

#define PDMA_WIDTH_16

DMA Transfer Width 16-bit

Definition at line 42 of file pdma.h.

## ◆ PDMA_WIDTH_32

#define PDMA_WIDTH_32

DMA Transfer Width 32-bit

Definition at line 43 of file pdma.h.

## ◆ PDMA_WIDTH_8

#define PDMA_WIDTH_8

DMA Transfer Width 8-bit

Definition at line 41 of file pdma.h.