| M480 BSP V3.05.001 The Board Support Package for M480 Series

Macros
CRC Exported Constants
Standard Driver » CRC Driver

## Macros
#define | CRC_CCITT
#define | CRC_8
#define | CRC_16
#define | CRC_32
#define | CRC_CHECKSUM_COM
#define | CRC_CHECKSUM_RVS
#define | CRC_WDATA_COM
#define | CRC_WDATA_RVS
#define | CRC_CPU_WDATA_8
#define | CRC_CPU_WDATA_16
#define | CRC_CPU_WDATA_32

## Detailed Description

## Macro Definition Documentation

## ◆ CRC_16

#define CRC_16

CRC Polynomial Mode - CRC16

Definition at line 34 of file crc.h.

## ◆ CRC_32

#define CRC_32

CRC Polynomial Mode - CRC32

Definition at line 35 of file crc.h.

## ◆ CRC_8

#define CRC_8

CRC Polynomial Mode - CRC8

Definition at line 33 of file crc.h.

## ◆ CRC_CCITT

#define CRC_CCITT

CRC Polynomial Mode - CCITT

Definition at line 32 of file crc.h.

## ◆ CRC_CHECKSUM_COM

#define CRC_CHECKSUM_COM

CRC Checksum Complement

Definition at line 40 of file crc.h.

## ◆ CRC_CHECKSUM_RVS

#define CRC_CHECKSUM_RVS

CRC Checksum Reverse

Definition at line 41 of file crc.h.

## ◆ CRC_CPU_WDATA_16

#define CRC_CPU_WDATA_16

CRC CPU Write Data length is 16-bit

Definition at line 49 of file crc.h.

## ◆ CRC_CPU_WDATA_32

#define CRC_CPU_WDATA_32

CRC CPU Write Data length is 32-bit

Definition at line 50 of file crc.h.

## ◆ CRC_CPU_WDATA_8

#define CRC_CPU_WDATA_8

CRC CPU Write Data length is 8-bit

Definition at line 48 of file crc.h.

## ◆ CRC_WDATA_COM

#define CRC_WDATA_COM

CRC Write Data Complement

Definition at line 42 of file crc.h.

## ◆ CRC_WDATA_RVS

#define CRC_WDATA_RVS

CRC Write Data Reverse

Definition at line 43 of file crc.h.