| M480 BSP V3.05.001 The Board Support Package for M480 Series

Macros
DAC Exported Constants
Standard Driver » DAC Driver

## Macros
#define | DAC_CTL_LALIGN_RIGHT_ALIGN
#define | DAC_CTL_LALIGN_LEFT_ALIGN
#define | DAC_WRITE_DAT_TRIGGER
#define | DAC_SOFTWARE_TRIGGER
#define | DAC_LOW_LEVEL_TRIGGER
#define | DAC_HIGH_LEVEL_TRIGGER
#define | DAC_FALLING_EDGE_TRIGGER
#define | DAC_RISING_EDGE_TRIGGER
#define | DAC_TIMER0_TRIGGER
#define | DAC_TIMER1_TRIGGER
#define | DAC_TIMER2_TRIGGER
#define | DAC_TIMER3_TRIGGER
#define | DAC_EPWM0_TRIGGER
#define | DAC_EPWM1_TRIGGER
#define | DAC_TRIGGER_MODE_DISABLE
#define | DAC_TRIGGER_MODE_ENABLE

## Detailed Description

## Macro Definition Documentation

## ◆ DAC_CTL_LALIGN_LEFT_ALIGN

#define DAC_CTL_LALIGN_LEFT_ALIGN

Left alignment

Definition at line 35 of file dac.h.

## ◆ DAC_CTL_LALIGN_RIGHT_ALIGN

#define DAC_CTL_LALIGN_RIGHT_ALIGN

Right alignment.

Definition at line 34 of file dac.h.

## ◆ DAC_EPWM0_TRIGGER

#define DAC_EPWM0_TRIGGER

EPWM0 trigger

Definition at line 47 of file dac.h.

## ◆ DAC_EPWM1_TRIGGER

#define DAC_EPWM1_TRIGGER

EPWM1 trigger

Definition at line 48 of file dac.h.

## ◆ DAC_FALLING_EDGE_TRIGGER

#define DAC_FALLING_EDGE_TRIGGER

STDAC pin falling edge trigger

Definition at line 41 of file dac.h.

## ◆ DAC_HIGH_LEVEL_TRIGGER

#define DAC_HIGH_LEVEL_TRIGGER

STDAC pin high level trigger

Definition at line 40 of file dac.h.

## ◆ DAC_LOW_LEVEL_TRIGGER

#define DAC_LOW_LEVEL_TRIGGER

STDAC pin low level trigger

Definition at line 39 of file dac.h.

## ◆ DAC_RISING_EDGE_TRIGGER

#define DAC_RISING_EDGE_TRIGGER

STDAC pin rising edge trigger

Definition at line 42 of file dac.h.

## ◆ DAC_SOFTWARE_TRIGGER

#define DAC_SOFTWARE_TRIGGER

Software trigger

Definition at line 38 of file dac.h.

## ◆ DAC_TIMER0_TRIGGER

#define DAC_TIMER0_TRIGGER

Timer 0 trigger

Definition at line 43 of file dac.h.

## ◆ DAC_TIMER1_TRIGGER

#define DAC_TIMER1_TRIGGER

Timer 1 trigger

Definition at line 44 of file dac.h.

## ◆ DAC_TIMER2_TRIGGER

#define DAC_TIMER2_TRIGGER

Timer 2 trigger

Definition at line 45 of file dac.h.

## ◆ DAC_TIMER3_TRIGGER

#define DAC_TIMER3_TRIGGER

Timer 3 trigger

Definition at line 46 of file dac.h.

## ◆ DAC_TRIGGER_MODE_DISABLE

#define DAC_TRIGGER_MODE_DISABLE

Trigger mode disable

Definition at line 50 of file dac.h.

## ◆ DAC_TRIGGER_MODE_ENABLE

#define DAC_TRIGGER_MODE_ENABLE

Trigger mode enable

Definition at line 51 of file dac.h.

## ◆ DAC_WRITE_DAT_TRIGGER

#define DAC_WRITE_DAT_TRIGGER

Write DAC_DAT trigger

Definition at line 37 of file dac.h.