| M480 BSP V3.05.001 The Board Support Package for M480 Series

Macros
FMC Exported Macros
Standard Driver » FMC Driver

## Macros
#define | FMC_SET_APROM_BOOT()
#define | FMC_SET_LDROM_BOOT()
#define | FMC_ENABLE_AP_UPDATE()
#define | FMC_DISABLE_AP_UPDATE()
#define | FMC_ENABLE_CFG_UPDATE()
#define | FMC_DISABLE_CFG_UPDATE()
#define | FMC_ENABLE_LD_UPDATE()
#define | FMC_DISABLE_LD_UPDATE()
#define | FMC_ENABLE_SP_UPDATE()
#define | FMC_DISABLE_SP_UPDATE()
#define | FMC_DISABLE_ISP()
#define | FMC_ENABLE_ISP()
#define | FMC_GET_FAIL_FLAG()
#define | FMC_CLR_FAIL_FLAG()

## Detailed Description

## Macro Definition Documentation

## ◆ FMC_CLR_FAIL_FLAG

#define FMC_CLR_FAIL_FLAG | ( |  | ) |

Clear ISP fail flag

Definition at line 127 of file fmc.h.

## ◆ FMC_DISABLE_AP_UPDATE

#define FMC_DISABLE_AP_UPDATE | ( |  | ) |

Disable APROM update

Definition at line 117 of file fmc.h.

## ◆ FMC_DISABLE_CFG_UPDATE

#define FMC_DISABLE_CFG_UPDATE | ( |  | ) |

Disable User Config update

Definition at line 119 of file fmc.h.

## ◆ FMC_DISABLE_ISP

#define FMC_DISABLE_ISP | ( |  | ) |

Disable ISP function

Definition at line 124 of file fmc.h.

## ◆ FMC_DISABLE_LD_UPDATE

#define FMC_DISABLE_LD_UPDATE | ( |  | ) |

Disable LDROM update

Definition at line 121 of file fmc.h.

## ◆ FMC_DISABLE_SP_UPDATE

#define FMC_DISABLE_SP_UPDATE | ( |  | ) |

Disable SPROM update

Definition at line 123 of file fmc.h.

## ◆ FMC_ENABLE_AP_UPDATE

#define FMC_ENABLE_AP_UPDATE | ( |  | ) |

Enable APROM update

Definition at line 116 of file fmc.h.

## ◆ FMC_ENABLE_CFG_UPDATE

#define FMC_ENABLE_CFG_UPDATE | ( |  | ) |

Enable User Config update

Definition at line 118 of file fmc.h.

## ◆ FMC_ENABLE_ISP

#define FMC_ENABLE_ISP | ( |  | ) |

Enable ISP function

Definition at line 125 of file fmc.h.

## ◆ FMC_ENABLE_LD_UPDATE

#define FMC_ENABLE_LD_UPDATE | ( |  | ) |

Enable LDROM update

Definition at line 120 of file fmc.h.

## ◆ FMC_ENABLE_SP_UPDATE

#define FMC_ENABLE_SP_UPDATE | ( |  | ) |

Enable SPROM update

Definition at line 122 of file fmc.h.

## ◆ FMC_GET_FAIL_FLAG

#define FMC_GET_FAIL_FLAG | ( |  | ) |

Get ISP fail flag

Definition at line 126 of file fmc.h.

## ◆ FMC_SET_APROM_BOOT

#define FMC_SET_APROM_BOOT | ( |  | ) |

Select booting from APROM

Definition at line 114 of file fmc.h.

## ◆ FMC_SET_LDROM_BOOT

#define FMC_SET_LDROM_BOOT | ( |  | ) |

Select booting from LDROM

Definition at line 115 of file fmc.h.