CMSIS-CORE: D-Cache Functions

| CMSIS-CORE Version 4.30 CMSIS-CORE support for Cortex-M processor-based devices

- Main Page
- Usage and Description
- Reference

All Data Structures Files Functions Variables Enumerations Enumerator Groups Pages
Functions
D-Cache Functions
Cache Functions (only Cortex-M7)

Functions for the data cache. More...

## Functions
__STATIC_INLINE void | SCB_EnableDCache (void)
| Enable D-Cache.
__STATIC_INLINE void | SCB_DisableDCache (void)
| Disable D-Cache.
__STATIC_INLINE void | SCB_InvalidateDCache (void)
| Invalidate D-Cache.
__STATIC_INLINE void | SCB_CleanDCache (void)
| Clean D-Cache.
__STATIC_INLINE void | SCB_CleanInvalidateDCache (void)
| Clean & Invalidate D-Cache.
__STATIC_INLINE void | SCB_InvalidateDCache_by_Addr (uint32_t *addr, int32_t dsize)
| D-Cache Invalidate by address.
__STATIC_INLINE void | SCB_CleanDCache_by_Addr (uint32_t *addr, int32_t dsize)
| D-Cache Clean by address.
__STATIC_INLINE void | SCB_CleanInvalidateDCache_by_Addr (uint32_t *addr, int32_t dsize)
| D-Cache Clean and Invalidate by address.

## Description

// close ICache functions

## Function Documentation

__STATIC_INLINE void SCB_CleanDCache | ( | void |  | ) |

The function cleans the entire data cache.

__STATIC_INLINE void SCB_CleanDCache_by_Addr | ( | uint32_t * | addr,
|  | int32_t | dsize
| ) |  |

Parameters

  [in] | addr | address (aligned to 32-byte boundary)
  [in] | dsize | size of memory block (in number of bytes)

The function cleans a memory block of size dsize [bytes] starting at address address. The address is aligned to 32-byte boundry.

__STATIC_INLINE void SCB_CleanInvalidateDCache | ( | void |  | ) |

The function cleans and invalidates the entire data cache.

__STATIC_INLINE void SCB_CleanInvalidateDCache_by_Addr | ( | uint32_t * | addr,
|  | int32_t | dsize
| ) |  |

Parameters

  [in] | addr | address (aligned to 32-byte boundary)
  [in] | dsize | size of memory block (in number of bytes)

The function invalidates and cleans a memory block of size dsize [bytes] starting at address address. The address is aligned to 32-byte boundry.

__STATIC_INLINE void SCB_DisableDCache | ( | void |  | ) |

The function turns off the entire data cache.

Note
  When disabling the data cache, you must clean (SCB_CleanDCache) the entire cache to ensure that any dirty data is flushed to external memory.

__STATIC_INLINE void SCB_EnableDCache | ( | void |  | ) |

The function turns on the entire data cache.

Note
  Before enabling the data cache, you must invalidate the entire data cache (SCB_InvalidateDCache), because external memory might have changed from when the cache was disabled.
  After reset, you must invalidate (SCB_InvalidateDCache) each cache before enabling it.

__STATIC_INLINE void SCB_InvalidateDCache | ( | void |  | ) |

The function invalidates the entire data cache.

Note
  After reset, you must invalidate each cache before enabling (SCB_EnableDCache) it.

__STATIC_INLINE void SCB_InvalidateDCache_by_Addr | ( | uint32_t * | addr,
|  | int32_t | dsize
| ) |  |

Parameters

  [in] | addr | address (aligned to 32-byte boundary)
  [in] | dsize | size of memory block (in number of bytes)

The function invalidates a memory block of size dsize [bytes] starting at address address. The address is aligned to 32-byte boundry.