CMSIS-CORE: FPU Functions (only Cortex-M7)

| CMSIS-CORE Version 4.30 CMSIS-CORE support for Cortex-M processor-based devices

- Main Page
- Usage and Description
- Reference

All Data Structures Files Functions Variables Enumerations Enumerator Groups Pages
Functions
FPU Functions (only Cortex-M7)

Functions that relate to the Floating-Point Arithmetic Unit. More...

## Functions
__STATIC_INLINE uint32_t | SCB_GetFPUType (void)
| Get the FPU type.

## Description

The Cortex-M7 processor includes optional floating-point arithmetic functionality, with support for single and double-precision arithmetic. The Cortex-M7 processor with FPU is an implementation of the single-precision and double-precision variant of the ARMv7-M Architecture with Floating-Point Extension (FPv5).

## Function Documentation

__STATIC_INLINE uint32_t SCB_GetFPUType | ( | void |  | ) |

Returns
  - 0: No FPU
  - 1: Single precision FPU
  - 2: Double + Single precision FPU

The function returns the implemented FPU type.