CMSIS-DAP: DAP_Disconnect

| CMSIS-DAP Version 1.1.0 Interface Firmware for CoreSight Debug Access Port

- Main Page
- Usage and Description
- Reference

All Functions Groups Pages
DAP_Disconnect
General Commands

Disconnect from active Debug Port. More...

Disconnect from active Debug Port.

The DAP_Disconnect Command de-initializes the DAP I/O pins by calling the function PORT_OFF.

DAP_Disconnect Command:

BYTE |
> 0x03 |
******|

DAP_Disconnect Response:

BYTE | BYTE |
< 0x03 | Status |
******|********|

- Status: Response Status