| CMSIS-Core (Cortex-M) CMSIS-Core support for Cortex-M processor-based devices |

Loading...
Searching...
No Matches
Data Structures
Here are the data structures with brief descriptions:

C APSR_Type | Union type to access the Application Program Status Register (APSR)
C ARM_MPU_Region_t | Setup information of a single MPU Region
C CONTROL_Type | Union type to access the Control Registers (CONTROL)
C CoreDebug_Type | [Deprecated] Structure type to access the Core Debug Register
C DCB_Type | Structure type to access the Debug Control Block Registers (DCB)
C DIB_Type | Structure type to access the Debug Identification Block Registers (DIB)
C DWT_Type | Structure type to access the Data Watchpoint and Trace Register (DWT)
C EWIC_Type | Structure type to access the External Wakeup Interrupt Controller Registers (EWIC)
C FPU_Type | Structure type to access the Floating Point Unit (FPU)
C ICB_Type | Structure type to access the Implementation Control Block Register (ICB)
C IPSR_Type | Union type to access the Interrupt Program Status Register (IPSR)
C ITM_Type | Structure type to access the Instrumentation Trace Macrocell Register (ITM)
C MPU_Type | Structure type to access the Memory Protection Unit (MPU)
C NVIC_Type | Structure type to access the Nested Vectored Interrupt Controller (NVIC)
C PMU_Type | Structure type to access the Performance Monitoring Unit (PMU)
C SCB_Type | Structure type to access the System Control Block (SCB)
C SCnSCB_Type | Structure type to access the System Control and ID Register not in the SCB
C SysTick_Type | Structure type to access the System Timer (SysTick)
C TPIU_Type | Structure type to access the Trace Port Interface Register (TPI)
C xPSR_Type | Union type to access the Special-Purpose Program Status Registers (xPSR)