CMSIS-DAP: Transfer Commands

| CMSIS-DAP Version 1.1.0 Interface Firmware for CoreSight Debug Access Port

- Main Page
- Usage and Description
- Reference

All Functions Groups Pages
Content
Transfer Commands
CMSIS-DAP Commands

Read and Writes to CoreSight registers. More...

## Content
| DAP_TransferConfigure
| Configure Transfers.
| DAP_Transfer
| Read/write single and multiple registers.
| DAP_TransferBlock
| Read/Write a block of data from/to a single register.
| DAP_TransferAbort
| Abort current Transfer.

## Description

Read and Writes to CoreSight registers.

The Transfer Commands allow to:

- Configure the parameters for information exchange with CoreSight registers.
- Transfer (read or write) a single data word or a data block with CoreSight registers.
- Terminate an active data transfer.