| MINI55_BSP V3.02.004 The Board Support Package for Mini55 Series MCU

Modules | Data Structures
MINI55 Definitions
Collaboration diagram for MINI55 Definitions:

## Modules
| Device CMSIS Definitions

## Data Structures
struct | CLK_T
#define | CLK_PWRCTL_XTLEN_Pos (0)
#define | CLK_PWRCTL_XTLEN_Msk (0x3ul << CLK_PWRCTL_XTLEN_Pos)
#define | CLK_PWRCTL_HIRCEN_Pos (2)
#define | CLK_PWRCTL_HIRCEN_Msk (0x1ul << CLK_PWRCTL_HIRCEN_Pos)
#define | CLK_PWRCTL_LIRCEN_Pos (3)
#define | CLK_PWRCTL_LIRCEN_Msk (0x1ul << CLK_PWRCTL_LIRCEN_Pos)
#define | CLK_PWRCTL_PDWKDLY_Pos (4)
#define | CLK_PWRCTL_PDWKDLY_Msk (0x1ul << CLK_PWRCTL_PDWKDLY_Pos)
#define | CLK_PWRCTL_PDWKIEN_Pos (5)
#define | CLK_PWRCTL_PDWKIEN_Msk (0x1ul << CLK_PWRCTL_PDWKIEN_Pos)
#define | CLK_PWRCTL_PDWKIF_Pos (6)
#define | CLK_PWRCTL_PDWKIF_Msk (0x1ul << CLK_PWRCTL_PDWKIF_Pos)
#define | CLK_PWRCTL_PDEN_Pos (7)
#define | CLK_PWRCTL_PDEN_Msk (0x1ul << CLK_PWRCTL_PDEN_Pos)
#define | CLK_PWRCTL_PDLXT_Pos (9)
#define | CLK_PWRCTL_PDLXT_Msk (0x1ul << CLK_PWRCTL_PDLXT_Pos)
#define | CLK_PWRCTL_HXTGAIN_Pos (10)
#define | CLK_PWRCTL_HXTGAIN_Msk (0x3ul << CLK_PWRCTL_HXTGAIN_Pos)
#define | CLK_AHBCLK_ISPCKEN_Pos (2)
#define | CLK_AHBCLK_ISPCKEN_Msk (0x1ul << CLK_AHBCLK_ISPCKEN_Pos)
#define | CLK_AHBCLK_HDIVCKEN_Pos (4)
#define | CLK_AHBCLK_HDIVCKEN_Msk (0x1ul << CLK_AHBCLK_HDIVCKEN_Pos)
#define | CLK_APBCLK_WDTCKEN_Pos (0)
#define | CLK_APBCLK_WDTCKEN_Msk (0x1ul << CLK_APBCLK_WDTCKEN_Pos)
#define | CLK_APBCLK_TMR0CKEN_Pos (2)
#define | CLK_APBCLK_TMR0CKEN_Msk (0x1ul << CLK_APBCLK_TMR0CKEN_Pos)
#define | CLK_APBCLK_TMR1CKEN_Pos (3)
#define | CLK_APBCLK_TMR1CKEN_Msk (0x1ul << CLK_APBCLK_TMR1CKEN_Pos)
#define | CLK_APBCLK_CLKOCKEN_Pos (6)
#define | CLK_APBCLK_CLKOCKEN_Msk (0x1ul << CLK_APBCLK_CLKOCKEN_Pos)
#define | CLK_APBCLK_I2CCKEN_Pos (8)
#define | CLK_APBCLK_I2CCKEN_Msk (0x1ul << CLK_APBCLK_I2CCKEN_Pos)
#define | CLK_APBCLK_SPICKEN_Pos (12)
#define | CLK_APBCLK_SPICKEN_Msk (0x1ul << CLK_APBCLK_SPICKEN_Pos)
#define | CLK_APBCLK_UART0CKEN_Pos (16)
#define | CLK_APBCLK_UART0CKEN_Msk (0x1ul << CLK_APBCLK_UART0CKEN_Pos)
#define | CLK_APBCLK_UART1CKEN_Pos (17)
#define | CLK_APBCLK_UART1CKEN_Msk (0x1ul << CLK_APBCLK_UART1CKEN_Pos)
#define | CLK_APBCLK_PWMCH01CKEN_Pos (20)
#define | CLK_APBCLK_PWMCH01CKEN_Msk (0x1ul << CLK_APBCLK_PWMCH01CKEN_Pos)
#define | CLK_APBCLK_PWMCH23CKEN_Pos (21)
#define | CLK_APBCLK_PWMCH23CKEN_Msk (0x1ul << CLK_APBCLK_PWMCH23CKEN_Pos)
#define | CLK_APBCLK_PWMCH45CKEN_Pos (22)
#define | CLK_APBCLK_PWMCH45CKEN_Msk (0x1ul << CLK_APBCLK_PWMCH45CKEN_Pos)
#define | CLK_APBCLK_ADCCKEN_Pos (28)
#define | CLK_APBCLK_ADCCKEN_Msk (0x1ul << CLK_APBCLK_ADCCKEN_Pos)
#define | CLK_APBCLK_ACMPCKEN_Pos (30)
#define | CLK_APBCLK_ACMPCKEN_Msk (0x1ul << CLK_APBCLK_ACMPCKEN_Pos)
#define | CLK_STATUS_XTLSTB_Pos (0)
#define | CLK_STATUS_XTLSTB_Msk (0x1ul << CLK_STATUS_XTLSTB_Pos)
#define | CLK_STATUS_LIRCSTB_Pos (3)
#define | CLK_STATUS_LIRCSTB_Msk (0x1ul << CLK_STATUS_LIRCSTB_Pos)
#define | CLK_STATUS_HIRCSTB_Pos (4)
#define | CLK_STATUS_HIRCSTB_Msk (0x1ul << CLK_STATUS_HIRCSTB_Pos)
#define | CLK_STATUS_CLKSFAIL_Pos (7)
#define | CLK_STATUS_CLKSFAIL_Msk (0x1ul << CLK_STATUS_CLKSFAIL_Pos)
#define | CLK_CLKSEL0_HCLKSEL_Pos (0)
#define | CLK_CLKSEL0_HCLKSEL_Msk (0x7ul << CLK_CLKSEL0_HCLKSEL_Pos)
#define | CLK_CLKSEL0_STCLKSEL_Pos (3)
#define | CLK_CLKSEL0_STCLKSEL_Msk (0x7ul << CLK_CLKSEL0_STCLKSEL_Pos)
#define | CLK_CLKSEL1_WDTSEL_Pos (0)
#define | CLK_CLKSEL1_WDTSEL_Msk (0x3ul << CLK_CLKSEL1_WDTSEL_Pos)
#define | CLK_CLKSEL1_ADCSEL_Pos (2)
#define | CLK_CLKSEL1_ADCSEL_Msk (0x3ul << CLK_CLKSEL1_ADCSEL_Pos)
#define | CLK_CLKSEL1_SPISEL_Pos (4)
#define | CLK_CLKSEL1_SPISEL_Msk (0x1ul << CLK_CLKSEL1_SPISEL_Pos)
#define | CLK_CLKSEL1_TMR0SEL_Pos (8)
#define | CLK_CLKSEL1_TMR0SEL_Msk (0x7ul << CLK_CLKSEL1_TMR0SEL_Pos)
#define | CLK_CLKSEL1_TMR1SEL_Pos (12)
#define | CLK_CLKSEL1_TMR1SEL_Msk (0x7ul << CLK_CLKSEL1_TMR1SEL_Pos)
#define | CLK_CLKSEL1_UART0SEL_Pos (24)
#define | CLK_CLKSEL1_UART0SEL_Msk (0x3ul << CLK_CLKSEL1_UART0SEL_Pos)
#define | CLK_CLKSEL1_UART1SEL_Pos (26)
#define | CLK_CLKSEL1_UART1SEL_Msk (0x3ul << CLK_CLKSEL1_UART1SEL_Pos)
#define | CLK_CLKDIV_HCLKDIV_Pos (0)
#define | CLK_CLKDIV_HCLKDIV_Msk (0xful << CLK_CLKDIV_HCLKDIV_Pos)
#define | CLK_CLKDIV_UART0DIV_Pos (8)
#define | CLK_CLKDIV_UART0DIV_Msk (0xful << CLK_CLKDIV_UART0DIV_Pos)
#define | CLK_CLKDIV_UART1DIV_Pos (12)
#define | CLK_CLKDIV_UART1DIV_Msk (0xful << CLK_CLKDIV_UART1DIV_Pos)
#define | CLK_CLKDIV_ADCDIV_Pos (16)
#define | CLK_CLKDIV_ADCDIV_Msk (0xfful << CLK_CLKDIV_ADCDIV_Pos)
#define | CLK_CLKSEL2_FDIVSEL_Pos (2)
#define | CLK_CLKSEL2_FDIVSEL_Msk (0x3ul << CLK_CLKSEL2_FDIVSEL_Pos)
#define | CLK_CLKOCTL_FSEL_Pos (0)
#define | CLK_CLKOCTL_FSEL_Msk (0xful << CLK_CLKOCTL_FSEL_Pos)
#define | CLK_CLKOCTL_CLKOEN_Pos (4)
#define | CLK_CLKOCTL_CLKOEN_Msk (0x1ul << CLK_CLKOCTL_CLKOEN_Pos)
#define | CLK_CLKOCTL_DIV1EN_Pos (5)
#define | CLK_CLKOCTL_DIV1EN_Msk (0x1ul << CLK_CLKOCTL_DIV1EN_Pos)

## Detailed Description

This file defines all structures and symbols for Mini55:

- interrupt numbers
- registers and bit fields
- peripheral base address
- peripheral ID
- Peripheral definitions

## Macro Definition Documentation

## ◆ CLK_AHBCLK_HDIVCKEN_Msk

#define CLK_AHBCLK_HDIVCKEN_Msk (0x1ul << CLK_AHBCLK_HDIVCKEN_Pos)

CLK_T::AHBCLK: HDIVCKEN Mask

Definition at line 1160 of file Mini55Series.h.

## ◆ CLK_AHBCLK_HDIVCKEN_Pos

#define CLK_AHBCLK_HDIVCKEN_Pos (4)

CLK_T::AHBCLK: HDIVCKEN Position

Definition at line 1159 of file Mini55Series.h.

## ◆ CLK_AHBCLK_ISPCKEN_Msk

#define CLK_AHBCLK_ISPCKEN_Msk (0x1ul << CLK_AHBCLK_ISPCKEN_Pos)

CLK_T::AHBCLK: ISPCKEN Mask

Definition at line 1157 of file Mini55Series.h.

## ◆ CLK_AHBCLK_ISPCKEN_Pos

#define CLK_AHBCLK_ISPCKEN_Pos (2)

CLK_T::AHBCLK: ISPCKEN Position

Definition at line 1156 of file Mini55Series.h.

## ◆ CLK_APBCLK_ACMPCKEN_Msk

#define CLK_APBCLK_ACMPCKEN_Msk (0x1ul << CLK_APBCLK_ACMPCKEN_Pos)

CLK_T::APBCLK: ACMPCKEN Mask

Definition at line 1199 of file Mini55Series.h.

## ◆ CLK_APBCLK_ACMPCKEN_Pos

#define CLK_APBCLK_ACMPCKEN_Pos (30)

CLK_T::APBCLK: ACMPCKEN Position

Definition at line 1198 of file Mini55Series.h.

## ◆ CLK_APBCLK_ADCCKEN_Msk

#define CLK_APBCLK_ADCCKEN_Msk (0x1ul << CLK_APBCLK_ADCCKEN_Pos)

CLK_T::APBCLK: ADCCKEN Mask

Definition at line 1196 of file Mini55Series.h.

## ◆ CLK_APBCLK_ADCCKEN_Pos

#define CLK_APBCLK_ADCCKEN_Pos (28)

CLK_T::APBCLK: ADCCKEN Position

Definition at line 1195 of file Mini55Series.h.

## ◆ CLK_APBCLK_CLKOCKEN_Msk

#define CLK_APBCLK_CLKOCKEN_Msk (0x1ul << CLK_APBCLK_CLKOCKEN_Pos)

CLK_T::APBCLK: CLKOCKEN Mask

Definition at line 1172 of file Mini55Series.h.

## ◆ CLK_APBCLK_CLKOCKEN_Pos

#define CLK_APBCLK_CLKOCKEN_Pos (6)

CLK_T::APBCLK: CLKOCKEN Position

Definition at line 1171 of file Mini55Series.h.

## ◆ CLK_APBCLK_I2CCKEN_Msk

#define CLK_APBCLK_I2CCKEN_Msk (0x1ul << CLK_APBCLK_I2CCKEN_Pos)

CLK_T::APBCLK: I2CCKEN Mask

Definition at line 1175 of file Mini55Series.h.

## ◆ CLK_APBCLK_I2CCKEN_Pos

#define CLK_APBCLK_I2CCKEN_Pos (8)

CLK_T::APBCLK: I2CCKEN Position

Definition at line 1174 of file Mini55Series.h.

## ◆ CLK_APBCLK_PWMCH01CKEN_Msk

#define CLK_APBCLK_PWMCH01CKEN_Msk (0x1ul << CLK_APBCLK_PWMCH01CKEN_Pos)

CLK_T::APBCLK: PWMCH01CKEN Mask

Definition at line 1187 of file Mini55Series.h.

## ◆ CLK_APBCLK_PWMCH01CKEN_Pos

#define CLK_APBCLK_PWMCH01CKEN_Pos (20)

CLK_T::APBCLK: PWMCH01CKEN Position

Definition at line 1186 of file Mini55Series.h.

## ◆ CLK_APBCLK_PWMCH23CKEN_Msk

#define CLK_APBCLK_PWMCH23CKEN_Msk (0x1ul << CLK_APBCLK_PWMCH23CKEN_Pos)

CLK_T::APBCLK: PWMCH23CKEN Mask

Definition at line 1190 of file Mini55Series.h.

## ◆ CLK_APBCLK_PWMCH23CKEN_Pos

#define CLK_APBCLK_PWMCH23CKEN_Pos (21)

CLK_T::APBCLK: PWMCH23CKEN Position

Definition at line 1189 of file Mini55Series.h.

## ◆ CLK_APBCLK_PWMCH45CKEN_Msk

#define CLK_APBCLK_PWMCH45CKEN_Msk (0x1ul << CLK_APBCLK_PWMCH45CKEN_Pos)

CLK_T::APBCLK: PWMCH45CKEN Mask

Definition at line 1193 of file Mini55Series.h.

## ◆ CLK_APBCLK_PWMCH45CKEN_Pos

#define CLK_APBCLK_PWMCH45CKEN_Pos (22)

CLK_T::APBCLK: PWMCH45CKEN Position

Definition at line 1192 of file Mini55Series.h.

## ◆ CLK_APBCLK_SPICKEN_Msk

#define CLK_APBCLK_SPICKEN_Msk (0x1ul << CLK_APBCLK_SPICKEN_Pos)

CLK_T::APBCLK: SPICKEN Mask

Definition at line 1178 of file Mini55Series.h.

## ◆ CLK_APBCLK_SPICKEN_Pos

#define CLK_APBCLK_SPICKEN_Pos (12)

CLK_T::APBCLK: SPICKEN Position

Definition at line 1177 of file Mini55Series.h.

## ◆ CLK_APBCLK_TMR0CKEN_Msk

#define CLK_APBCLK_TMR0CKEN_Msk (0x1ul << CLK_APBCLK_TMR0CKEN_Pos)

CLK_T::APBCLK: TMR0CKEN Mask

Definition at line 1166 of file Mini55Series.h.

## ◆ CLK_APBCLK_TMR0CKEN_Pos

#define CLK_APBCLK_TMR0CKEN_Pos (2)

CLK_T::APBCLK: TMR0CKEN Position

Definition at line 1165 of file Mini55Series.h.

## ◆ CLK_APBCLK_TMR1CKEN_Msk

#define CLK_APBCLK_TMR1CKEN_Msk (0x1ul << CLK_APBCLK_TMR1CKEN_Pos)

CLK_T::APBCLK: TMR1CKEN Mask

Definition at line 1169 of file Mini55Series.h.

## ◆ CLK_APBCLK_TMR1CKEN_Pos

#define CLK_APBCLK_TMR1CKEN_Pos (3)

CLK_T::APBCLK: TMR1CKEN Position

Definition at line 1168 of file Mini55Series.h.

## ◆ CLK_APBCLK_UART0CKEN_Msk

#define CLK_APBCLK_UART0CKEN_Msk (0x1ul << CLK_APBCLK_UART0CKEN_Pos)

CLK_T::APBCLK: UART0CKEN Mask

Definition at line 1181 of file Mini55Series.h.

## ◆ CLK_APBCLK_UART0CKEN_Pos

#define CLK_APBCLK_UART0CKEN_Pos (16)

CLK_T::APBCLK: UART0CKEN Position

Definition at line 1180 of file Mini55Series.h.

## ◆ CLK_APBCLK_UART1CKEN_Msk

#define CLK_APBCLK_UART1CKEN_Msk (0x1ul << CLK_APBCLK_UART1CKEN_Pos)

CLK_T::APBCLK: UART1CKEN Mask

Definition at line 1184 of file Mini55Series.h.

## ◆ CLK_APBCLK_UART1CKEN_Pos

#define CLK_APBCLK_UART1CKEN_Pos (17)

CLK_T::APBCLK: UART1CKEN Position

Definition at line 1183 of file Mini55Series.h.

## ◆ CLK_APBCLK_WDTCKEN_Msk

#define CLK_APBCLK_WDTCKEN_Msk (0x1ul << CLK_APBCLK_WDTCKEN_Pos)

CLK_T::APBCLK: WDTCKEN Mask

Definition at line 1163 of file Mini55Series.h.

## ◆ CLK_APBCLK_WDTCKEN_Pos

#define CLK_APBCLK_WDTCKEN_Pos (0)

CLK_T::APBCLK: WDTCKEN Position

Definition at line 1162 of file Mini55Series.h.

## ◆ CLK_CLKDIV_ADCDIV_Msk

#define CLK_CLKDIV_ADCDIV_Msk (0xfful << CLK_CLKDIV_ADCDIV_Pos)

CLK_T::CLKDIV: ADCDIV Mask

Definition at line 1250 of file Mini55Series.h.

## ◆ CLK_CLKDIV_ADCDIV_Pos

#define CLK_CLKDIV_ADCDIV_Pos (16)

CLK_T::CLKDIV: ADCDIV Position

Definition at line 1249 of file Mini55Series.h.

## ◆ CLK_CLKDIV_HCLKDIV_Msk

#define CLK_CLKDIV_HCLKDIV_Msk (0xful << CLK_CLKDIV_HCLKDIV_Pos)

CLK_T::CLKDIV: HCLKDIV Mask

Definition at line 1241 of file Mini55Series.h.

## ◆ CLK_CLKDIV_HCLKDIV_Pos

#define CLK_CLKDIV_HCLKDIV_Pos (0)

CLK_T::CLKDIV: HCLKDIV Position

Definition at line 1240 of file Mini55Series.h.

## ◆ CLK_CLKDIV_UART0DIV_Msk

#define CLK_CLKDIV_UART0DIV_Msk (0xful << CLK_CLKDIV_UART0DIV_Pos)

CLK_T::CLKDIV: UART0DIV Mask

Definition at line 1244 of file Mini55Series.h.

## ◆ CLK_CLKDIV_UART0DIV_Pos

#define CLK_CLKDIV_UART0DIV_Pos (8)

CLK_T::CLKDIV: UART0DIV Position

Definition at line 1243 of file Mini55Series.h.

## ◆ CLK_CLKDIV_UART1DIV_Msk

#define CLK_CLKDIV_UART1DIV_Msk (0xful << CLK_CLKDIV_UART1DIV_Pos)

CLK_T::CLKDIV: UART1DIV Mask

Definition at line 1247 of file Mini55Series.h.

## ◆ CLK_CLKDIV_UART1DIV_Pos

#define CLK_CLKDIV_UART1DIV_Pos (12)

CLK_T::CLKDIV: UART1DIV Position

Definition at line 1246 of file Mini55Series.h.

## ◆ CLK_CLKOCTL_CLKOEN_Msk

#define CLK_CLKOCTL_CLKOEN_Msk (0x1ul << CLK_CLKOCTL_CLKOEN_Pos)

CLK_T::CLKOCTL: CLKOEN Mask

Definition at line 1259 of file Mini55Series.h.

## ◆ CLK_CLKOCTL_CLKOEN_Pos

#define CLK_CLKOCTL_CLKOEN_Pos (4)

CLK_T::CLKOCTL: CLKOEN Position

Definition at line 1258 of file Mini55Series.h.

## ◆ CLK_CLKOCTL_DIV1EN_Msk

#define CLK_CLKOCTL_DIV1EN_Msk (0x1ul << CLK_CLKOCTL_DIV1EN_Pos)

CLK_T::CLKOCTL: DIV1EN Mask

Definition at line 1262 of file Mini55Series.h.

## ◆ CLK_CLKOCTL_DIV1EN_Pos

#define CLK_CLKOCTL_DIV1EN_Pos (5)

CLK_T::CLKOCTL: DIV1EN Position

Definition at line 1261 of file Mini55Series.h.

## ◆ CLK_CLKOCTL_FSEL_Msk

#define CLK_CLKOCTL_FSEL_Msk (0xful << CLK_CLKOCTL_FSEL_Pos)

CLK_T::CLKOCTL: FSEL Mask

Definition at line 1256 of file Mini55Series.h.

## ◆ CLK_CLKOCTL_FSEL_Pos

#define CLK_CLKOCTL_FSEL_Pos (0)

CLK_T::CLKOCTL: FSEL Position

Definition at line 1255 of file Mini55Series.h.

## ◆ CLK_CLKSEL0_HCLKSEL_Msk

#define CLK_CLKSEL0_HCLKSEL_Msk (0x7ul << CLK_CLKSEL0_HCLKSEL_Pos)

CLK_T::CLKSEL0: HCLKSEL Mask

Definition at line 1214 of file Mini55Series.h.

## ◆ CLK_CLKSEL0_HCLKSEL_Pos

#define CLK_CLKSEL0_HCLKSEL_Pos (0)

CLK_T::CLKSEL0: HCLKSEL Position

Definition at line 1213 of file Mini55Series.h.

## ◆ CLK_CLKSEL0_STCLKSEL_Msk

#define CLK_CLKSEL0_STCLKSEL_Msk (0x7ul << CLK_CLKSEL0_STCLKSEL_Pos)

CLK_T::CLKSEL0: STCLKSEL Mask

Definition at line 1217 of file Mini55Series.h.

## ◆ CLK_CLKSEL0_STCLKSEL_Pos

#define CLK_CLKSEL0_STCLKSEL_Pos (3)

CLK_T::CLKSEL0: STCLKSEL Position

Definition at line 1216 of file Mini55Series.h.

## ◆ CLK_CLKSEL1_ADCSEL_Msk

#define CLK_CLKSEL1_ADCSEL_Msk (0x3ul << CLK_CLKSEL1_ADCSEL_Pos)

CLK_T::CLKSEL1: ADCSEL Mask

Definition at line 1223 of file Mini55Series.h.

## ◆ CLK_CLKSEL1_ADCSEL_Pos

#define CLK_CLKSEL1_ADCSEL_Pos (2)

CLK_T::CLKSEL1: ADCSEL Position

Definition at line 1222 of file Mini55Series.h.

## ◆ CLK_CLKSEL1_SPISEL_Msk

#define CLK_CLKSEL1_SPISEL_Msk (0x1ul << CLK_CLKSEL1_SPISEL_Pos)

CLK_T::CLKSEL1: SPISEL Mask

Definition at line 1226 of file Mini55Series.h.

## ◆ CLK_CLKSEL1_SPISEL_Pos

#define CLK_CLKSEL1_SPISEL_Pos (4)

CLK_T::CLKSEL1: SPISEL Position

Definition at line 1225 of file Mini55Series.h.

## ◆ CLK_CLKSEL1_TMR0SEL_Msk

#define CLK_CLKSEL1_TMR0SEL_Msk (0x7ul << CLK_CLKSEL1_TMR0SEL_Pos)

CLK_T::CLKSEL1: TMR0SEL Mask

Definition at line 1229 of file Mini55Series.h.

## ◆ CLK_CLKSEL1_TMR0SEL_Pos

#define CLK_CLKSEL1_TMR0SEL_Pos (8)

CLK_T::CLKSEL1: TMR0SEL Position

Definition at line 1228 of file Mini55Series.h.

## ◆ CLK_CLKSEL1_TMR1SEL_Msk

#define CLK_CLKSEL1_TMR1SEL_Msk (0x7ul << CLK_CLKSEL1_TMR1SEL_Pos)

CLK_T::CLKSEL1: TMR1SEL Mask

Definition at line 1232 of file Mini55Series.h.

## ◆ CLK_CLKSEL1_TMR1SEL_Pos

#define CLK_CLKSEL1_TMR1SEL_Pos (12)

CLK_T::CLKSEL1: TMR1SEL Position

Definition at line 1231 of file Mini55Series.h.

## ◆ CLK_CLKSEL1_UART0SEL_Msk

#define CLK_CLKSEL1_UART0SEL_Msk (0x3ul << CLK_CLKSEL1_UART0SEL_Pos)

CLK_T::CLKSEL1: UART0SEL Mask

Definition at line 1235 of file Mini55Series.h.

## ◆ CLK_CLKSEL1_UART0SEL_Pos

#define CLK_CLKSEL1_UART0SEL_Pos (24)

CLK_T::CLKSEL1: UART0SEL Position

Definition at line 1234 of file Mini55Series.h.

## ◆ CLK_CLKSEL1_UART1SEL_Msk

#define CLK_CLKSEL1_UART1SEL_Msk (0x3ul << CLK_CLKSEL1_UART1SEL_Pos)

CLK_T::CLKSEL1: UART1SEL Mask

Definition at line 1238 of file Mini55Series.h.

## ◆ CLK_CLKSEL1_UART1SEL_Pos

#define CLK_CLKSEL1_UART1SEL_Pos (26)

CLK_T::CLKSEL1: UART1SEL Position

Definition at line 1237 of file Mini55Series.h.

## ◆ CLK_CLKSEL1_WDTSEL_Msk

#define CLK_CLKSEL1_WDTSEL_Msk (0x3ul << CLK_CLKSEL1_WDTSEL_Pos)

CLK_T::CLKSEL1: WDTSEL Mask

Definition at line 1220 of file Mini55Series.h.

## ◆ CLK_CLKSEL1_WDTSEL_Pos

#define CLK_CLKSEL1_WDTSEL_Pos (0)

CLK_T::CLKSEL1: WDTSEL Position

Definition at line 1219 of file Mini55Series.h.

## ◆ CLK_CLKSEL2_FDIVSEL_Msk

#define CLK_CLKSEL2_FDIVSEL_Msk (0x3ul << CLK_CLKSEL2_FDIVSEL_Pos)

CLK_T::CLKSEL2: FDIVSEL Mask

Definition at line 1253 of file Mini55Series.h.

## ◆ CLK_CLKSEL2_FDIVSEL_Pos

#define CLK_CLKSEL2_FDIVSEL_Pos (2)

CLK_T::CLKSEL2: FDIVSEL Position

Definition at line 1252 of file Mini55Series.h.

## ◆ CLK_PWRCTL_HIRCEN_Msk

#define CLK_PWRCTL_HIRCEN_Msk (0x1ul << CLK_PWRCTL_HIRCEN_Pos)

CLK_T::PWRCTL: HIRCEN Mask

Definition at line 1133 of file Mini55Series.h.

## ◆ CLK_PWRCTL_HIRCEN_Pos

#define CLK_PWRCTL_HIRCEN_Pos (2)

CLK_T::PWRCTL: HIRCEN Position

Definition at line 1132 of file Mini55Series.h.

## ◆ CLK_PWRCTL_HXTGAIN_Msk

#define CLK_PWRCTL_HXTGAIN_Msk (0x3ul << CLK_PWRCTL_HXTGAIN_Pos)

CLK_T::PWRCTL: HXTGAIN Mask

Definition at line 1154 of file Mini55Series.h.

## ◆ CLK_PWRCTL_HXTGAIN_Pos

#define CLK_PWRCTL_HXTGAIN_Pos (10)

CLK_T::PWRCTL: HXTGAIN Position

Definition at line 1153 of file Mini55Series.h.

## ◆ CLK_PWRCTL_LIRCEN_Msk

#define CLK_PWRCTL_LIRCEN_Msk (0x1ul << CLK_PWRCTL_LIRCEN_Pos)

CLK_T::PWRCTL: LIRCEN Mask

Definition at line 1136 of file Mini55Series.h.

## ◆ CLK_PWRCTL_LIRCEN_Pos

#define CLK_PWRCTL_LIRCEN_Pos (3)

CLK_T::PWRCTL: LIRCEN Position

Definition at line 1135 of file Mini55Series.h.

## ◆ CLK_PWRCTL_PDEN_Msk

#define CLK_PWRCTL_PDEN_Msk (0x1ul << CLK_PWRCTL_PDEN_Pos)

CLK_T::PWRCTL: PDEN Mask

Definition at line 1148 of file Mini55Series.h.

## ◆ CLK_PWRCTL_PDEN_Pos

#define CLK_PWRCTL_PDEN_Pos (7)

CLK_T::PWRCTL: PDEN Position

Definition at line 1147 of file Mini55Series.h.

## ◆ CLK_PWRCTL_PDLXT_Msk

#define CLK_PWRCTL_PDLXT_Msk (0x1ul << CLK_PWRCTL_PDLXT_Pos)

CLK_T::PWRCTL: PDLXT Mask

Definition at line 1151 of file Mini55Series.h.

## ◆ CLK_PWRCTL_PDLXT_Pos

#define CLK_PWRCTL_PDLXT_Pos (9)

CLK_T::PWRCTL: PDLXT Position

Definition at line 1150 of file Mini55Series.h.

## ◆ CLK_PWRCTL_PDWKDLY_Msk

#define CLK_PWRCTL_PDWKDLY_Msk (0x1ul << CLK_PWRCTL_PDWKDLY_Pos)

CLK_T::PWRCTL: PDWKDLY Mask

Definition at line 1139 of file Mini55Series.h.

## ◆ CLK_PWRCTL_PDWKDLY_Pos

#define CLK_PWRCTL_PDWKDLY_Pos (4)

CLK_T::PWRCTL: PDWKDLY Position

Definition at line 1138 of file Mini55Series.h.

## ◆ CLK_PWRCTL_PDWKIEN_Msk

#define CLK_PWRCTL_PDWKIEN_Msk (0x1ul << CLK_PWRCTL_PDWKIEN_Pos)

CLK_T::PWRCTL: PDWKIEN Mask

Definition at line 1142 of file Mini55Series.h.

## ◆ CLK_PWRCTL_PDWKIEN_Pos

#define CLK_PWRCTL_PDWKIEN_Pos (5)

CLK_T::PWRCTL: PDWKIEN Position

Definition at line 1141 of file Mini55Series.h.

## ◆ CLK_PWRCTL_PDWKIF_Msk

#define CLK_PWRCTL_PDWKIF_Msk (0x1ul << CLK_PWRCTL_PDWKIF_Pos)

CLK_T::PWRCTL: PDWKIF Mask

Definition at line 1145 of file Mini55Series.h.

## ◆ CLK_PWRCTL_PDWKIF_Pos

#define CLK_PWRCTL_PDWKIF_Pos (6)

CLK_T::PWRCTL: PDWKIF Position

Definition at line 1144 of file Mini55Series.h.

## ◆ CLK_PWRCTL_XTLEN_Msk

#define CLK_PWRCTL_XTLEN_Msk (0x3ul << CLK_PWRCTL_XTLEN_Pos)

CLK_T::PWRCTL: XTLEN Mask

Definition at line 1130 of file Mini55Series.h.

## ◆ CLK_PWRCTL_XTLEN_Pos

#define CLK_PWRCTL_XTLEN_Pos (0)

    @addtogroup CLK_CONST CLK Bit Field Definition
    Constant Definitions for CLK Controller

CLK_T::PWRCTL: XTLEN Position

Definition at line 1129 of file Mini55Series.h.

## ◆ CLK_STATUS_CLKSFAIL_Msk

#define CLK_STATUS_CLKSFAIL_Msk (0x1ul << CLK_STATUS_CLKSFAIL_Pos)

CLK_T::STATUS: CLKSFAIL Mask

Definition at line 1211 of file Mini55Series.h.

## ◆ CLK_STATUS_CLKSFAIL_Pos

#define CLK_STATUS_CLKSFAIL_Pos (7)

CLK_T::STATUS: CLKSFAIL Position

Definition at line 1210 of file Mini55Series.h.

## ◆ CLK_STATUS_HIRCSTB_Msk

#define CLK_STATUS_HIRCSTB_Msk (0x1ul << CLK_STATUS_HIRCSTB_Pos)

CLK_T::STATUS: HIRCSTB Mask

Definition at line 1208 of file Mini55Series.h.

## ◆ CLK_STATUS_HIRCSTB_Pos

#define CLK_STATUS_HIRCSTB_Pos (4)

CLK_T::STATUS: HIRCSTB Position

Definition at line 1207 of file Mini55Series.h.

## ◆ CLK_STATUS_LIRCSTB_Msk

#define CLK_STATUS_LIRCSTB_Msk (0x1ul << CLK_STATUS_LIRCSTB_Pos)

CLK_T::STATUS: LIRCSTB Mask

Definition at line 1205 of file Mini55Series.h.

## ◆ CLK_STATUS_LIRCSTB_Pos

#define CLK_STATUS_LIRCSTB_Pos (3)

CLK_T::STATUS: LIRCSTB Position

Definition at line 1204 of file Mini55Series.h.

## ◆ CLK_STATUS_XTLSTB_Msk

#define CLK_STATUS_XTLSTB_Msk (0x1ul << CLK_STATUS_XTLSTB_Pos)

CLK_T::STATUS: XTLSTB Mask

Definition at line 1202 of file Mini55Series.h.

## ◆ CLK_STATUS_XTLSTB_Pos

#define CLK_STATUS_XTLSTB_Pos (0)

CLK_T::STATUS: XTLSTB Position

Definition at line 1201 of file Mini55Series.h.