| NUC029FAE_BSP V3.02.000 The Board Support Package for NUC029FAE MCU

Data Fields
NVIC_Type Struct Reference
Defines and Type Definitions » Status and Control Registers » Nested Vectored Interrupt Controller (NVIC)

Structure type to access the Nested Vectored Interrupt Controller (NVIC). More...

`#include <core_cm0.h>`

## Data Fields
__IOM uint32_t | ISER [1U]
uint32_t | RESERVED0 [31U]
__IOM uint32_t | ICER [1U]
uint32_t | RSERVED1 [31U]
__IOM uint32_t | ISPR [1U]
uint32_t | RESERVED2 [31U]
__IOM uint32_t | ICPR [1U]
uint32_t | RESERVED3 [31U]
uint32_t | RESERVED4 [64U]
__IOM uint32_t | IP [8U]

## Detailed Description

Structure type to access the Nested Vectored Interrupt Controller (NVIC).

Definition at line 362 of file core_cm0.h.

The documentation for this struct was generated from the following file:

- CMSIS/Include/core_cm0.h