| NANO100_BSP V3.05.000 The Board Support Package for Nano100BN Series

Modules | Macros
DAC Exported Constants
NANO100 Device Driver » DAC Driver
Collaboration diagram for DAC Exported Constants:

## Modules
| DAC Exported Functions

## Macros
#define | DAC_WRITE_DAT_TRIGGER
| Write DACx_DAT trigger. More...
#define | DAC_PDMA_TRIGGER
| PDMA trigger. More...
#define | DAC_TIMER0_TRIGGER
| Timer 0 trigger. More...
#define | DAC_TIMER1_TRIGGER
| Timer 1 trigger. More...
#define | DAC_TIMER2_TRIGGER
| Timer 2 trigger. More...
#define | DAC_TIMER3_TRIGGER
| Timer 3 trigger. More...
#define | DAC_REFSEL_POWER
| DAC reference voltage source selection set to power. More...
#define | DAC_REFSEL_INT_VREF
| DAC reference voltage source selection set to Int_VREF. More...
#define | DAC_REFSEL_VREF
| DAC reference voltage source selection set to VREF. More...

## Detailed Description

## Macro Definition Documentation

## ◆ DAC_PDMA_TRIGGER

#define DAC_PDMA_TRIGGER

PDMA trigger.

Definition at line 34 of file dac.h.

## ◆ DAC_REFSEL_INT_VREF

#define DAC_REFSEL_INT_VREF

DAC reference voltage source selection set to Int_VREF.

Definition at line 41 of file dac.h.

## ◆ DAC_REFSEL_POWER

#define DAC_REFSEL_POWER

DAC reference voltage source selection set to power.

Definition at line 40 of file dac.h.

## ◆ DAC_REFSEL_VREF

#define DAC_REFSEL_VREF

DAC reference voltage source selection set to VREF.

Definition at line 42 of file dac.h.

## ◆ DAC_TIMER0_TRIGGER

#define DAC_TIMER0_TRIGGER

Timer 0 trigger.

Definition at line 35 of file dac.h.

## ◆ DAC_TIMER1_TRIGGER

#define DAC_TIMER1_TRIGGER

Timer 1 trigger.

Definition at line 36 of file dac.h.

## ◆ DAC_TIMER2_TRIGGER

#define DAC_TIMER2_TRIGGER

Timer 2 trigger.

Definition at line 37 of file dac.h.

## ◆ DAC_TIMER3_TRIGGER

#define DAC_TIMER3_TRIGGER

Timer 3 trigger.

Definition at line 38 of file dac.h.

## ◆ DAC_WRITE_DAT_TRIGGER

#define DAC_WRITE_DAT_TRIGGER

Write DACx_DAT trigger.

Definition at line 33 of file dac.h.