| Nano102_112 Series BSP V3.03.002 The Board Support Package for Nano102_112 Series

Modules | Data Structures
NANO102/112 Definitions

## Modules
| Device CMSIS Definitions
| NANO102/112 Peripherals

## Data Structures
struct | ADC_T
#define | ADC_RESULT_RSLT_Pos (0)
#define | ADC_RESULT_RSLT_Msk (0xffful << ADC_RESULT_RSLT_Pos)
#define | ADC_RESULT_VALID_Pos (16)
#define | ADC_RESULT_VALID_Msk (0x1ul << ADC_RESULT_VALID_Pos)
#define | ADC_RESULT_OVERRUN_Pos (17)
#define | ADC_RESULT_OVERRUN_Msk (0x1ul << ADC_RESULT_OVERRUN_Pos)
#define | ADC_CR_ADEN_Pos (0)
#define | ADC_CR_ADEN_Msk (0x1ul << ADC_CR_ADEN_Pos)
#define | ADC_CR_ADIE_Pos (1)
#define | ADC_CR_ADIE_Msk (0x1ul << ADC_CR_ADIE_Pos)
#define | ADC_CR_ADMD_Pos (2)
#define | ADC_CR_ADMD_Msk (0x3ul << ADC_CR_ADMD_Pos)
#define | ADC_CR_TRGS_Pos (4)
#define | ADC_CR_TRGS_Msk (0x3ul << ADC_CR_TRGS_Pos)
#define | ADC_CR_TRGCOND_Pos (6)
#define | ADC_CR_TRGCOND_Msk (0x3ul << ADC_CR_TRGCOND_Pos)
#define | ADC_CR_TRGE_Pos (8)
#define | ADC_CR_TRGE_Msk (0x1ul << ADC_CR_TRGE_Pos)
#define | ADC_CR_PTEN_Pos (9)
#define | ADC_CR_PTEN_Msk (0x1ul << ADC_CR_PTEN_Pos)
#define | ADC_CR_DIFF_Pos (10)
#define | ADC_CR_DIFF_Msk (0x1ul << ADC_CR_DIFF_Pos)
#define | ADC_CR_ADST_Pos (11)
#define | ADC_CR_ADST_Msk (0x1ul << ADC_CR_ADST_Pos)
#define | ADC_CR_TMSEL_Pos (12)
#define | ADC_CR_TMSEL_Msk (0x3ul << ADC_CR_TMSEL_Pos)
#define | ADC_CR_TMTRGMOD_Pos (15)
#define | ADC_CR_TMTRGMOD_Msk (0x1ul << ADC_CR_TMTRGMOD_Pos)
#define | ADC_CR_REFSEL_Pos (16)
#define | ADC_CR_REFSEL_Msk (0x3ul << ADC_CR_REFSEL_Pos)
#define | ADC_CR_RESSEL_Pos (18)
#define | ADC_CR_RESSEL_Msk (0x3ul << ADC_CR_RESSEL_Pos)
#define | ADC_CR_TMPDMACNT_Pos (24)
#define | ADC_CR_TMPDMACNT_Msk (0xfful << ADC_CR_TMPDMACNT_Pos)
#define | ADC_CHEN_CHEN0_Pos (0)
#define | ADC_CHEN_CHEN0_Msk (0x1ul << ADC_CHEN_CHEN0_Pos)
#define | ADC_CMPR_CMPEN_Pos (0)
#define | ADC_CMPR_CMPEN_Msk (0x1ul << ADC_CMPR_CMPEN_Pos)
#define | ADC_CMPR_CMPIE_Pos (1)
#define | ADC_CMPR_CMPIE_Msk (0x1ul << ADC_CMPR_CMPIE_Pos)
#define | ADC_CMPR_CMPCOND_Pos (2)
#define | ADC_CMPR_CMPCOND_Msk (0x1ul << ADC_CMPR_CMPCOND_Pos)
#define | ADC_CMPR_CMPCH_Pos (3)
#define | ADC_CMPR_CMPCH_Msk (0x1ful << ADC_CMPR_CMPCH_Pos)
#define | ADC_CMPR_CMPMATCNT_Pos (8)
#define | ADC_CMPR_CMPMATCNT_Msk (0xful << ADC_CMPR_CMPMATCNT_Pos)
#define | ADC_CMPR_CMPD_Pos (16)
#define | ADC_CMPR_CMPD_Msk (0xffful << ADC_CMPR_CMPD_Pos)
#define | ADC_SR_ADF_Pos (0)
#define | ADC_SR_ADF_Msk (0x1ul << ADC_SR_ADF_Pos)
#define | ADC_SR_CMPF0_Pos (1)
#define | ADC_SR_CMPF0_Msk (0x1ul << ADC_SR_CMPF0_Pos)
#define | ADC_SR_CMPF1_Pos (2)
#define | ADC_SR_CMPF1_Msk (0x1ul << ADC_SR_CMPF1_Pos)
#define | ADC_SR_BUSY_Pos (3)
#define | ADC_SR_BUSY_Msk (0x1ul << ADC_SR_BUSY_Pos)
#define | ADC_SR_CHANNEL_Pos (4)
#define | ADC_SR_CHANNEL_Msk (0x1ful << ADC_SR_CHANNEL_Pos)
#define | ADC_SR_INITRDY_Pos (16)
#define | ADC_SR_INITRDY_Msk (0x1ul << ADC_SR_INITRDY_Pos)
#define | ADC_PDMA_AD_PDMA_Pos (0)
#define | ADC_PDMA_AD_PDMA_Msk (0xffful << ADC_PDMA_AD_PDMA_Pos)
#define | ADC_PWRCTL_PWUPRDY_Pos (0)
#define | ADC_PWRCTL_PWUPRDY_Msk (0x1ul << ADC_PWRCTL_PWUPRDY_Pos)
#define | ADC_PWRCTL_PWDCALEN_Pos (1)
#define | ADC_PWRCTL_PWDCALEN_Msk (0x1ul << ADC_PWRCTL_PWDCALEN_Pos)
#define | ADC_PWRCTL_PWDMOD_Pos (2)
#define | ADC_PWRCTL_PWDMOD_Msk (0x3ul << ADC_PWRCTL_PWDMOD_Pos)
#define | ADC_CALCTL_CALEN_Pos (0)
#define | ADC_CALCTL_CALEN_Msk (0x1ul << ADC_CALCTL_CALEN_Pos)
#define | ADC_CALCTL_CALSTART_Pos (1)
#define | ADC_CALCTL_CALSTART_Msk (0x1ul << ADC_CALCTL_CALSTART_Pos)
#define | ADC_CALCTL_CALDONE_Pos (2)
#define | ADC_CALCTL_CALDONE_Msk (0x1ul << ADC_CALCTL_CALDONE_Pos)
#define | ADC_CALCTL_CALSEL_Pos (3)
#define | ADC_CALCTL_CALSEL_Msk (0x1ul << ADC_CALCTL_CALSEL_Pos)
#define | ADC_CALWORD_CALWORD_Pos (0)
#define | ADC_CALWORD_CALWORD_Msk (0x7ful << ADC_CALWORD_CALWORD_Pos)
#define | ADC_SMPLCNT0_CH0SAMPCNT_Pos (0)
#define | ADC_SMPLCNT0_CH0SAMPCNT_Msk (0xful << ADC_SMPLCNT0_CH0SAMPCNT_Pos)
#define | ADC_SMPLCNT1_CH8SAMPCNT_Pos (0)
#define | ADC_SMPLCNT1_CH8SAMPCNT_Msk (0xful << ADC_SMPLCNT1_CH8SAMPCNT_Pos)
#define | ADC_SMPLCNT1_INTCHSAMPCNT_Pos (16)
#define | ADC_SMPLCNT1_INTCHSAMPCNT_Msk (0xful << ADC_SMPLCNT1_INTCHSAMPCNT_Pos)

## Detailed Description

This file defines all structures and symbols for NANO102/112:

- interrupt numbers
- registers and bit fields
- peripheral base address
- peripheral ID
- Peripheral definitions

## Macro Definition Documentation

## ◆ ADC_CALCTL_CALDONE_Msk

#define ADC_CALCTL_CALDONE_Msk (0x1ul << ADC_CALCTL_CALDONE_Pos)

ADC_T::CALCTL: CALDONE Mask

Definition at line 876 of file Nano1X2Series.h.

## ◆ ADC_CALCTL_CALDONE_Pos

#define ADC_CALCTL_CALDONE_Pos (2)

ADC_T::CALCTL: CALDONE Position

Definition at line 875 of file Nano1X2Series.h.

## ◆ ADC_CALCTL_CALEN_Msk

#define ADC_CALCTL_CALEN_Msk (0x1ul << ADC_CALCTL_CALEN_Pos)

ADC_T::CALCTL: CALEN Mask

Definition at line 870 of file Nano1X2Series.h.

## ◆ ADC_CALCTL_CALEN_Pos

#define ADC_CALCTL_CALEN_Pos (0)

ADC_T::CALCTL: CALEN Position

Definition at line 869 of file Nano1X2Series.h.

## ◆ ADC_CALCTL_CALSEL_Msk

#define ADC_CALCTL_CALSEL_Msk (0x1ul << ADC_CALCTL_CALSEL_Pos)

ADC_T::CALCTL: CALSEL Mask

Definition at line 879 of file Nano1X2Series.h.

## ◆ ADC_CALCTL_CALSEL_Pos

#define ADC_CALCTL_CALSEL_Pos (3)

ADC_T::CALCTL: CALSEL Position

Definition at line 878 of file Nano1X2Series.h.

## ◆ ADC_CALCTL_CALSTART_Msk

#define ADC_CALCTL_CALSTART_Msk (0x1ul << ADC_CALCTL_CALSTART_Pos)

ADC_T::CALCTL: CALSTART Mask

Definition at line 873 of file Nano1X2Series.h.

## ◆ ADC_CALCTL_CALSTART_Pos

#define ADC_CALCTL_CALSTART_Pos (1)

ADC_T::CALCTL: CALSTART Position

Definition at line 872 of file Nano1X2Series.h.

## ◆ ADC_CALWORD_CALWORD_Msk

#define ADC_CALWORD_CALWORD_Msk (0x7ful << ADC_CALWORD_CALWORD_Pos)

ADC_T::CALWORD: CALWORD Mask

Definition at line 882 of file Nano1X2Series.h.

## ◆ ADC_CALWORD_CALWORD_Pos

#define ADC_CALWORD_CALWORD_Pos (0)

ADC_T::CALWORD: CALWORD Position

Definition at line 881 of file Nano1X2Series.h.

## ◆ ADC_CHEN_CHEN0_Msk

#define ADC_CHEN_CHEN0_Msk (0x1ul << ADC_CHEN_CHEN0_Pos)

ADC_T::CHEN: CHEN0 Mask

Definition at line 819 of file Nano1X2Series.h.

## ◆ ADC_CHEN_CHEN0_Pos

#define ADC_CHEN_CHEN0_Pos (0)

ADC_T::CHEN: CHEN0 Position

Definition at line 818 of file Nano1X2Series.h.

## ◆ ADC_CMPR_CMPCH_Msk

#define ADC_CMPR_CMPCH_Msk (0x1ful << ADC_CMPR_CMPCH_Pos)

ADC_T::CMPR: CMPCH Mask

Definition at line 831 of file Nano1X2Series.h.

## ◆ ADC_CMPR_CMPCH_Pos

#define ADC_CMPR_CMPCH_Pos (3)

ADC_T::CMPR: CMPCH Position

Definition at line 830 of file Nano1X2Series.h.

## ◆ ADC_CMPR_CMPCOND_Msk

#define ADC_CMPR_CMPCOND_Msk (0x1ul << ADC_CMPR_CMPCOND_Pos)

ADC_T::CMPR: CMPCOND Mask

Definition at line 828 of file Nano1X2Series.h.

## ◆ ADC_CMPR_CMPCOND_Pos

#define ADC_CMPR_CMPCOND_Pos (2)

ADC_T::CMPR: CMPCOND Position

Definition at line 827 of file Nano1X2Series.h.

## ◆ ADC_CMPR_CMPD_Msk

#define ADC_CMPR_CMPD_Msk (0xffful << ADC_CMPR_CMPD_Pos)

ADC_T::CMPR: CMPD Mask

Definition at line 837 of file Nano1X2Series.h.

## ◆ ADC_CMPR_CMPD_Pos

#define ADC_CMPR_CMPD_Pos (16)

ADC_T::CMPR: CMPD Position

Definition at line 836 of file Nano1X2Series.h.

## ◆ ADC_CMPR_CMPEN_Msk

#define ADC_CMPR_CMPEN_Msk (0x1ul << ADC_CMPR_CMPEN_Pos)

ADC_T::CMPR: CMPEN Mask

Definition at line 822 of file Nano1X2Series.h.

## ◆ ADC_CMPR_CMPEN_Pos

#define ADC_CMPR_CMPEN_Pos (0)

ADC_T::CMPR: CMPEN Position

Definition at line 821 of file Nano1X2Series.h.

## ◆ ADC_CMPR_CMPIE_Msk

#define ADC_CMPR_CMPIE_Msk (0x1ul << ADC_CMPR_CMPIE_Pos)

ADC_T::CMPR: CMPIE Mask

Definition at line 825 of file Nano1X2Series.h.

## ◆ ADC_CMPR_CMPIE_Pos

#define ADC_CMPR_CMPIE_Pos (1)

ADC_T::CMPR: CMPIE Position

Definition at line 824 of file Nano1X2Series.h.

## ◆ ADC_CMPR_CMPMATCNT_Msk

#define ADC_CMPR_CMPMATCNT_Msk (0xful << ADC_CMPR_CMPMATCNT_Pos)

ADC_T::CMPR: CMPMATCNT Mask

Definition at line 834 of file Nano1X2Series.h.

## ◆ ADC_CMPR_CMPMATCNT_Pos

#define ADC_CMPR_CMPMATCNT_Pos (8)

ADC_T::CMPR: CMPMATCNT Position

Definition at line 833 of file Nano1X2Series.h.

## ◆ ADC_CR_ADEN_Msk

#define ADC_CR_ADEN_Msk (0x1ul << ADC_CR_ADEN_Pos)

ADC_T::CR: ADEN Mask

Definition at line 777 of file Nano1X2Series.h.

## ◆ ADC_CR_ADEN_Pos

#define ADC_CR_ADEN_Pos (0)

ADC_T::CR: ADEN Position

Definition at line 776 of file Nano1X2Series.h.

## ◆ ADC_CR_ADIE_Msk

#define ADC_CR_ADIE_Msk (0x1ul << ADC_CR_ADIE_Pos)

ADC_T::CR: ADIE Mask

Definition at line 780 of file Nano1X2Series.h.

## ◆ ADC_CR_ADIE_Pos

#define ADC_CR_ADIE_Pos (1)

ADC_T::CR: ADIE Position

Definition at line 779 of file Nano1X2Series.h.

## ◆ ADC_CR_ADMD_Msk

#define ADC_CR_ADMD_Msk (0x3ul << ADC_CR_ADMD_Pos)

ADC_T::CR: ADMD Mask

Definition at line 783 of file Nano1X2Series.h.

## ◆ ADC_CR_ADMD_Pos

#define ADC_CR_ADMD_Pos (2)

ADC_T::CR: ADMD Position

Definition at line 782 of file Nano1X2Series.h.

## ◆ ADC_CR_ADST_Msk

#define ADC_CR_ADST_Msk (0x1ul << ADC_CR_ADST_Pos)

ADC_T::CR: ADST Mask

Definition at line 801 of file Nano1X2Series.h.

## ◆ ADC_CR_ADST_Pos

#define ADC_CR_ADST_Pos (11)

ADC_T::CR: ADST Position

Definition at line 800 of file Nano1X2Series.h.

## ◆ ADC_CR_DIFF_Msk

#define ADC_CR_DIFF_Msk (0x1ul << ADC_CR_DIFF_Pos)

ADC_T::CR: DIFF Mask

Definition at line 798 of file Nano1X2Series.h.

## ◆ ADC_CR_DIFF_Pos

#define ADC_CR_DIFF_Pos (10)

ADC_T::CR: DIFF Position

Definition at line 797 of file Nano1X2Series.h.

## ◆ ADC_CR_PTEN_Msk

#define ADC_CR_PTEN_Msk (0x1ul << ADC_CR_PTEN_Pos)

ADC_T::CR: PTEN Mask

Definition at line 795 of file Nano1X2Series.h.

## ◆ ADC_CR_PTEN_Pos

#define ADC_CR_PTEN_Pos (9)

ADC_T::CR: PTEN Position

Definition at line 794 of file Nano1X2Series.h.

## ◆ ADC_CR_REFSEL_Msk

#define ADC_CR_REFSEL_Msk (0x3ul << ADC_CR_REFSEL_Pos)

ADC_T::CR: REFSEL Mask

Definition at line 810 of file Nano1X2Series.h.

## ◆ ADC_CR_REFSEL_Pos

#define ADC_CR_REFSEL_Pos (16)

ADC_T::CR: REFSEL Position

Definition at line 809 of file Nano1X2Series.h.

## ◆ ADC_CR_RESSEL_Msk

#define ADC_CR_RESSEL_Msk (0x3ul << ADC_CR_RESSEL_Pos)

ADC_T::CR: RESSEL Mask

Definition at line 813 of file Nano1X2Series.h.

## ◆ ADC_CR_RESSEL_Pos

#define ADC_CR_RESSEL_Pos (18)

ADC_T::CR: RESSEL Position

Definition at line 812 of file Nano1X2Series.h.

## ◆ ADC_CR_TMPDMACNT_Msk

#define ADC_CR_TMPDMACNT_Msk (0xfful << ADC_CR_TMPDMACNT_Pos)

ADC_T::CR: TMPDMACNT Mask

Definition at line 816 of file Nano1X2Series.h.

## ◆ ADC_CR_TMPDMACNT_Pos

#define ADC_CR_TMPDMACNT_Pos (24)

ADC_T::CR: TMPDMACNT Position

Definition at line 815 of file Nano1X2Series.h.

## ◆ ADC_CR_TMSEL_Msk

#define ADC_CR_TMSEL_Msk (0x3ul << ADC_CR_TMSEL_Pos)

ADC_T::CR: TMSEL Mask

Definition at line 804 of file Nano1X2Series.h.

## ◆ ADC_CR_TMSEL_Pos

#define ADC_CR_TMSEL_Pos (12)

ADC_T::CR: TMSEL Position

Definition at line 803 of file Nano1X2Series.h.

## ◆ ADC_CR_TMTRGMOD_Msk

#define ADC_CR_TMTRGMOD_Msk (0x1ul << ADC_CR_TMTRGMOD_Pos)

ADC_T::CR: TMTRGMOD Mask

Definition at line 807 of file Nano1X2Series.h.

## ◆ ADC_CR_TMTRGMOD_Pos

#define ADC_CR_TMTRGMOD_Pos (15)

ADC_T::CR: TMTRGMOD Position

Definition at line 806 of file Nano1X2Series.h.

## ◆ ADC_CR_TRGCOND_Msk

#define ADC_CR_TRGCOND_Msk (0x3ul << ADC_CR_TRGCOND_Pos)

ADC_T::CR: TRGCOND Mask

Definition at line 789 of file Nano1X2Series.h.

## ◆ ADC_CR_TRGCOND_Pos

#define ADC_CR_TRGCOND_Pos (6)

ADC_T::CR: TRGCOND Position

Definition at line 788 of file Nano1X2Series.h.

## ◆ ADC_CR_TRGE_Msk

#define ADC_CR_TRGE_Msk (0x1ul << ADC_CR_TRGE_Pos)

ADC_T::CR: TRGE Mask

Definition at line 792 of file Nano1X2Series.h.

## ◆ ADC_CR_TRGE_Pos

#define ADC_CR_TRGE_Pos (8)

ADC_T::CR: TRGE Position

Definition at line 791 of file Nano1X2Series.h.

## ◆ ADC_CR_TRGS_Msk

#define ADC_CR_TRGS_Msk (0x3ul << ADC_CR_TRGS_Pos)

ADC_T::CR: TRGS Mask

Definition at line 786 of file Nano1X2Series.h.

## ◆ ADC_CR_TRGS_Pos

#define ADC_CR_TRGS_Pos (4)

ADC_T::CR: TRGS Position

Definition at line 785 of file Nano1X2Series.h.

## ◆ ADC_PDMA_AD_PDMA_Msk

#define ADC_PDMA_AD_PDMA_Msk (0xffful << ADC_PDMA_AD_PDMA_Pos)

ADC_T::PDMA: AD_PDMA Mask

Definition at line 858 of file Nano1X2Series.h.

## ◆ ADC_PDMA_AD_PDMA_Pos

#define ADC_PDMA_AD_PDMA_Pos (0)

ADC_T::PDMA: AD_PDMA Position

Definition at line 857 of file Nano1X2Series.h.

## ◆ ADC_PWRCTL_PWDCALEN_Msk

#define ADC_PWRCTL_PWDCALEN_Msk (0x1ul << ADC_PWRCTL_PWDCALEN_Pos)

ADC_T::PWRCTL: PWDCALEN Mask

Definition at line 864 of file Nano1X2Series.h.

## ◆ ADC_PWRCTL_PWDCALEN_Pos

#define ADC_PWRCTL_PWDCALEN_Pos (1)

ADC_T::PWRCTL: PWDCALEN Position

Definition at line 863 of file Nano1X2Series.h.

## ◆ ADC_PWRCTL_PWDMOD_Msk

#define ADC_PWRCTL_PWDMOD_Msk (0x3ul << ADC_PWRCTL_PWDMOD_Pos)

ADC_T::PWRCTL: PWDMOD Mask

Definition at line 867 of file Nano1X2Series.h.

## ◆ ADC_PWRCTL_PWDMOD_Pos

#define ADC_PWRCTL_PWDMOD_Pos (2)

ADC_T::PWRCTL: PWDMOD Position

Definition at line 866 of file Nano1X2Series.h.

## ◆ ADC_PWRCTL_PWUPRDY_Msk

#define ADC_PWRCTL_PWUPRDY_Msk (0x1ul << ADC_PWRCTL_PWUPRDY_Pos)

ADC_T::PWRCTL: PWUPRDY Mask

Definition at line 861 of file Nano1X2Series.h.

## ◆ ADC_PWRCTL_PWUPRDY_Pos

#define ADC_PWRCTL_PWUPRDY_Pos (0)

ADC_T::PWRCTL: PWUPRDY Position

Definition at line 860 of file Nano1X2Series.h.

## ◆ ADC_RESULT_OVERRUN_Msk

#define ADC_RESULT_OVERRUN_Msk (0x1ul << ADC_RESULT_OVERRUN_Pos)

ADC_T::RESULT: OVERRUN Mask

Definition at line 774 of file Nano1X2Series.h.

## ◆ ADC_RESULT_OVERRUN_Pos

#define ADC_RESULT_OVERRUN_Pos (17)

ADC_T::RESULT: OVERRUN Position

Definition at line 773 of file Nano1X2Series.h.

## ◆ ADC_RESULT_RSLT_Msk

#define ADC_RESULT_RSLT_Msk (0xffful << ADC_RESULT_RSLT_Pos)

ADC_T::RESULT: RSLT Mask

Definition at line 768 of file Nano1X2Series.h.

## ◆ ADC_RESULT_RSLT_Pos

#define ADC_RESULT_RSLT_Pos (0)

    @addtogroup ADC_CONST ADC Bit Field Definition
    Constant Definitions for ADC Controller

ADC_T::RESULT: RSLT Position

Definition at line 767 of file Nano1X2Series.h.

## ◆ ADC_RESULT_VALID_Msk

#define ADC_RESULT_VALID_Msk (0x1ul << ADC_RESULT_VALID_Pos)

ADC_T::RESULT: VALID Mask

Definition at line 771 of file Nano1X2Series.h.

## ◆ ADC_RESULT_VALID_Pos

#define ADC_RESULT_VALID_Pos (16)

ADC_T::RESULT: VALID Position

Definition at line 770 of file Nano1X2Series.h.

## ◆ ADC_SMPLCNT0_CH0SAMPCNT_Msk

#define ADC_SMPLCNT0_CH0SAMPCNT_Msk (0xful << ADC_SMPLCNT0_CH0SAMPCNT_Pos)

ADC_T::SMPLCNT0: CH0SAMPCNT Mask

Definition at line 885 of file Nano1X2Series.h.

## ◆ ADC_SMPLCNT0_CH0SAMPCNT_Pos

#define ADC_SMPLCNT0_CH0SAMPCNT_Pos (0)

ADC_T::SMPLCNT0: CH0SAMPCNT Position

Definition at line 884 of file Nano1X2Series.h.

## ◆ ADC_SMPLCNT1_CH8SAMPCNT_Msk

#define ADC_SMPLCNT1_CH8SAMPCNT_Msk (0xful << ADC_SMPLCNT1_CH8SAMPCNT_Pos)

ADC_T::SMPLCNT1: CH8SAMPCNT Mask

Definition at line 888 of file Nano1X2Series.h.

## ◆ ADC_SMPLCNT1_CH8SAMPCNT_Pos

#define ADC_SMPLCNT1_CH8SAMPCNT_Pos (0)

ADC_T::SMPLCNT1: CH8SAMPCNT Position

Definition at line 887 of file Nano1X2Series.h.

## ◆ ADC_SMPLCNT1_INTCHSAMPCNT_Msk

#define ADC_SMPLCNT1_INTCHSAMPCNT_Msk (0xful << ADC_SMPLCNT1_INTCHSAMPCNT_Pos)

ADC_T::SMPLCNT1: INTCHSAMPCNT Mask

Definition at line 891 of file Nano1X2Series.h.

## ◆ ADC_SMPLCNT1_INTCHSAMPCNT_Pos

#define ADC_SMPLCNT1_INTCHSAMPCNT_Pos (16)

ADC_T::SMPLCNT1: INTCHSAMPCNT Position

Definition at line 890 of file Nano1X2Series.h.

## ◆ ADC_SR_ADF_Msk

#define ADC_SR_ADF_Msk (0x1ul << ADC_SR_ADF_Pos)

ADC_T::SR: ADF Mask

Definition at line 840 of file Nano1X2Series.h.

## ◆ ADC_SR_ADF_Pos

#define ADC_SR_ADF_Pos (0)

ADC_T::SR: ADF Position

Definition at line 839 of file Nano1X2Series.h.

## ◆ ADC_SR_BUSY_Msk

#define ADC_SR_BUSY_Msk (0x1ul << ADC_SR_BUSY_Pos)

ADC_T::SR: BUSY Mask

Definition at line 849 of file Nano1X2Series.h.

## ◆ ADC_SR_BUSY_Pos

#define ADC_SR_BUSY_Pos (3)

ADC_T::SR: BUSY Position

Definition at line 848 of file Nano1X2Series.h.

## ◆ ADC_SR_CHANNEL_Msk

#define ADC_SR_CHANNEL_Msk (0x1ful << ADC_SR_CHANNEL_Pos)

ADC_T::SR: CHANNEL Mask

Definition at line 852 of file Nano1X2Series.h.

## ◆ ADC_SR_CHANNEL_Pos

#define ADC_SR_CHANNEL_Pos (4)

ADC_T::SR: CHANNEL Position

Definition at line 851 of file Nano1X2Series.h.

## ◆ ADC_SR_CMPF0_Msk

#define ADC_SR_CMPF0_Msk (0x1ul << ADC_SR_CMPF0_Pos)

ADC_T::SR: CMPF0 Mask

Definition at line 843 of file Nano1X2Series.h.

## ◆ ADC_SR_CMPF0_Pos

#define ADC_SR_CMPF0_Pos (1)

ADC_T::SR: CMPF0 Position

Definition at line 842 of file Nano1X2Series.h.

## ◆ ADC_SR_CMPF1_Msk

#define ADC_SR_CMPF1_Msk (0x1ul << ADC_SR_CMPF1_Pos)

ADC_T::SR: CMPF1 Mask

Definition at line 846 of file Nano1X2Series.h.

## ◆ ADC_SR_CMPF1_Pos

#define ADC_SR_CMPF1_Pos (2)

ADC_T::SR: CMPF1 Position

Definition at line 845 of file Nano1X2Series.h.

## ◆ ADC_SR_INITRDY_Msk

#define ADC_SR_INITRDY_Msk (0x1ul << ADC_SR_INITRDY_Pos)

ADC_T::SR: INITRDY Mask

Definition at line 855 of file Nano1X2Series.h.

## ◆ ADC_SR_INITRDY_Pos

#define ADC_SR_INITRDY_Pos (16)

ADC_T::SR: INITRDY Position

Definition at line 854 of file Nano1X2Series.h.