| CMSIS-Core (Cortex-A) CMSIS-Core support for Cortex-A processor-based devices |

Loading...
Searching...
No Matches
Macros
DACR Dn field values
Core Register Access » Domain Access Control Register (DACR)

Valid values for DACR Dn field. More...

## Macros
#define | DACR_Dn_NOACCESS 0U
| DACR Dn field: No access.
#define | DACR_Dn_CLIENT 1U
| DACR Dn field: Client.
#define | DACR_Dn_MANAGER 3U
| DACR Dn field: Manager.

## Description

Valid values for DACR Dn field.

The Dn field can contain one of these values which indicates the domain n access permission.

## Macro Definition Documentation

## ◆ DACR_Dn_CLIENT

#define DACR_Dn_CLIENT 1U

DACR Dn field: Client.

Accesses are checked against the permission bits in the translation tables.

## ◆ DACR_Dn_MANAGER

#define DACR_Dn_MANAGER 3U

DACR Dn field: Manager.

Accesses are not checked against the permission bits in the translation tables.

## ◆ DACR_Dn_NOACCESS

#define DACR_Dn_NOACCESS 0U

DACR Dn field: No access.

Any access to the domain generates a Domain fault.